/*Modified at 2023-12-24 17:14:56*/
/****************************************************
 *  Automatically-generated file. Do not edit!	*
 ****************************************************/

#include "project_config.h"
#include "djyos.h"
#include "stdint.h"
#include "stddef.h"
#include "cpu_peri.h"
#include <Iboot_info.h>

#include <djyfs/filesystems.h>

extern ptu32_t djy_main(void);
//如果这个CN_MANUFACTURER_NAME名字要改，那djysrc里的Iboot_info.c中相应的名字也要改
const char CN_MANUFACTURER_NAME[] = PRODUCT_MANUFACTURER_NAME;


const struct ProductInfo Djy_Product_Info __attribute__ ((section(".DjyProductInfo"))) =
{
    .VersionNumber[0] = PRODUCT_VERSION_LARGE,
    .VersionNumber[1] = PRODUCT_VERSION_MEDIUM,
    .VersionNumber[2] = PRODUCT_VERSION_SMALL,
#if(CN_PTR_BITS < 64)
    .ManufacturerNameAddr      = (u32)(&CN_MANUFACTURER_NAME),
    .ManufacturerNamereserved32    = 0xffffffff,
#else
    .ManufacturerNameAddr      = (u64)(&CN_MANUFACTURER_NAME),
#endif
    .ProductClassify = PRODUCT_PRODUCT_CLASSIFY,
    .ProductType = PRODUCT_PRODUCT_MODEL,

    .TypeCode = PRODUCT_PRODUCT_MODEL_CODE,

    .ProductionTime = {'*','*','*','*'},
    .ProductionNumber = {'*','*','*','*','*'},
    .reserved8 = 0,
    .BoardType = PRODUCT_BOARD_TYPE,
    .CPU_Type = PRODUCT_CPU_TYPE,
    .Reserved ={
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff
            },
};


ptu32_t __djy_main(void)
{
    //modbus
    extern bool_t ModuleInstall_Modbus(void);
    ModuleInstall_Modbus();
    //end modbus

    djy_main();

	return 0;
}

void Sys_ModuleInit(void)
{
	uint16_t evtt_main;

    //shell
    extern void Stdio_KnlInOutInit(char * StdioIn, char *StdioOut);
    Stdio_KnlInOutInit(CFG_STDIO_IN_NAME,CFG_STDIO_OUT_NAME);
    extern s32 ModuleInstall_Shell(ptu32_t para);
    ModuleInstall_Shell(0);
    //end shell

    //----------------------------early----------------------------//

    //device file system
    extern s32 ModuleInstall_dev(void);
    ModuleInstall_dev();    // 安装设备文件系统；
    //end device file system

    //djybus
    extern bool_t ModuleInstall_DjyBus(void);
    ModuleInstall_DjyBus ( );
    //end djybus

    //message queue
    extern bool_t ModuleInstall_MsgQ(void);
    ModuleInstall_MsgQ ( );
    //end message queue

    //multiplex
    extern bool_t ModuleInstall_Multiplex(void);
    ModuleInstall_Multiplex ();
    //end multiplex

    //spi bus
    extern bool_t ModuleInstall_SPIBus(void);
    ModuleInstall_SPIBus();
    //end spi bus

    //xip iboot file system
    extern s32 ModuleInstall_XIP_IBOOT_FS(u32 opt, void *data);
    ModuleInstall_XIP_IBOOT_FS(0,NULL);
    //end xip iboot file system

    //cpu onchip spi
    extern bool_t ModuleInstall_SPI(u8 port);
    #if CFG_SPI1_ENABLE==1
    ModuleInstall_SPI(CN_SPI1);
    #endif
    #if CFG_SPI2_ENABLE==1
    ModuleInstall_SPI(CN_SPI2);
    #endif
    #if CFG_SPI3_ENABLE==1
    ModuleInstall_SPI(CN_SPI3);
    #endif
    #if CFG_SPI4_ENABLE==1
    ModuleInstall_SPI(CN_SPI4);
    #endif
    //end cpu onchip spi

    //cpu onchip uart
    extern ptu32_t ModuleInstall_UART(ptu32_t SerialNo);
    #if CFG_UART1_ENABLE ==1
    ModuleInstall_UART(CN_UART1);
    #endif
    #if CFG_UART2_ENABLE ==1
    ModuleInstall_UART(CN_UART2);
    #endif
    #if CFG_UART3_ENABLE ==1
    ModuleInstall_UART(CN_UART3);
    #endif
    #if CFG_UART4_ENABLE ==1
    ModuleInstall_UART(CN_UART4);
    #endif
    #if CFG_UART5_ENABLE ==1
    ModuleInstall_UART(CN_UART5);
    #endif
    #if CFG_UART6_ENABLE ==1
    ModuleInstall_UART(CN_UART6);
    #endif
    #if CFG_UART7_ENABLE ==1
    ModuleInstall_UART(CN_UART7);
    #endif
    #if CFG_UART8_ENABLE ==1
    ModuleInstall_UART(CN_UART8);
    #endif
    //end cpu onchip uart

    //fat file system
    extern s32 ModuleInstall_FAT(const char *dir, u32 opt, void *data);
    ModuleInstall_FAT(CFG_FAT_MOUNT_POINT, CFG_FAT_MS_INSTALLUSE, CFG_FAT_MEDIA_KIND);
    //end fat file system

    //cpu onchip timer
    extern bool_t ModuleInstall_HardTimer(void);
    ModuleInstall_HardTimer();
    //end cpu onchip timer

    //kernel
    #if(CFG_OS_TINY == flase)
    extern s32 kernel_command(void);
    kernel_command();
    #endif
    //end kernel

    //Nls Charset
    extern ptu32_t ModuleInstall_Charset(ptu32_t para);
    ModuleInstall_Charset(0);
    extern void ModuleInstall_CharsetNls(const char * DefaultCharset);
    ModuleInstall_CharsetNls("C");
    //end Nls Charset

    //Software Timers
    extern bool_t ModuleInstall_Timer(void);
    ModuleInstall_Timer();
    //end Software Timers

    //tcpip
    extern bool_t ModuleInstall_TcpIp(void);
    ModuleInstall_TcpIp( );
    //end tcpip

    //cpu onchip ETH
    extern bool_t ModuleInstall_ETH(void);
    ModuleInstall_ETH( );
    //end cpu onchip ETH

    //norflash W25QXX
    extern s32 ModuleInstall_W25qxx(void);
    ModuleInstall_W25qxx();
    //end norflash W25QXX

    //W25QXX FAT
    extern bool_t ModuleInstall_W25qxxInstallFat(const char *TargetFs, s32 bend, u32 doformat);
    ModuleInstall_W25qxxInstallFat(CFG_W25_FAT_MOUNT_NAME,CFG_W25_FAT_PART_END,CFG_W25_FAT_PART_FORMAT);
    //end W25QXX FAT

    //----------------------------later----------------------------//
    //stdio
    #if(CFG_STDIO_STDIOFILE == true)
    extern s32 ModuleInstall_STDIO(const char *in,const char *out, const char *err);
    ModuleInstall_STDIO(CFG_STDIO_IN_NAME,CFG_STDIO_OUT_NAME,CFG_STDIO_ERR_NAME);
    #endif
    //end stdio

    //network config
    extern void ModuleInstall_InitNet( );
    ModuleInstall_InitNet( );
    //end network config

	evtt_main = DJY_EvttRegist(EN_CORRELATIVE,CN_PRIO_RRS,0,0,
		__djy_main,NULL,CFG_MAINSTACK_LIMIT, "main function");
	//事件的两个参数暂设为0,如果用shell启动,可用来采集shell命令行参数
	DJY_EventPop(evtt_main,NULL,0,0,0,0);

    //----------------------------medium----------------------------//
    //heap
    #if ((CFG_DYNAMIC_MEM == true))
    extern bool_t Heap_DynamicModuleInit(void);
    Heap_DynamicModuleInit ( );
    #endif
    //end heap



	return ;
}

/*Modified at 2023-12-24 19:24:12*/
/****************************************************
 *  Automatically-generated file. Do not edit!	*
 ****************************************************/

#include "project_config.h"
#include "djyos.h"
#include "stdint.h"
#include "stddef.h"
#include "cpu_peri.h"
#include <Iboot_info.h>

#include <djyfs/filesystems.h>

extern ptu32_t djy_main(void);
//如果这个CN_MANUFACTURER_NAME名字要改，那djysrc里的Iboot_info.c中相应的名字也要改
const char CN_MANUFACTURER_NAME[] = PRODUCT_MANUFACTURER_NAME;


const struct ProductInfo Djy_Product_Info __attribute__ ((section(".DjyProductInfo"))) =
{
    .VersionNumber[0] = PRODUCT_VERSION_LARGE,
    .VersionNumber[1] = PRODUCT_VERSION_MEDIUM,
    .VersionNumber[2] = PRODUCT_VERSION_SMALL,
#if(CN_PTR_BITS < 64)
    .ManufacturerNameAddr      = (u32)(&CN_MANUFACTURER_NAME),
    .ManufacturerNamereserved32    = 0xffffffff,
#else
    .ManufacturerNameAddr      = (u64)(&CN_MANUFACTURER_NAME),
#endif
    .ProductClassify = PRODUCT_PRODUCT_CLASSIFY,
    .ProductType = PRODUCT_PRODUCT_MODEL,

    .TypeCode = PRODUCT_PRODUCT_MODEL_CODE,

    .ProductionTime = {'*','*','*','*'},
    .ProductionNumber = {'*','*','*','*','*'},
    .reserved8 = 0,
    .BoardType = PRODUCT_BOARD_TYPE,
    .CPU_Type = PRODUCT_CPU_TYPE,
    .Reserved ={
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff
            },
};


ptu32_t __djy_main(void)
{
    //modbus
    extern bool_t ModuleInstall_Modbus(void);
    ModuleInstall_Modbus();
    //end modbus

    djy_main();

	return 0;
}

void Sys_ModuleInit(void)
{
	uint16_t evtt_main;

    //shell
    extern void Stdio_KnlInOutInit(char * StdioIn, char *StdioOut);
    Stdio_KnlInOutInit(CFG_STDIO_IN_NAME,CFG_STDIO_OUT_NAME);
    extern s32 ModuleInstall_Shell(ptu32_t para);
    ModuleInstall_Shell(0);
    //end shell

    //----------------------------early----------------------------//

    //device file system
    extern s32 ModuleInstall_dev(void);
    ModuleInstall_dev();    // 安装设备文件系统；
    //end device file system

    //djybus
    extern bool_t ModuleInstall_DjyBus(void);
    ModuleInstall_DjyBus ( );
    //end djybus

    //message queue
    extern bool_t ModuleInstall_MsgQ(void);
    ModuleInstall_MsgQ ( );
    //end message queue

    //multiplex
    extern bool_t ModuleInstall_Multiplex(void);
    ModuleInstall_Multiplex ();
    //end multiplex

    //spi bus
    extern bool_t ModuleInstall_SPIBus(void);
    ModuleInstall_SPIBus();
    //end spi bus

    //cpu onchip spi
    extern bool_t ModuleInstall_SPI(u8 port);
    #if CFG_SPI1_ENABLE==1
    ModuleInstall_SPI(CN_SPI1);
    #endif
    #if CFG_SPI2_ENABLE==1
    ModuleInstall_SPI(CN_SPI2);
    #endif
    #if CFG_SPI3_ENABLE==1
    ModuleInstall_SPI(CN_SPI3);
    #endif
    #if CFG_SPI4_ENABLE==1
    ModuleInstall_SPI(CN_SPI4);
    #endif
    //end cpu onchip spi

    //xip iboot file system
    extern s32 ModuleInstall_XIP_IBOOT_FS(u32 opt, void *data);
    ModuleInstall_XIP_IBOOT_FS(0,NULL);
    //end xip iboot file system

    //cpu drive inner flash
    s32 ModuleInstall_EmbededFlash(u32 doformat);
    ModuleInstall_EmbededFlash(CFG_EFLASH_PART_FORMAT);
    //end cpu drive inner flash

    //emflash insatall xip
    extern s32 ModuleInstall_EmFlashInstallXIP(const char *TargetFs,s32 bstart, s32 bend, u32 doformat);
    ModuleInstall_EmFlashInstallXIP(CFG_EFLASH_XIPFSMOUNT_NAME,CFG_EFLASH_XIP_PART_START,
    CFG_EFLASH_XIP_PART_END, CFG_EFLASH_XIP_PART_FORMAT);
    //end emflash insatall xip

    //kernel
    #if(CFG_OS_TINY == flase)
    extern s32 kernel_command(void);
    kernel_command();
    #endif
    //end kernel

    //Nls Charset
    extern ptu32_t ModuleInstall_Charset(ptu32_t para);
    ModuleInstall_Charset(0);
    extern void ModuleInstall_CharsetNls(const char * DefaultCharset);
    ModuleInstall_CharsetNls("C");
    //end Nls Charset

    //fat file system
    extern s32 ModuleInstall_FAT(const char *dir, u32 opt, void *data);
    ModuleInstall_FAT(CFG_FAT_MOUNT_POINT, CFG_FAT_MS_INSTALLUSE, CFG_FAT_MEDIA_KIND);
    //end fat file system

    //Software Timers
    extern bool_t ModuleInstall_Timer(void);
    ModuleInstall_Timer();
    //end Software Timers

    //cpu onchip timer
    extern bool_t ModuleInstall_HardTimer(void);
    ModuleInstall_HardTimer();
    //end cpu onchip timer

    //tcpip
    extern bool_t ModuleInstall_TcpIp(void);
    ModuleInstall_TcpIp( );
    //end tcpip

    //cpu onchip ETH
    extern bool_t ModuleInstall_ETH(void);
    ModuleInstall_ETH( );
    //end cpu onchip ETH

    //cpu onchip uart
    extern ptu32_t ModuleInstall_UART(ptu32_t SerialNo);
    #if CFG_UART1_ENABLE ==1
    ModuleInstall_UART(CN_UART1);
    #endif
    #if CFG_UART2_ENABLE ==1
    ModuleInstall_UART(CN_UART2);
    #endif
    #if CFG_UART3_ENABLE ==1
    ModuleInstall_UART(CN_UART3);
    #endif
    #if CFG_UART4_ENABLE ==1
    ModuleInstall_UART(CN_UART4);
    #endif
    #if CFG_UART5_ENABLE ==1
    ModuleInstall_UART(CN_UART5);
    #endif
    #if CFG_UART6_ENABLE ==1
    ModuleInstall_UART(CN_UART6);
    #endif
    #if CFG_UART7_ENABLE ==1
    ModuleInstall_UART(CN_UART7);
    #endif
    #if CFG_UART8_ENABLE ==1
    ModuleInstall_UART(CN_UART8);
    #endif
    //end cpu onchip uart

    //norflash W25QXX
    extern s32 ModuleInstall_W25qxx(void);
    ModuleInstall_W25qxx();
    //end norflash W25QXX

    //W25QXX FAT
    extern bool_t ModuleInstall_W25qxxInstallFat(const char *TargetFs, s32 bend, u32 doformat);
    ModuleInstall_W25qxxInstallFat(CFG_W25_FAT_MOUNT_NAME,CFG_W25_FAT_PART_END,CFG_W25_FAT_PART_FORMAT);
    //end W25QXX FAT

    //----------------------------later----------------------------//
    //stdio
    #if(CFG_STDIO_STDIOFILE == true)
    extern s32 ModuleInstall_STDIO(const char *in,const char *out, const char *err);
    ModuleInstall_STDIO(CFG_STDIO_IN_NAME,CFG_STDIO_OUT_NAME,CFG_STDIO_ERR_NAME);
    #endif
    //end stdio

    //network config
    extern void ModuleInstall_InitNet( );
    ModuleInstall_InitNet( );
    //end network config

	evtt_main = DJY_EvttRegist(EN_CORRELATIVE,CN_PRIO_RRS,0,0,
		__djy_main,NULL,CFG_MAINSTACK_LIMIT, "main function");
	//事件的两个参数暂设为0,如果用shell启动,可用来采集shell命令行参数
	DJY_EventPop(evtt_main,NULL,0,0,0,0);

    //----------------------------medium----------------------------//
    //heap
    #if ((CFG_DYNAMIC_MEM == true))
    extern bool_t Heap_DynamicModuleInit(void);
    Heap_DynamicModuleInit ( );
    #endif
    //end heap



	return ;
}

/*Modified at 2023-12-24 19:24:21*/
/****************************************************
 *  Automatically-generated file. Do not edit!	*
 ****************************************************/

#include "project_config.h"
#include "djyos.h"
#include "stdint.h"
#include "stddef.h"
#include "cpu_peri.h"
#include <Iboot_info.h>

#include <djyfs/filesystems.h>

extern ptu32_t djy_main(void);
//如果这个CN_MANUFACTURER_NAME名字要改，那djysrc里的Iboot_info.c中相应的名字也要改
const char CN_MANUFACTURER_NAME[] = PRODUCT_MANUFACTURER_NAME;


const struct ProductInfo Djy_Product_Info __attribute__ ((section(".DjyProductInfo"))) =
{
    .VersionNumber[0] = PRODUCT_VERSION_LARGE,
    .VersionNumber[1] = PRODUCT_VERSION_MEDIUM,
    .VersionNumber[2] = PRODUCT_VERSION_SMALL,
#if(CN_PTR_BITS < 64)
    .ManufacturerNameAddr      = (u32)(&CN_MANUFACTURER_NAME),
    .ManufacturerNamereserved32    = 0xffffffff,
#else
    .ManufacturerNameAddr      = (u64)(&CN_MANUFACTURER_NAME),
#endif
    .ProductClassify = PRODUCT_PRODUCT_CLASSIFY,
    .ProductType = PRODUCT_PRODUCT_MODEL,

    .TypeCode = PRODUCT_PRODUCT_MODEL_CODE,

    .ProductionTime = {'*','*','*','*'},
    .ProductionNumber = {'*','*','*','*','*'},
    .reserved8 = 0,
    .BoardType = PRODUCT_BOARD_TYPE,
    .CPU_Type = PRODUCT_CPU_TYPE,
    .Reserved ={
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff
            },
};


ptu32_t __djy_main(void)
{
    //modbus
    extern bool_t ModuleInstall_Modbus(void);
    ModuleInstall_Modbus();
    //end modbus

    djy_main();

	return 0;
}

void Sys_ModuleInit(void)
{
	uint16_t evtt_main;

    //shell
    extern void Stdio_KnlInOutInit(char * StdioIn, char *StdioOut);
    Stdio_KnlInOutInit(CFG_STDIO_IN_NAME,CFG_STDIO_OUT_NAME);
    extern s32 ModuleInstall_Shell(ptu32_t para);
    ModuleInstall_Shell(0);
    //end shell

    //----------------------------early----------------------------//
    //black box
    extern void ModuleInstall_BlackBox(void);
    ModuleInstall_BlackBox( );
    //end black box

    //device file system
    extern s32 ModuleInstall_dev(void);
    ModuleInstall_dev();    // 安装设备文件系统；
    //end device file system

    //djybus
    extern bool_t ModuleInstall_DjyBus(void);
    ModuleInstall_DjyBus ( );
    //end djybus

    //message queue
    extern bool_t ModuleInstall_MsgQ(void);
    ModuleInstall_MsgQ ( );
    //end message queue

    //multiplex
    extern bool_t ModuleInstall_Multiplex(void);
    ModuleInstall_Multiplex ();
    //end multiplex

    //spi bus
    extern bool_t ModuleInstall_SPIBus(void);
    ModuleInstall_SPIBus();
    //end spi bus

    //xip iboot file system
    extern s32 ModuleInstall_XIP_IBOOT_FS(u32 opt, void *data);
    ModuleInstall_XIP_IBOOT_FS(0,NULL);
    //end xip iboot file system

    //cpu onchip spi
    extern bool_t ModuleInstall_SPI(u8 port);
    #if CFG_SPI1_ENABLE==1
    ModuleInstall_SPI(CN_SPI1);
    #endif
    #if CFG_SPI2_ENABLE==1
    ModuleInstall_SPI(CN_SPI2);
    #endif
    #if CFG_SPI3_ENABLE==1
    ModuleInstall_SPI(CN_SPI3);
    #endif
    #if CFG_SPI4_ENABLE==1
    ModuleInstall_SPI(CN_SPI4);
    #endif
    //end cpu onchip spi

    //cpu onchip uart
    extern ptu32_t ModuleInstall_UART(ptu32_t SerialNo);
    #if CFG_UART1_ENABLE ==1
    ModuleInstall_UART(CN_UART1);
    #endif
    #if CFG_UART2_ENABLE ==1
    ModuleInstall_UART(CN_UART2);
    #endif
    #if CFG_UART3_ENABLE ==1
    ModuleInstall_UART(CN_UART3);
    #endif
    #if CFG_UART4_ENABLE ==1
    ModuleInstall_UART(CN_UART4);
    #endif
    #if CFG_UART5_ENABLE ==1
    ModuleInstall_UART(CN_UART5);
    #endif
    #if CFG_UART6_ENABLE ==1
    ModuleInstall_UART(CN_UART6);
    #endif
    #if CFG_UART7_ENABLE ==1
    ModuleInstall_UART(CN_UART7);
    #endif
    #if CFG_UART8_ENABLE ==1
    ModuleInstall_UART(CN_UART8);
    #endif
    //end cpu onchip uart

    //fat file system
    extern s32 ModuleInstall_FAT(const char *dir, u32 opt, void *data);
    ModuleInstall_FAT(CFG_FAT_MOUNT_POINT, CFG_FAT_MS_INSTALLUSE, CFG_FAT_MEDIA_KIND);
    //end fat file system

    //cpu onchip timer
    extern bool_t ModuleInstall_HardTimer(void);
    ModuleInstall_HardTimer();
    //end cpu onchip timer

    //cpu drive inner flash
    s32 ModuleInstall_EmbededFlash(u32 doformat);
    ModuleInstall_EmbededFlash(CFG_EFLASH_PART_FORMAT);
    //end cpu drive inner flash

    //emflash insatall xip
    extern s32 ModuleInstall_EmFlashInstallXIP(const char *TargetFs,s32 bstart, s32 bend, u32 doformat);
    ModuleInstall_EmFlashInstallXIP(CFG_EFLASH_XIPFSMOUNT_NAME,CFG_EFLASH_XIP_PART_START,
    CFG_EFLASH_XIP_PART_END, CFG_EFLASH_XIP_PART_FORMAT);
    //end emflash insatall xip

    //kernel
    #if(CFG_OS_TINY == flase)
    extern s32 kernel_command(void);
    kernel_command();
    #endif
    //end kernel

    //Nls Charset
    extern ptu32_t ModuleInstall_Charset(ptu32_t para);
    ModuleInstall_Charset(0);
    extern void ModuleInstall_CharsetNls(const char * DefaultCharset);
    ModuleInstall_CharsetNls("C");
    //end Nls Charset

    //Software Timers
    extern bool_t ModuleInstall_Timer(void);
    ModuleInstall_Timer();
    //end Software Timers

    //tcpip
    extern bool_t ModuleInstall_TcpIp(void);
    ModuleInstall_TcpIp( );
    //end tcpip

    //cpu onchip ETH
    extern bool_t ModuleInstall_ETH(void);
    ModuleInstall_ETH( );
    //end cpu onchip ETH

    //norflash W25QXX
    extern s32 ModuleInstall_W25qxx(void);
    ModuleInstall_W25qxx();
    //end norflash W25QXX

    //W25QXX FAT
    extern bool_t ModuleInstall_W25qxxInstallFat(const char *TargetFs, s32 bend, u32 doformat);
    ModuleInstall_W25qxxInstallFat(CFG_W25_FAT_MOUNT_NAME,CFG_W25_FAT_PART_END,CFG_W25_FAT_PART_FORMAT);
    //end W25QXX FAT

    //----------------------------later----------------------------//
    //stdio
    #if(CFG_STDIO_STDIOFILE == true)
    extern s32 ModuleInstall_STDIO(const char *in,const char *out, const char *err);
    ModuleInstall_STDIO(CFG_STDIO_IN_NAME,CFG_STDIO_OUT_NAME,CFG_STDIO_ERR_NAME);
    #endif
    //end stdio

    //network config
    extern void ModuleInstall_InitNet( );
    ModuleInstall_InitNet( );
    //end network config

	evtt_main = DJY_EvttRegist(EN_CORRELATIVE,CN_PRIO_RRS,0,0,
		__djy_main,NULL,CFG_MAINSTACK_LIMIT, "main function");
	//事件的两个参数暂设为0,如果用shell启动,可用来采集shell命令行参数
	DJY_EventPop(evtt_main,NULL,0,0,0,0);

    //----------------------------medium----------------------------//
    //heap
    #if ((CFG_DYNAMIC_MEM == true))
    extern bool_t Heap_DynamicModuleInit(void);
    Heap_DynamicModuleInit ( );
    #endif
    //end heap



	return ;
}

/*Modified at 2023-12-24 19:43:56*/
/****************************************************
 *  Automatically-generated file. Do not edit!	*
 ****************************************************/

#include "project_config.h"
#include "djyos.h"
#include "stdint.h"
#include "stddef.h"
#include "cpu_peri.h"
#include <Iboot_info.h>

#include <djyfs/filesystems.h>

extern ptu32_t djy_main(void);
//如果这个CN_MANUFACTURER_NAME名字要改，那djysrc里的Iboot_info.c中相应的名字也要改
const char CN_MANUFACTURER_NAME[] = PRODUCT_MANUFACTURER_NAME;


const struct ProductInfo Djy_Product_Info __attribute__ ((section(".DjyProductInfo"))) =
{
    .VersionNumber[0] = PRODUCT_VERSION_LARGE,
    .VersionNumber[1] = PRODUCT_VERSION_MEDIUM,
    .VersionNumber[2] = PRODUCT_VERSION_SMALL,
#if(CN_PTR_BITS < 64)
    .ManufacturerNameAddr      = (u32)(&CN_MANUFACTURER_NAME),
    .ManufacturerNamereserved32    = 0xffffffff,
#else
    .ManufacturerNameAddr      = (u64)(&CN_MANUFACTURER_NAME),
#endif
    .ProductClassify = PRODUCT_PRODUCT_CLASSIFY,
    .ProductType = PRODUCT_PRODUCT_MODEL,

    .TypeCode = PRODUCT_PRODUCT_MODEL_CODE,

    .ProductionTime = {'*','*','*','*'},
    .ProductionNumber = {'*','*','*','*','*'},
    .reserved8 = 0,
    .BoardType = PRODUCT_BOARD_TYPE,
    .CPU_Type = PRODUCT_CPU_TYPE,
    .Reserved ={
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff
            },
};


ptu32_t __djy_main(void)
{
    //modbus
    extern bool_t ModuleInstall_Modbus(void);
    ModuleInstall_Modbus();
    //end modbus

    djy_main();

	return 0;
}

void Sys_ModuleInit(void)
{
	uint16_t evtt_main;

    //shell
    extern void Stdio_KnlInOutInit(char * StdioIn, char *StdioOut);
    Stdio_KnlInOutInit(CFG_STDIO_IN_NAME,CFG_STDIO_OUT_NAME);
    extern s32 ModuleInstall_Shell(ptu32_t para);
    ModuleInstall_Shell(0);
    //end shell

    //----------------------------early----------------------------//
    //black box
    extern void ModuleInstall_BlackBox(void);
    ModuleInstall_BlackBox( );
    //end black box

    //device file system
    extern s32 ModuleInstall_dev(void);
    ModuleInstall_dev();    // 安装设备文件系统；
    //end device file system

    //djybus
    extern bool_t ModuleInstall_DjyBus(void);
    ModuleInstall_DjyBus ( );
    //end djybus

    //message queue
    extern bool_t ModuleInstall_MsgQ(void);
    ModuleInstall_MsgQ ( );
    //end message queue

    //multiplex
    extern bool_t ModuleInstall_Multiplex(void);
    ModuleInstall_Multiplex ();
    //end multiplex

    //spi bus
    extern bool_t ModuleInstall_SPIBus(void);
    ModuleInstall_SPIBus();
    //end spi bus

    //cpu onchip spi
    extern bool_t ModuleInstall_SPI(u8 port);
    #if CFG_SPI1_ENABLE==1
    ModuleInstall_SPI(CN_SPI1);
    #endif
    #if CFG_SPI2_ENABLE==1
    ModuleInstall_SPI(CN_SPI2);
    #endif
    #if CFG_SPI3_ENABLE==1
    ModuleInstall_SPI(CN_SPI3);
    #endif
    #if CFG_SPI4_ENABLE==1
    ModuleInstall_SPI(CN_SPI4);
    #endif
    //end cpu onchip spi

    //xip iboot file system
    extern s32 ModuleInstall_XIP_IBOOT_FS(u32 opt, void *data);
    ModuleInstall_XIP_IBOOT_FS(0,NULL);
    //end xip iboot file system

    //cpu drive inner flash
    s32 ModuleInstall_EmbededFlash(u32 doformat);
    ModuleInstall_EmbededFlash(CFG_EFLASH_PART_FORMAT);
    //end cpu drive inner flash

    //emflash insatall xip
    extern s32 ModuleInstall_EmFlashInstallXIP(const char *TargetFs,s32 bstart, s32 bend, u32 doformat);
    ModuleInstall_EmFlashInstallXIP(CFG_EFLASH_XIPFSMOUNT_NAME,CFG_EFLASH_XIP_PART_START,
    CFG_EFLASH_XIP_PART_END, CFG_EFLASH_XIP_PART_FORMAT);
    //end emflash insatall xip

    //kernel
    #if(CFG_OS_TINY == flase)
    extern s32 kernel_command(void);
    kernel_command();
    #endif
    //end kernel

    //Nls Charset
    extern ptu32_t ModuleInstall_Charset(ptu32_t para);
    ModuleInstall_Charset(0);
    extern void ModuleInstall_CharsetNls(const char * DefaultCharset);
    ModuleInstall_CharsetNls("C");
    //end Nls Charset

    //fat file system
    extern s32 ModuleInstall_FAT(const char *dir, u32 opt, void *data);
    ModuleInstall_FAT(CFG_FAT_MOUNT_POINT, CFG_FAT_MS_INSTALLUSE, CFG_FAT_MEDIA_KIND);
    //end fat file system

    //Software Timers
    extern bool_t ModuleInstall_Timer(void);
    ModuleInstall_Timer();
    //end Software Timers

    //cpu onchip timer
    extern bool_t ModuleInstall_HardTimer(void);
    ModuleInstall_HardTimer();
    //end cpu onchip timer

    //tcpip
    extern bool_t ModuleInstall_TcpIp(void);
    ModuleInstall_TcpIp( );
    //end tcpip

    //cpu onchip ETH
    extern bool_t ModuleInstall_ETH(void);
    ModuleInstall_ETH( );
    //end cpu onchip ETH

    //cpu onchip uart
    extern ptu32_t ModuleInstall_UART(ptu32_t SerialNo);
    #if CFG_UART1_ENABLE ==1
    ModuleInstall_UART(CN_UART1);
    #endif
    #if CFG_UART2_ENABLE ==1
    ModuleInstall_UART(CN_UART2);
    #endif
    #if CFG_UART3_ENABLE ==1
    ModuleInstall_UART(CN_UART3);
    #endif
    #if CFG_UART4_ENABLE ==1
    ModuleInstall_UART(CN_UART4);
    #endif
    #if CFG_UART5_ENABLE ==1
    ModuleInstall_UART(CN_UART5);
    #endif
    #if CFG_UART6_ENABLE ==1
    ModuleInstall_UART(CN_UART6);
    #endif
    #if CFG_UART7_ENABLE ==1
    ModuleInstall_UART(CN_UART7);
    #endif
    #if CFG_UART8_ENABLE ==1
    ModuleInstall_UART(CN_UART8);
    #endif
    //end cpu onchip uart

    //norflash W25QXX
    extern s32 ModuleInstall_W25qxx(void);
    ModuleInstall_W25qxx();
    //end norflash W25QXX

    //W25QXX FAT
    extern bool_t ModuleInstall_W25qxxInstallFat(const char *TargetFs, s32 bend, u32 doformat);
    ModuleInstall_W25qxxInstallFat(CFG_W25_FAT_MOUNT_NAME,CFG_W25_FAT_PART_END,CFG_W25_FAT_PART_FORMAT);
    //end W25QXX FAT

    //----------------------------later----------------------------//

    //stdio
    #if(CFG_STDIO_STDIOFILE == true)
    extern s32 ModuleInstall_STDIO(const char *in,const char *out, const char *err);
    ModuleInstall_STDIO(CFG_STDIO_IN_NAME,CFG_STDIO_OUT_NAME,CFG_STDIO_ERR_NAME);
    #endif
    //end stdio

    //network config
    extern void ModuleInstall_InitNet( );
    ModuleInstall_InitNet( );
    //end network config

	evtt_main = DJY_EvttRegist(EN_CORRELATIVE,CN_PRIO_RRS,0,0,
		__djy_main,NULL,CFG_MAINSTACK_LIMIT, "main function");
	//事件的两个参数暂设为0,如果用shell启动,可用来采集shell命令行参数
	DJY_EventPop(evtt_main,NULL,0,0,0,0);

    //----------------------------medium----------------------------//
    //heap
    #if ((CFG_DYNAMIC_MEM == true))
    extern bool_t Heap_DynamicModuleInit(void);
    Heap_DynamicModuleInit ( );
    #endif
    //end heap



	return ;
}

/*Modified at 2023-12-24 19:44:00*/
/****************************************************
 *  Automatically-generated file. Do not edit!	*
 ****************************************************/

#include "project_config.h"
#include "djyos.h"
#include "stdint.h"
#include "stddef.h"
#include "cpu_peri.h"
#include <Iboot_info.h>

#include <djyfs/filesystems.h>

extern ptu32_t djy_main(void);
//如果这个CN_MANUFACTURER_NAME名字要改，那djysrc里的Iboot_info.c中相应的名字也要改
const char CN_MANUFACTURER_NAME[] = PRODUCT_MANUFACTURER_NAME;


const struct ProductInfo Djy_Product_Info __attribute__ ((section(".DjyProductInfo"))) =
{
    .VersionNumber[0] = PRODUCT_VERSION_LARGE,
    .VersionNumber[1] = PRODUCT_VERSION_MEDIUM,
    .VersionNumber[2] = PRODUCT_VERSION_SMALL,
#if(CN_PTR_BITS < 64)
    .ManufacturerNameAddr      = (u32)(&CN_MANUFACTURER_NAME),
    .ManufacturerNamereserved32    = 0xffffffff,
#else
    .ManufacturerNameAddr      = (u64)(&CN_MANUFACTURER_NAME),
#endif
    .ProductClassify = PRODUCT_PRODUCT_CLASSIFY,
    .ProductType = PRODUCT_PRODUCT_MODEL,

    .TypeCode = PRODUCT_PRODUCT_MODEL_CODE,

    .ProductionTime = {'*','*','*','*'},
    .ProductionNumber = {'*','*','*','*','*'},
    .reserved8 = 0,
    .BoardType = PRODUCT_BOARD_TYPE,
    .CPU_Type = PRODUCT_CPU_TYPE,
    .Reserved ={
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff
            },
};


ptu32_t __djy_main(void)
{
    //modbus
    extern bool_t ModuleInstall_Modbus(void);
    ModuleInstall_Modbus();
    //end modbus

    djy_main();

	return 0;
}

void Sys_ModuleInit(void)
{
	uint16_t evtt_main;

    //shell
    extern void Stdio_KnlInOutInit(char * StdioIn, char *StdioOut);
    Stdio_KnlInOutInit(CFG_STDIO_IN_NAME,CFG_STDIO_OUT_NAME);
    extern s32 ModuleInstall_Shell(ptu32_t para);
    ModuleInstall_Shell(0);
    //end shell

    //----------------------------early----------------------------//
    //black box
    extern void ModuleInstall_BlackBox(void);
    ModuleInstall_BlackBox( );
    //end black box

    //device file system
    extern s32 ModuleInstall_dev(void);
    ModuleInstall_dev();    // 安装设备文件系统；
    //end device file system

    //djybus
    extern bool_t ModuleInstall_DjyBus(void);
    ModuleInstall_DjyBus ( );
    //end djybus

    //message queue
    extern bool_t ModuleInstall_MsgQ(void);
    ModuleInstall_MsgQ ( );
    //end message queue

    //multiplex
    extern bool_t ModuleInstall_Multiplex(void);
    ModuleInstall_Multiplex ();
    //end multiplex

    //spi bus
    extern bool_t ModuleInstall_SPIBus(void);
    ModuleInstall_SPIBus();
    //end spi bus

    //xip iboot file system
    extern s32 ModuleInstall_XIP_IBOOT_FS(u32 opt, void *data);
    ModuleInstall_XIP_IBOOT_FS(0,NULL);
    //end xip iboot file system

    //cpu onchip spi
    extern bool_t ModuleInstall_SPI(u8 port);
    #if CFG_SPI1_ENABLE==1
    ModuleInstall_SPI(CN_SPI1);
    #endif
    #if CFG_SPI2_ENABLE==1
    ModuleInstall_SPI(CN_SPI2);
    #endif
    #if CFG_SPI3_ENABLE==1
    ModuleInstall_SPI(CN_SPI3);
    #endif
    #if CFG_SPI4_ENABLE==1
    ModuleInstall_SPI(CN_SPI4);
    #endif
    //end cpu onchip spi

    //cpu onchip uart
    extern ptu32_t ModuleInstall_UART(ptu32_t SerialNo);
    #if CFG_UART1_ENABLE ==1
    ModuleInstall_UART(CN_UART1);
    #endif
    #if CFG_UART2_ENABLE ==1
    ModuleInstall_UART(CN_UART2);
    #endif
    #if CFG_UART3_ENABLE ==1
    ModuleInstall_UART(CN_UART3);
    #endif
    #if CFG_UART4_ENABLE ==1
    ModuleInstall_UART(CN_UART4);
    #endif
    #if CFG_UART5_ENABLE ==1
    ModuleInstall_UART(CN_UART5);
    #endif
    #if CFG_UART6_ENABLE ==1
    ModuleInstall_UART(CN_UART6);
    #endif
    #if CFG_UART7_ENABLE ==1
    ModuleInstall_UART(CN_UART7);
    #endif
    #if CFG_UART8_ENABLE ==1
    ModuleInstall_UART(CN_UART8);
    #endif
    //end cpu onchip uart

    //fat file system
    extern s32 ModuleInstall_FAT(const char *dir, u32 opt, void *data);
    ModuleInstall_FAT(CFG_FAT_MOUNT_POINT, CFG_FAT_MS_INSTALLUSE, CFG_FAT_MEDIA_KIND);
    //end fat file system

    //cpu onchip timer
    extern bool_t ModuleInstall_HardTimer(void);
    ModuleInstall_HardTimer();
    //end cpu onchip timer

    //cpu drive inner flash
    s32 ModuleInstall_EmbededFlash(u32 doformat);
    ModuleInstall_EmbededFlash(CFG_EFLASH_PART_FORMAT);
    //end cpu drive inner flash

    //emflash insatall xip
    extern s32 ModuleInstall_EmFlashInstallXIP(const char *TargetFs,s32 bstart, s32 bend, u32 doformat);
    ModuleInstall_EmFlashInstallXIP(CFG_EFLASH_XIPFSMOUNT_NAME,CFG_EFLASH_XIP_PART_START,
    CFG_EFLASH_XIP_PART_END, CFG_EFLASH_XIP_PART_FORMAT);
    //end emflash insatall xip

    //kernel
    #if(CFG_OS_TINY == flase)
    extern s32 kernel_command(void);
    kernel_command();
    #endif
    //end kernel

    //Nls Charset
    extern ptu32_t ModuleInstall_Charset(ptu32_t para);
    ModuleInstall_Charset(0);
    extern void ModuleInstall_CharsetNls(const char * DefaultCharset);
    ModuleInstall_CharsetNls("C");
    //end Nls Charset

    //Software Timers
    extern bool_t ModuleInstall_Timer(void);
    ModuleInstall_Timer();
    //end Software Timers

    //tcpip
    extern bool_t ModuleInstall_TcpIp(void);
    ModuleInstall_TcpIp( );
    //end tcpip

    //cpu onchip ETH
    extern bool_t ModuleInstall_ETH(void);
    ModuleInstall_ETH( );
    //end cpu onchip ETH

    //norflash W25QXX
    extern s32 ModuleInstall_W25qxx(void);
    ModuleInstall_W25qxx();
    //end norflash W25QXX

    //W25QXX FAT
    extern bool_t ModuleInstall_W25qxxInstallFat(const char *TargetFs, s32 bend, u32 doformat);
    ModuleInstall_W25qxxInstallFat(CFG_W25_FAT_MOUNT_NAME,CFG_W25_FAT_PART_END,CFG_W25_FAT_PART_FORMAT);
    //end W25QXX FAT

    //----------------------------later----------------------------//

    //stdio
    #if(CFG_STDIO_STDIOFILE == true)
    extern s32 ModuleInstall_STDIO(const char *in,const char *out, const char *err);
    ModuleInstall_STDIO(CFG_STDIO_IN_NAME,CFG_STDIO_OUT_NAME,CFG_STDIO_ERR_NAME);
    #endif
    //end stdio

    //network config
    extern void ModuleInstall_InitNet( );
    ModuleInstall_InitNet( );
    //end network config

	evtt_main = DJY_EvttRegist(EN_CORRELATIVE,CN_PRIO_RRS,0,0,
		__djy_main,NULL,CFG_MAINSTACK_LIMIT, "main function");
	//事件的两个参数暂设为0,如果用shell启动,可用来采集shell命令行参数
	DJY_EventPop(evtt_main,NULL,0,0,0,0);

    //----------------------------medium----------------------------//
    //heap
    #if ((CFG_DYNAMIC_MEM == true))
    extern bool_t Heap_DynamicModuleInit(void);
    Heap_DynamicModuleInit ( );
    #endif
    //end heap



	return ;
}

/*Modified at 2023-12-24 19:48:36*/
/****************************************************
 *  Automatically-generated file. Do not edit!	*
 ****************************************************/

#include "project_config.h"
#include "djyos.h"
#include "stdint.h"
#include "stddef.h"
#include "cpu_peri.h"
#include <Iboot_info.h>

#include <djyfs/filesystems.h>

extern ptu32_t djy_main(void);
//如果这个CN_MANUFACTURER_NAME名字要改，那djysrc里的Iboot_info.c中相应的名字也要改
const char CN_MANUFACTURER_NAME[] = PRODUCT_MANUFACTURER_NAME;


const struct ProductInfo Djy_Product_Info __attribute__ ((section(".DjyProductInfo"))) =
{
    .VersionNumber[0] = PRODUCT_VERSION_LARGE,
    .VersionNumber[1] = PRODUCT_VERSION_MEDIUM,
    .VersionNumber[2] = PRODUCT_VERSION_SMALL,
#if(CN_PTR_BITS < 64)
    .ManufacturerNameAddr      = (u32)(&CN_MANUFACTURER_NAME),
    .ManufacturerNamereserved32    = 0xffffffff,
#else
    .ManufacturerNameAddr      = (u64)(&CN_MANUFACTURER_NAME),
#endif
    .ProductClassify = PRODUCT_PRODUCT_CLASSIFY,
    .ProductType = PRODUCT_PRODUCT_MODEL,

    .TypeCode = PRODUCT_PRODUCT_MODEL_CODE,

    .ProductionTime = {'*','*','*','*'},
    .ProductionNumber = {'*','*','*','*','*'},
    .reserved8 = 0,
    .BoardType = PRODUCT_BOARD_TYPE,
    .CPU_Type = PRODUCT_CPU_TYPE,
    .Reserved ={
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff
            },
};


ptu32_t __djy_main(void)
{
    //modbus
    extern bool_t ModuleInstall_Modbus(void);
    ModuleInstall_Modbus();
    //end modbus

    djy_main();

	return 0;
}

void Sys_ModuleInit(void)
{
	uint16_t evtt_main;

    //shell
    extern void Stdio_KnlInOutInit(char * StdioIn, char *StdioOut);
    Stdio_KnlInOutInit(CFG_STDIO_IN_NAME,CFG_STDIO_OUT_NAME);
    extern s32 ModuleInstall_Shell(ptu32_t para);
    ModuleInstall_Shell(0);
    //end shell

    //----------------------------early----------------------------//
    //black box
    extern void ModuleInstall_BlackBox(void);
    ModuleInstall_BlackBox( );
    //end black box

    //device file system
    extern s32 ModuleInstall_dev(void);
    ModuleInstall_dev();    // 安装设备文件系统；
    //end device file system

    //djybus
    extern bool_t ModuleInstall_DjyBus(void);
    ModuleInstall_DjyBus ( );
    //end djybus

    //message queue
    extern bool_t ModuleInstall_MsgQ(void);
    ModuleInstall_MsgQ ( );
    //end message queue

    //multiplex
    extern bool_t ModuleInstall_Multiplex(void);
    ModuleInstall_Multiplex ();
    //end multiplex

    //spi bus
    extern bool_t ModuleInstall_SPIBus(void);
    ModuleInstall_SPIBus();
    //end spi bus

    //cpu onchip spi
    extern bool_t ModuleInstall_SPI(u8 port);
    #if CFG_SPI1_ENABLE==1
    ModuleInstall_SPI(CN_SPI1);
    #endif
    #if CFG_SPI2_ENABLE==1
    ModuleInstall_SPI(CN_SPI2);
    #endif
    #if CFG_SPI3_ENABLE==1
    ModuleInstall_SPI(CN_SPI3);
    #endif
    #if CFG_SPI4_ENABLE==1
    ModuleInstall_SPI(CN_SPI4);
    #endif
    //end cpu onchip spi

    //xip iboot file system
    extern s32 ModuleInstall_XIP_IBOOT_FS(u32 opt, void *data);
    ModuleInstall_XIP_IBOOT_FS(0,NULL);
    //end xip iboot file system

    //cpu drive inner flash
    s32 ModuleInstall_EmbededFlash(u32 doformat);
    ModuleInstall_EmbededFlash(CFG_EFLASH_PART_FORMAT);
    //end cpu drive inner flash

    //emflash insatall xip
    extern s32 ModuleInstall_EmFlashInstallXIP(const char *TargetFs,s32 bstart, s32 bend, u32 doformat);
    ModuleInstall_EmFlashInstallXIP(CFG_EFLASH_XIPFSMOUNT_NAME,CFG_EFLASH_XIP_PART_START,
    CFG_EFLASH_XIP_PART_END, CFG_EFLASH_XIP_PART_FORMAT);
    //end emflash insatall xip

    //kernel
    #if(CFG_OS_TINY == flase)
    extern s32 kernel_command(void);
    kernel_command();
    #endif
    //end kernel

    //Nls Charset
    extern ptu32_t ModuleInstall_Charset(ptu32_t para);
    ModuleInstall_Charset(0);
    extern void ModuleInstall_CharsetNls(const char * DefaultCharset);
    ModuleInstall_CharsetNls("C");
    //end Nls Charset

    //fat file system
    extern s32 ModuleInstall_FAT(const char *dir, u32 opt, void *data);
    ModuleInstall_FAT(CFG_FAT_MOUNT_POINT, CFG_FAT_MS_INSTALLUSE, CFG_FAT_MEDIA_KIND);
    //end fat file system

    //Software Timers
    extern bool_t ModuleInstall_Timer(void);
    ModuleInstall_Timer();
    //end Software Timers

    //cpu onchip timer
    extern bool_t ModuleInstall_HardTimer(void);
    ModuleInstall_HardTimer();
    //end cpu onchip timer

    //tcpip
    extern bool_t ModuleInstall_TcpIp(void);
    ModuleInstall_TcpIp( );
    //end tcpip

    //cpu onchip ETH
    extern bool_t ModuleInstall_ETH(void);
    ModuleInstall_ETH( );
    //end cpu onchip ETH

    //cpu onchip uart
    extern ptu32_t ModuleInstall_UART(ptu32_t SerialNo);
    #if CFG_UART1_ENABLE ==1
    ModuleInstall_UART(CN_UART1);
    #endif
    #if CFG_UART2_ENABLE ==1
    ModuleInstall_UART(CN_UART2);
    #endif
    #if CFG_UART3_ENABLE ==1
    ModuleInstall_UART(CN_UART3);
    #endif
    #if CFG_UART4_ENABLE ==1
    ModuleInstall_UART(CN_UART4);
    #endif
    #if CFG_UART5_ENABLE ==1
    ModuleInstall_UART(CN_UART5);
    #endif
    #if CFG_UART6_ENABLE ==1
    ModuleInstall_UART(CN_UART6);
    #endif
    #if CFG_UART7_ENABLE ==1
    ModuleInstall_UART(CN_UART7);
    #endif
    #if CFG_UART8_ENABLE ==1
    ModuleInstall_UART(CN_UART8);
    #endif
    //end cpu onchip uart

    //norflash W25QXX
    extern s32 ModuleInstall_W25qxx(void);
    ModuleInstall_W25qxx();
    //end norflash W25QXX

    //W25QXX FAT
    extern bool_t ModuleInstall_W25qxxInstallFat(const char *TargetFs, s32 bend, u32 doformat);
    ModuleInstall_W25qxxInstallFat(CFG_W25_FAT_MOUNT_NAME,CFG_W25_FAT_PART_END,CFG_W25_FAT_PART_FORMAT);
    //end W25QXX FAT

    //----------------------------later----------------------------//

    //stdio
    #if(CFG_STDIO_STDIOFILE == true)
    extern s32 ModuleInstall_STDIO(const char *in,const char *out, const char *err);
    ModuleInstall_STDIO(CFG_STDIO_IN_NAME,CFG_STDIO_OUT_NAME,CFG_STDIO_ERR_NAME);
    #endif
    //end stdio

    //network config
    extern void ModuleInstall_InitNet( );
    ModuleInstall_InitNet( );
    //end network config

	evtt_main = DJY_EvttRegist(EN_CORRELATIVE,CN_PRIO_RRS,0,0,
		__djy_main,NULL,CFG_MAINSTACK_LIMIT, "main function");
	//事件的两个参数暂设为0,如果用shell启动,可用来采集shell命令行参数
	DJY_EventPop(evtt_main,NULL,0,0,0,0);

    //----------------------------medium----------------------------//
    //heap
    #if ((CFG_DYNAMIC_MEM == true))
    extern bool_t Heap_DynamicModuleInit(void);
    Heap_DynamicModuleInit ( );
    #endif
    //end heap



	return ;
}

/*Modified at 2023-12-24 19:48:41*/
/****************************************************
 *  Automatically-generated file. Do not edit!	*
 ****************************************************/

#include "project_config.h"
#include "djyos.h"
#include "stdint.h"
#include "stddef.h"
#include "cpu_peri.h"
#include <Iboot_info.h>

#include <djyfs/filesystems.h>

extern ptu32_t djy_main(void);
//如果这个CN_MANUFACTURER_NAME名字要改，那djysrc里的Iboot_info.c中相应的名字也要改
const char CN_MANUFACTURER_NAME[] = PRODUCT_MANUFACTURER_NAME;


const struct ProductInfo Djy_Product_Info __attribute__ ((section(".DjyProductInfo"))) =
{
    .VersionNumber[0] = PRODUCT_VERSION_LARGE,
    .VersionNumber[1] = PRODUCT_VERSION_MEDIUM,
    .VersionNumber[2] = PRODUCT_VERSION_SMALL,
#if(CN_PTR_BITS < 64)
    .ManufacturerNameAddr      = (u32)(&CN_MANUFACTURER_NAME),
    .ManufacturerNamereserved32    = 0xffffffff,
#else
    .ManufacturerNameAddr      = (u64)(&CN_MANUFACTURER_NAME),
#endif
    .ProductClassify = PRODUCT_PRODUCT_CLASSIFY,
    .ProductType = PRODUCT_PRODUCT_MODEL,

    .TypeCode = PRODUCT_PRODUCT_MODEL_CODE,

    .ProductionTime = {'*','*','*','*'},
    .ProductionNumber = {'*','*','*','*','*'},
    .reserved8 = 0,
    .BoardType = PRODUCT_BOARD_TYPE,
    .CPU_Type = PRODUCT_CPU_TYPE,
    .Reserved ={
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff
            },
};


ptu32_t __djy_main(void)
{
    //modbus
    extern bool_t ModuleInstall_Modbus(void);
    ModuleInstall_Modbus();
    //end modbus

    djy_main();

	return 0;
}

void Sys_ModuleInit(void)
{
	uint16_t evtt_main;

    //shell
    extern void Stdio_KnlInOutInit(char * StdioIn, char *StdioOut);
    Stdio_KnlInOutInit(CFG_STDIO_IN_NAME,CFG_STDIO_OUT_NAME);
    extern s32 ModuleInstall_Shell(ptu32_t para);
    ModuleInstall_Shell(0);
    //end shell

    //----------------------------early----------------------------//
    //black box
    extern void ModuleInstall_BlackBox(void);
    ModuleInstall_BlackBox( );
    //end black box

    //device file system
    extern s32 ModuleInstall_dev(void);
    ModuleInstall_dev();    // 安装设备文件系统；
    //end device file system

    //djybus
    extern bool_t ModuleInstall_DjyBus(void);
    ModuleInstall_DjyBus ( );
    //end djybus

    //message queue
    extern bool_t ModuleInstall_MsgQ(void);
    ModuleInstall_MsgQ ( );
    //end message queue

    //multiplex
    extern bool_t ModuleInstall_Multiplex(void);
    ModuleInstall_Multiplex ();
    //end multiplex

    //spi bus
    extern bool_t ModuleInstall_SPIBus(void);
    ModuleInstall_SPIBus();
    //end spi bus

    //xip iboot file system
    extern s32 ModuleInstall_XIP_IBOOT_FS(u32 opt, void *data);
    ModuleInstall_XIP_IBOOT_FS(0,NULL);
    //end xip iboot file system

    //cpu onchip spi
    extern bool_t ModuleInstall_SPI(u8 port);
    #if CFG_SPI1_ENABLE==1
    ModuleInstall_SPI(CN_SPI1);
    #endif
    #if CFG_SPI2_ENABLE==1
    ModuleInstall_SPI(CN_SPI2);
    #endif
    #if CFG_SPI3_ENABLE==1
    ModuleInstall_SPI(CN_SPI3);
    #endif
    #if CFG_SPI4_ENABLE==1
    ModuleInstall_SPI(CN_SPI4);
    #endif
    //end cpu onchip spi

    //cpu onchip uart
    extern ptu32_t ModuleInstall_UART(ptu32_t SerialNo);
    #if CFG_UART1_ENABLE ==1
    ModuleInstall_UART(CN_UART1);
    #endif
    #if CFG_UART2_ENABLE ==1
    ModuleInstall_UART(CN_UART2);
    #endif
    #if CFG_UART3_ENABLE ==1
    ModuleInstall_UART(CN_UART3);
    #endif
    #if CFG_UART4_ENABLE ==1
    ModuleInstall_UART(CN_UART4);
    #endif
    #if CFG_UART5_ENABLE ==1
    ModuleInstall_UART(CN_UART5);
    #endif
    #if CFG_UART6_ENABLE ==1
    ModuleInstall_UART(CN_UART6);
    #endif
    #if CFG_UART7_ENABLE ==1
    ModuleInstall_UART(CN_UART7);
    #endif
    #if CFG_UART8_ENABLE ==1
    ModuleInstall_UART(CN_UART8);
    #endif
    //end cpu onchip uart

    //fat file system
    extern s32 ModuleInstall_FAT(const char *dir, u32 opt, void *data);
    ModuleInstall_FAT(CFG_FAT_MOUNT_POINT, CFG_FAT_MS_INSTALLUSE, CFG_FAT_MEDIA_KIND);
    //end fat file system

    //cpu onchip timer
    extern bool_t ModuleInstall_HardTimer(void);
    ModuleInstall_HardTimer();
    //end cpu onchip timer

    //cpu drive inner flash
    s32 ModuleInstall_EmbededFlash(u32 doformat);
    ModuleInstall_EmbededFlash(CFG_EFLASH_PART_FORMAT);
    //end cpu drive inner flash

    //emflash insatall xip
    extern s32 ModuleInstall_EmFlashInstallXIP(const char *TargetFs,s32 bstart, s32 bend, u32 doformat);
    ModuleInstall_EmFlashInstallXIP(CFG_EFLASH_XIPFSMOUNT_NAME,CFG_EFLASH_XIP_PART_START,
    CFG_EFLASH_XIP_PART_END, CFG_EFLASH_XIP_PART_FORMAT);
    //end emflash insatall xip

    //kernel
    #if(CFG_OS_TINY == flase)
    extern s32 kernel_command(void);
    kernel_command();
    #endif
    //end kernel

    //Nls Charset
    extern ptu32_t ModuleInstall_Charset(ptu32_t para);
    ModuleInstall_Charset(0);
    extern void ModuleInstall_CharsetNls(const char * DefaultCharset);
    ModuleInstall_CharsetNls("C");
    //end Nls Charset

    //Software Timers
    extern bool_t ModuleInstall_Timer(void);
    ModuleInstall_Timer();
    //end Software Timers

    //tcpip
    extern bool_t ModuleInstall_TcpIp(void);
    ModuleInstall_TcpIp( );
    //end tcpip

    //cpu onchip ETH
    extern bool_t ModuleInstall_ETH(void);
    ModuleInstall_ETH( );
    //end cpu onchip ETH

    //norflash W25QXX
    extern s32 ModuleInstall_W25qxx(void);
    ModuleInstall_W25qxx();
    //end norflash W25QXX

    //W25QXX FAT
    extern bool_t ModuleInstall_W25qxxInstallFat(const char *TargetFs, s32 bend, u32 doformat);
    ModuleInstall_W25qxxInstallFat(CFG_W25_FAT_MOUNT_NAME,CFG_W25_FAT_PART_END,CFG_W25_FAT_PART_FORMAT);
    //end W25QXX FAT

    //----------------------------later----------------------------//
    //stdio
    #if(CFG_STDIO_STDIOFILE == true)
    extern s32 ModuleInstall_STDIO(const char *in,const char *out, const char *err);
    ModuleInstall_STDIO(CFG_STDIO_IN_NAME,CFG_STDIO_OUT_NAME,CFG_STDIO_ERR_NAME);
    #endif
    //end stdio

    //network config
    extern void ModuleInstall_InitNet( );
    ModuleInstall_InitNet( );
    //end network config

	evtt_main = DJY_EvttRegist(EN_CORRELATIVE,CN_PRIO_RRS,0,0,
		__djy_main,NULL,CFG_MAINSTACK_LIMIT, "main function");
	//事件的两个参数暂设为0,如果用shell启动,可用来采集shell命令行参数
	DJY_EventPop(evtt_main,NULL,0,0,0,0);

    //----------------------------medium----------------------------//
    //heap
    #if ((CFG_DYNAMIC_MEM == true))
    extern bool_t Heap_DynamicModuleInit(void);
    Heap_DynamicModuleInit ( );
    #endif
    //end heap



	return ;
}

/*Modified at 2023-12-24 19:55:38*/
/****************************************************
 *  Automatically-generated file. Do not edit!	*
 ****************************************************/

#include "project_config.h"
#include "djyos.h"
#include "stdint.h"
#include "stddef.h"
#include "cpu_peri.h"
#include <Iboot_info.h>

#include <djyfs/filesystems.h>

extern ptu32_t djy_main(void);
//如果这个CN_MANUFACTURER_NAME名字要改，那djysrc里的Iboot_info.c中相应的名字也要改
const char CN_MANUFACTURER_NAME[] = PRODUCT_MANUFACTURER_NAME;


const struct ProductInfo Djy_Product_Info __attribute__ ((section(".DjyProductInfo"))) =
{
    .VersionNumber[0] = PRODUCT_VERSION_LARGE,
    .VersionNumber[1] = PRODUCT_VERSION_MEDIUM,
    .VersionNumber[2] = PRODUCT_VERSION_SMALL,
#if(CN_PTR_BITS < 64)
    .ManufacturerNameAddr      = (u32)(&CN_MANUFACTURER_NAME),
    .ManufacturerNamereserved32    = 0xffffffff,
#else
    .ManufacturerNameAddr      = (u64)(&CN_MANUFACTURER_NAME),
#endif
    .ProductClassify = PRODUCT_PRODUCT_CLASSIFY,
    .ProductType = PRODUCT_PRODUCT_MODEL,

    .TypeCode = PRODUCT_PRODUCT_MODEL_CODE,

    .ProductionTime = {'*','*','*','*'},
    .ProductionNumber = {'*','*','*','*','*'},
    .reserved8 = 0,
    .BoardType = PRODUCT_BOARD_TYPE,
    .CPU_Type = PRODUCT_CPU_TYPE,
    .Reserved ={
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff
            },
};


ptu32_t __djy_main(void)
{
    //modbus
    extern bool_t ModuleInstall_Modbus(void);
    ModuleInstall_Modbus();
    //end modbus

    djy_main();

	return 0;
}

void Sys_ModuleInit(void)
{
	uint16_t evtt_main;

    //shell
    extern void Stdio_KnlInOutInit(char * StdioIn, char *StdioOut);
    Stdio_KnlInOutInit(CFG_STDIO_IN_NAME,CFG_STDIO_OUT_NAME);
    extern s32 ModuleInstall_Shell(ptu32_t para);
    ModuleInstall_Shell(0);
    //end shell

    //----------------------------early----------------------------//
    //black box
    extern void ModuleInstall_BlackBox(void);
    ModuleInstall_BlackBox( );
    //end black box

    //device file system
    extern s32 ModuleInstall_dev(void);
    ModuleInstall_dev();    // 安装设备文件系统；
    //end device file system

    //djybus
    extern bool_t ModuleInstall_DjyBus(void);
    ModuleInstall_DjyBus ( );
    //end djybus

    //message queue
    extern bool_t ModuleInstall_MsgQ(void);
    ModuleInstall_MsgQ ( );
    //end message queue

    //multiplex
    extern bool_t ModuleInstall_Multiplex(void);
    ModuleInstall_Multiplex ();
    //end multiplex

    //spi bus
    extern bool_t ModuleInstall_SPIBus(void);
    ModuleInstall_SPIBus();
    //end spi bus

    //cpu onchip spi
    extern bool_t ModuleInstall_SPI(u8 port);
    #if CFG_SPI1_ENABLE==1
    ModuleInstall_SPI(CN_SPI1);
    #endif
    #if CFG_SPI2_ENABLE==1
    ModuleInstall_SPI(CN_SPI2);
    #endif
    #if CFG_SPI3_ENABLE==1
    ModuleInstall_SPI(CN_SPI3);
    #endif
    #if CFG_SPI4_ENABLE==1
    ModuleInstall_SPI(CN_SPI4);
    #endif
    //end cpu onchip spi

    //xip iboot file system
    extern s32 ModuleInstall_XIP_IBOOT_FS(u32 opt, void *data);
    ModuleInstall_XIP_IBOOT_FS(0,NULL);
    //end xip iboot file system

    //cpu drive inner flash
    s32 ModuleInstall_EmbededFlash(u32 doformat);
    ModuleInstall_EmbededFlash(CFG_EFLASH_PART_FORMAT);
    //end cpu drive inner flash

    //emflash insatall xip
    extern s32 ModuleInstall_EmFlashInstallXIP(const char *TargetFs,s32 bstart, s32 bend, u32 doformat);
    ModuleInstall_EmFlashInstallXIP(CFG_EFLASH_XIPFSMOUNT_NAME,CFG_EFLASH_XIP_PART_START,
    CFG_EFLASH_XIP_PART_END, CFG_EFLASH_XIP_PART_FORMAT);
    //end emflash insatall xip

    //kernel
    #if(CFG_OS_TINY == flase)
    extern s32 kernel_command(void);
    kernel_command();
    #endif
    //end kernel

    //Nls Charset
    extern ptu32_t ModuleInstall_Charset(ptu32_t para);
    ModuleInstall_Charset(0);
    extern void ModuleInstall_CharsetNls(const char * DefaultCharset);
    ModuleInstall_CharsetNls("C");
    //end Nls Charset

    //fat file system
    extern s32 ModuleInstall_FAT(const char *dir, u32 opt, void *data);
    ModuleInstall_FAT(CFG_FAT_MOUNT_POINT, CFG_FAT_MS_INSTALLUSE, CFG_FAT_MEDIA_KIND);
    //end fat file system

    //Software Timers
    extern bool_t ModuleInstall_Timer(void);
    ModuleInstall_Timer();
    //end Software Timers

    //cpu onchip timer
    extern bool_t ModuleInstall_HardTimer(void);
    ModuleInstall_HardTimer();
    //end cpu onchip timer

    //tcpip
    extern bool_t ModuleInstall_TcpIp(void);
    ModuleInstall_TcpIp( );
    //end tcpip

    //cpu onchip ETH
    extern bool_t ModuleInstall_ETH(void);
    ModuleInstall_ETH( );
    //end cpu onchip ETH

    //cpu onchip uart
    extern ptu32_t ModuleInstall_UART(ptu32_t SerialNo);
    #if CFG_UART1_ENABLE ==1
    ModuleInstall_UART(CN_UART1);
    #endif
    #if CFG_UART2_ENABLE ==1
    ModuleInstall_UART(CN_UART2);
    #endif
    #if CFG_UART3_ENABLE ==1
    ModuleInstall_UART(CN_UART3);
    #endif
    #if CFG_UART4_ENABLE ==1
    ModuleInstall_UART(CN_UART4);
    #endif
    #if CFG_UART5_ENABLE ==1
    ModuleInstall_UART(CN_UART5);
    #endif
    #if CFG_UART6_ENABLE ==1
    ModuleInstall_UART(CN_UART6);
    #endif
    #if CFG_UART7_ENABLE ==1
    ModuleInstall_UART(CN_UART7);
    #endif
    #if CFG_UART8_ENABLE ==1
    ModuleInstall_UART(CN_UART8);
    #endif
    //end cpu onchip uart

    //norflash W25QXX
    extern s32 ModuleInstall_W25qxx(void);
    ModuleInstall_W25qxx();
    //end norflash W25QXX

    //W25QXX FAT
    extern bool_t ModuleInstall_W25qxxInstallFat(const char *TargetFs, s32 bend, u32 doformat);
    ModuleInstall_W25qxxInstallFat(CFG_W25_FAT_MOUNT_NAME,CFG_W25_FAT_PART_END,CFG_W25_FAT_PART_FORMAT);
    //end W25QXX FAT

    //----------------------------later----------------------------//
    //stdio
    #if(CFG_STDIO_STDIOFILE == true)
    extern s32 ModuleInstall_STDIO(const char *in,const char *out, const char *err);
    ModuleInstall_STDIO(CFG_STDIO_IN_NAME,CFG_STDIO_OUT_NAME,CFG_STDIO_ERR_NAME);
    #endif
    //end stdio

    //network config
    extern void ModuleInstall_InitNet( );
    ModuleInstall_InitNet( );
    //end network config

	evtt_main = DJY_EvttRegist(EN_CORRELATIVE,CN_PRIO_RRS,0,0,
		__djy_main,NULL,CFG_MAINSTACK_LIMIT, "main function");
	//事件的两个参数暂设为0,如果用shell启动,可用来采集shell命令行参数
	DJY_EventPop(evtt_main,NULL,0,0,0,0);

    //----------------------------medium----------------------------//
    //heap
    #if ((CFG_DYNAMIC_MEM == true))
    extern bool_t Heap_DynamicModuleInit(void);
    Heap_DynamicModuleInit ( );
    #endif
    //end heap



	return ;
}

/*Modified at 2023-12-24 19:55:43*/
/****************************************************
 *  Automatically-generated file. Do not edit!	*
 ****************************************************/

#include "project_config.h"
#include "djyos.h"
#include "stdint.h"
#include "stddef.h"
#include "cpu_peri.h"
#include <Iboot_info.h>

#include <djyfs/filesystems.h>

extern ptu32_t djy_main(void);
//如果这个CN_MANUFACTURER_NAME名字要改，那djysrc里的Iboot_info.c中相应的名字也要改
const char CN_MANUFACTURER_NAME[] = PRODUCT_MANUFACTURER_NAME;


const struct ProductInfo Djy_Product_Info __attribute__ ((section(".DjyProductInfo"))) =
{
    .VersionNumber[0] = PRODUCT_VERSION_LARGE,
    .VersionNumber[1] = PRODUCT_VERSION_MEDIUM,
    .VersionNumber[2] = PRODUCT_VERSION_SMALL,
#if(CN_PTR_BITS < 64)
    .ManufacturerNameAddr      = (u32)(&CN_MANUFACTURER_NAME),
    .ManufacturerNamereserved32    = 0xffffffff,
#else
    .ManufacturerNameAddr      = (u64)(&CN_MANUFACTURER_NAME),
#endif
    .ProductClassify = PRODUCT_PRODUCT_CLASSIFY,
    .ProductType = PRODUCT_PRODUCT_MODEL,

    .TypeCode = PRODUCT_PRODUCT_MODEL_CODE,

    .ProductionTime = {'*','*','*','*'},
    .ProductionNumber = {'*','*','*','*','*'},
    .reserved8 = 0,
    .BoardType = PRODUCT_BOARD_TYPE,
    .CPU_Type = PRODUCT_CPU_TYPE,
    .Reserved ={
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff
            },
};


ptu32_t __djy_main(void)
{
    //modbus
    extern bool_t ModuleInstall_Modbus(void);
    ModuleInstall_Modbus();
    //end modbus

    djy_main();

	return 0;
}

void Sys_ModuleInit(void)
{
	uint16_t evtt_main;

    //shell
    extern void Stdio_KnlInOutInit(char * StdioIn, char *StdioOut);
    Stdio_KnlInOutInit(CFG_STDIO_IN_NAME,CFG_STDIO_OUT_NAME);
    extern s32 ModuleInstall_Shell(ptu32_t para);
    ModuleInstall_Shell(0);
    //end shell

    //----------------------------early----------------------------//
    //black box
    extern void ModuleInstall_BlackBox(void);
    ModuleInstall_BlackBox( );
    //end black box

    //device file system
    extern s32 ModuleInstall_dev(void);
    ModuleInstall_dev();    // 安装设备文件系统；
    //end device file system

    //djybus
    extern bool_t ModuleInstall_DjyBus(void);
    ModuleInstall_DjyBus ( );
    //end djybus

    //message queue
    extern bool_t ModuleInstall_MsgQ(void);
    ModuleInstall_MsgQ ( );
    //end message queue

    //multiplex
    extern bool_t ModuleInstall_Multiplex(void);
    ModuleInstall_Multiplex ();
    //end multiplex

    //spi bus
    extern bool_t ModuleInstall_SPIBus(void);
    ModuleInstall_SPIBus();
    //end spi bus

    //xip iboot file system
    extern s32 ModuleInstall_XIP_IBOOT_FS(u32 opt, void *data);
    ModuleInstall_XIP_IBOOT_FS(0,NULL);
    //end xip iboot file system

    //cpu onchip spi
    extern bool_t ModuleInstall_SPI(u8 port);
    #if CFG_SPI1_ENABLE==1
    ModuleInstall_SPI(CN_SPI1);
    #endif
    #if CFG_SPI2_ENABLE==1
    ModuleInstall_SPI(CN_SPI2);
    #endif
    #if CFG_SPI3_ENABLE==1
    ModuleInstall_SPI(CN_SPI3);
    #endif
    #if CFG_SPI4_ENABLE==1
    ModuleInstall_SPI(CN_SPI4);
    #endif
    //end cpu onchip spi

    //cpu onchip uart
    extern ptu32_t ModuleInstall_UART(ptu32_t SerialNo);
    #if CFG_UART1_ENABLE ==1
    ModuleInstall_UART(CN_UART1);
    #endif
    #if CFG_UART2_ENABLE ==1
    ModuleInstall_UART(CN_UART2);
    #endif
    #if CFG_UART3_ENABLE ==1
    ModuleInstall_UART(CN_UART3);
    #endif
    #if CFG_UART4_ENABLE ==1
    ModuleInstall_UART(CN_UART4);
    #endif
    #if CFG_UART5_ENABLE ==1
    ModuleInstall_UART(CN_UART5);
    #endif
    #if CFG_UART6_ENABLE ==1
    ModuleInstall_UART(CN_UART6);
    #endif
    #if CFG_UART7_ENABLE ==1
    ModuleInstall_UART(CN_UART7);
    #endif
    #if CFG_UART8_ENABLE ==1
    ModuleInstall_UART(CN_UART8);
    #endif
    //end cpu onchip uart

    //fat file system
    extern s32 ModuleInstall_FAT(const char *dir, u32 opt, void *data);
    ModuleInstall_FAT(CFG_FAT_MOUNT_POINT, CFG_FAT_MS_INSTALLUSE, CFG_FAT_MEDIA_KIND);
    //end fat file system

    //cpu onchip timer
    extern bool_t ModuleInstall_HardTimer(void);
    ModuleInstall_HardTimer();
    //end cpu onchip timer

    //cpu drive inner flash
    s32 ModuleInstall_EmbededFlash(u32 doformat);
    ModuleInstall_EmbededFlash(CFG_EFLASH_PART_FORMAT);
    //end cpu drive inner flash

    //emflash insatall xip
    extern s32 ModuleInstall_EmFlashInstallXIP(const char *TargetFs,s32 bstart, s32 bend, u32 doformat);
    ModuleInstall_EmFlashInstallXIP(CFG_EFLASH_XIPFSMOUNT_NAME,CFG_EFLASH_XIP_PART_START,
    CFG_EFLASH_XIP_PART_END, CFG_EFLASH_XIP_PART_FORMAT);
    //end emflash insatall xip

    //kernel
    #if(CFG_OS_TINY == flase)
    extern s32 kernel_command(void);
    kernel_command();
    #endif
    //end kernel

    //Nls Charset
    extern ptu32_t ModuleInstall_Charset(ptu32_t para);
    ModuleInstall_Charset(0);
    extern void ModuleInstall_CharsetNls(const char * DefaultCharset);
    ModuleInstall_CharsetNls("C");
    //end Nls Charset

    //Software Timers
    extern bool_t ModuleInstall_Timer(void);
    ModuleInstall_Timer();
    //end Software Timers

    //tcpip
    extern bool_t ModuleInstall_TcpIp(void);
    ModuleInstall_TcpIp( );
    //end tcpip

    //cpu onchip ETH
    extern bool_t ModuleInstall_ETH(void);
    ModuleInstall_ETH( );
    //end cpu onchip ETH

    //norflash W25QXX
    extern s32 ModuleInstall_W25qxx(void);
    ModuleInstall_W25qxx();
    //end norflash W25QXX

    //W25QXX FAT
    extern bool_t ModuleInstall_W25qxxInstallFat(const char *TargetFs, s32 bend, u32 doformat);
    ModuleInstall_W25qxxInstallFat(CFG_W25_FAT_MOUNT_NAME,CFG_W25_FAT_PART_END,CFG_W25_FAT_PART_FORMAT);
    //end W25QXX FAT

    //----------------------------later----------------------------//
    //stdio
    #if(CFG_STDIO_STDIOFILE == true)
    extern s32 ModuleInstall_STDIO(const char *in,const char *out, const char *err);
    ModuleInstall_STDIO(CFG_STDIO_IN_NAME,CFG_STDIO_OUT_NAME,CFG_STDIO_ERR_NAME);
    #endif
    //end stdio

    //network config
    extern void ModuleInstall_InitNet( );
    ModuleInstall_InitNet( );
    //end network config

	evtt_main = DJY_EvttRegist(EN_CORRELATIVE,CN_PRIO_RRS,0,0,
		__djy_main,NULL,CFG_MAINSTACK_LIMIT, "main function");
	//事件的两个参数暂设为0,如果用shell启动,可用来采集shell命令行参数
	DJY_EventPop(evtt_main,NULL,0,0,0,0);

    //----------------------------medium----------------------------//
    //heap
    #if ((CFG_DYNAMIC_MEM == true))
    extern bool_t Heap_DynamicModuleInit(void);
    Heap_DynamicModuleInit ( );
    #endif
    //end heap



	return ;
}

/*Modified at 2023-12-24 19:55:50*/
/****************************************************
 *  Automatically-generated file. Do not edit!	*
 ****************************************************/

#include "project_config.h"
#include "djyos.h"
#include "stdint.h"
#include "stddef.h"
#include "cpu_peri.h"
#include <Iboot_info.h>

#include <djyfs/filesystems.h>

extern ptu32_t djy_main(void);
//如果这个CN_MANUFACTURER_NAME名字要改，那djysrc里的Iboot_info.c中相应的名字也要改
const char CN_MANUFACTURER_NAME[] = PRODUCT_MANUFACTURER_NAME;


const struct ProductInfo Djy_Product_Info __attribute__ ((section(".DjyProductInfo"))) =
{
    .VersionNumber[0] = PRODUCT_VERSION_LARGE,
    .VersionNumber[1] = PRODUCT_VERSION_MEDIUM,
    .VersionNumber[2] = PRODUCT_VERSION_SMALL,
#if(CN_PTR_BITS < 64)
    .ManufacturerNameAddr      = (u32)(&CN_MANUFACTURER_NAME),
    .ManufacturerNamereserved32    = 0xffffffff,
#else
    .ManufacturerNameAddr      = (u64)(&CN_MANUFACTURER_NAME),
#endif
    .ProductClassify = PRODUCT_PRODUCT_CLASSIFY,
    .ProductType = PRODUCT_PRODUCT_MODEL,

    .TypeCode = PRODUCT_PRODUCT_MODEL_CODE,

    .ProductionTime = {'*','*','*','*'},
    .ProductionNumber = {'*','*','*','*','*'},
    .reserved8 = 0,
    .BoardType = PRODUCT_BOARD_TYPE,
    .CPU_Type = PRODUCT_CPU_TYPE,
    .Reserved ={
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff
            },
};


ptu32_t __djy_main(void)
{
    //modbus
    extern bool_t ModuleInstall_Modbus(void);
    ModuleInstall_Modbus();
    //end modbus

    djy_main();

	return 0;
}

void Sys_ModuleInit(void)
{
	uint16_t evtt_main;

    //shell
    extern void Stdio_KnlInOutInit(char * StdioIn, char *StdioOut);
    Stdio_KnlInOutInit(CFG_STDIO_IN_NAME,CFG_STDIO_OUT_NAME);
    extern s32 ModuleInstall_Shell(ptu32_t para);
    ModuleInstall_Shell(0);
    //end shell

    //----------------------------early----------------------------//
    //black box
    extern void ModuleInstall_BlackBox(void);
    ModuleInstall_BlackBox( );
    //end black box

    //device file system
    extern s32 ModuleInstall_dev(void);
    ModuleInstall_dev();    // 安装设备文件系统；
    //end device file system

    //djybus
    extern bool_t ModuleInstall_DjyBus(void);
    ModuleInstall_DjyBus ( );
    //end djybus

    //message queue
    extern bool_t ModuleInstall_MsgQ(void);
    ModuleInstall_MsgQ ( );
    //end message queue

    //multiplex
    extern bool_t ModuleInstall_Multiplex(void);
    ModuleInstall_Multiplex ();
    //end multiplex

    //spi bus
    extern bool_t ModuleInstall_SPIBus(void);
    ModuleInstall_SPIBus();
    //end spi bus

    //cpu onchip spi
    extern bool_t ModuleInstall_SPI(u8 port);
    #if CFG_SPI1_ENABLE==1
    ModuleInstall_SPI(CN_SPI1);
    #endif
    #if CFG_SPI2_ENABLE==1
    ModuleInstall_SPI(CN_SPI2);
    #endif
    #if CFG_SPI3_ENABLE==1
    ModuleInstall_SPI(CN_SPI3);
    #endif
    #if CFG_SPI4_ENABLE==1
    ModuleInstall_SPI(CN_SPI4);
    #endif
    //end cpu onchip spi

    //xip iboot file system
    extern s32 ModuleInstall_XIP_IBOOT_FS(u32 opt, void *data);
    ModuleInstall_XIP_IBOOT_FS(0,NULL);
    //end xip iboot file system

    //cpu drive inner flash
    s32 ModuleInstall_EmbededFlash(u32 doformat);
    ModuleInstall_EmbededFlash(CFG_EFLASH_PART_FORMAT);
    //end cpu drive inner flash

    //emflash insatall xip
    extern s32 ModuleInstall_EmFlashInstallXIP(const char *TargetFs,s32 bstart, s32 bend, u32 doformat);
    ModuleInstall_EmFlashInstallXIP(CFG_EFLASH_XIPFSMOUNT_NAME,CFG_EFLASH_XIP_PART_START,
    CFG_EFLASH_XIP_PART_END, CFG_EFLASH_XIP_PART_FORMAT);
    //end emflash insatall xip

    //kernel
    #if(CFG_OS_TINY == flase)
    extern s32 kernel_command(void);
    kernel_command();
    #endif
    //end kernel

    //Nls Charset
    extern ptu32_t ModuleInstall_Charset(ptu32_t para);
    ModuleInstall_Charset(0);
    extern void ModuleInstall_CharsetNls(const char * DefaultCharset);
    ModuleInstall_CharsetNls("C");
    //end Nls Charset

    //fat file system
    extern s32 ModuleInstall_FAT(const char *dir, u32 opt, void *data);
    ModuleInstall_FAT(CFG_FAT_MOUNT_POINT, CFG_FAT_MS_INSTALLUSE, CFG_FAT_MEDIA_KIND);
    //end fat file system

    //Software Timers
    extern bool_t ModuleInstall_Timer(void);
    ModuleInstall_Timer();
    //end Software Timers

    //cpu onchip timer
    extern bool_t ModuleInstall_HardTimer(void);
    ModuleInstall_HardTimer();
    //end cpu onchip timer

    //tcpip
    extern bool_t ModuleInstall_TcpIp(void);
    ModuleInstall_TcpIp( );
    //end tcpip

    //cpu onchip ETH
    extern bool_t ModuleInstall_ETH(void);
    ModuleInstall_ETH( );
    //end cpu onchip ETH

    //cpu onchip uart
    extern ptu32_t ModuleInstall_UART(ptu32_t SerialNo);
    #if CFG_UART1_ENABLE ==1
    ModuleInstall_UART(CN_UART1);
    #endif
    #if CFG_UART2_ENABLE ==1
    ModuleInstall_UART(CN_UART2);
    #endif
    #if CFG_UART3_ENABLE ==1
    ModuleInstall_UART(CN_UART3);
    #endif
    #if CFG_UART4_ENABLE ==1
    ModuleInstall_UART(CN_UART4);
    #endif
    #if CFG_UART5_ENABLE ==1
    ModuleInstall_UART(CN_UART5);
    #endif
    #if CFG_UART6_ENABLE ==1
    ModuleInstall_UART(CN_UART6);
    #endif
    #if CFG_UART7_ENABLE ==1
    ModuleInstall_UART(CN_UART7);
    #endif
    #if CFG_UART8_ENABLE ==1
    ModuleInstall_UART(CN_UART8);
    #endif
    //end cpu onchip uart

    //norflash W25QXX
    extern s32 ModuleInstall_W25qxx(void);
    ModuleInstall_W25qxx();
    //end norflash W25QXX

    //W25QXX FAT
    extern bool_t ModuleInstall_W25qxxInstallFat(const char *TargetFs, s32 bend, u32 doformat);
    ModuleInstall_W25qxxInstallFat(CFG_W25_FAT_MOUNT_NAME,CFG_W25_FAT_PART_END,CFG_W25_FAT_PART_FORMAT);
    //end W25QXX FAT

    //----------------------------later----------------------------//
    //stdio
    #if(CFG_STDIO_STDIOFILE == true)
    extern s32 ModuleInstall_STDIO(const char *in,const char *out, const char *err);
    ModuleInstall_STDIO(CFG_STDIO_IN_NAME,CFG_STDIO_OUT_NAME,CFG_STDIO_ERR_NAME);
    #endif
    //end stdio

    //network config
    extern void ModuleInstall_InitNet( );
    ModuleInstall_InitNet( );
    //end network config

	evtt_main = DJY_EvttRegist(EN_CORRELATIVE,CN_PRIO_RRS,0,0,
		__djy_main,NULL,CFG_MAINSTACK_LIMIT, "main function");
	//事件的两个参数暂设为0,如果用shell启动,可用来采集shell命令行参数
	DJY_EventPop(evtt_main,NULL,0,0,0,0);

    //----------------------------medium----------------------------//
    //heap
    #if ((CFG_DYNAMIC_MEM == true))
    extern bool_t Heap_DynamicModuleInit(void);
    Heap_DynamicModuleInit ( );
    #endif
    //end heap



	return ;
}

/*Modified at 2023-12-24 19:55:54*/
/****************************************************
 *  Automatically-generated file. Do not edit!	*
 ****************************************************/

#include "project_config.h"
#include "djyos.h"
#include "stdint.h"
#include "stddef.h"
#include "cpu_peri.h"
#include <Iboot_info.h>

#include <djyfs/filesystems.h>

extern ptu32_t djy_main(void);
//如果这个CN_MANUFACTURER_NAME名字要改，那djysrc里的Iboot_info.c中相应的名字也要改
const char CN_MANUFACTURER_NAME[] = PRODUCT_MANUFACTURER_NAME;


const struct ProductInfo Djy_Product_Info __attribute__ ((section(".DjyProductInfo"))) =
{
    .VersionNumber[0] = PRODUCT_VERSION_LARGE,
    .VersionNumber[1] = PRODUCT_VERSION_MEDIUM,
    .VersionNumber[2] = PRODUCT_VERSION_SMALL,
#if(CN_PTR_BITS < 64)
    .ManufacturerNameAddr      = (u32)(&CN_MANUFACTURER_NAME),
    .ManufacturerNamereserved32    = 0xffffffff,
#else
    .ManufacturerNameAddr      = (u64)(&CN_MANUFACTURER_NAME),
#endif
    .ProductClassify = PRODUCT_PRODUCT_CLASSIFY,
    .ProductType = PRODUCT_PRODUCT_MODEL,

    .TypeCode = PRODUCT_PRODUCT_MODEL_CODE,

    .ProductionTime = {'*','*','*','*'},
    .ProductionNumber = {'*','*','*','*','*'},
    .reserved8 = 0,
    .BoardType = PRODUCT_BOARD_TYPE,
    .CPU_Type = PRODUCT_CPU_TYPE,
    .Reserved ={
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff
            },
};


ptu32_t __djy_main(void)
{
    //modbus
    extern bool_t ModuleInstall_Modbus(void);
    ModuleInstall_Modbus();
    //end modbus

    djy_main();

	return 0;
}

void Sys_ModuleInit(void)
{
	uint16_t evtt_main;

    //shell
    extern void Stdio_KnlInOutInit(char * StdioIn, char *StdioOut);
    Stdio_KnlInOutInit(CFG_STDIO_IN_NAME,CFG_STDIO_OUT_NAME);
    extern s32 ModuleInstall_Shell(ptu32_t para);
    ModuleInstall_Shell(0);
    //end shell

    //----------------------------early----------------------------//
    //black box
    extern void ModuleInstall_BlackBox(void);
    ModuleInstall_BlackBox( );
    //end black box

    //device file system
    extern s32 ModuleInstall_dev(void);
    ModuleInstall_dev();    // 安装设备文件系统；
    //end device file system

    //djybus
    extern bool_t ModuleInstall_DjyBus(void);
    ModuleInstall_DjyBus ( );
    //end djybus

    //message queue
    extern bool_t ModuleInstall_MsgQ(void);
    ModuleInstall_MsgQ ( );
    //end message queue

    //multiplex
    extern bool_t ModuleInstall_Multiplex(void);
    ModuleInstall_Multiplex ();
    //end multiplex

    //spi bus
    extern bool_t ModuleInstall_SPIBus(void);
    ModuleInstall_SPIBus();
    //end spi bus

    //xip iboot file system
    extern s32 ModuleInstall_XIP_IBOOT_FS(u32 opt, void *data);
    ModuleInstall_XIP_IBOOT_FS(0,NULL);
    //end xip iboot file system

    //cpu onchip spi
    extern bool_t ModuleInstall_SPI(u8 port);
    #if CFG_SPI1_ENABLE==1
    ModuleInstall_SPI(CN_SPI1);
    #endif
    #if CFG_SPI2_ENABLE==1
    ModuleInstall_SPI(CN_SPI2);
    #endif
    #if CFG_SPI3_ENABLE==1
    ModuleInstall_SPI(CN_SPI3);
    #endif
    #if CFG_SPI4_ENABLE==1
    ModuleInstall_SPI(CN_SPI4);
    #endif
    //end cpu onchip spi

    //cpu onchip uart
    extern ptu32_t ModuleInstall_UART(ptu32_t SerialNo);
    #if CFG_UART1_ENABLE ==1
    ModuleInstall_UART(CN_UART1);
    #endif
    #if CFG_UART2_ENABLE ==1
    ModuleInstall_UART(CN_UART2);
    #endif
    #if CFG_UART3_ENABLE ==1
    ModuleInstall_UART(CN_UART3);
    #endif
    #if CFG_UART4_ENABLE ==1
    ModuleInstall_UART(CN_UART4);
    #endif
    #if CFG_UART5_ENABLE ==1
    ModuleInstall_UART(CN_UART5);
    #endif
    #if CFG_UART6_ENABLE ==1
    ModuleInstall_UART(CN_UART6);
    #endif
    #if CFG_UART7_ENABLE ==1
    ModuleInstall_UART(CN_UART7);
    #endif
    #if CFG_UART8_ENABLE ==1
    ModuleInstall_UART(CN_UART8);
    #endif
    //end cpu onchip uart

    //fat file system
    extern s32 ModuleInstall_FAT(const char *dir, u32 opt, void *data);
    ModuleInstall_FAT(CFG_FAT_MOUNT_POINT, CFG_FAT_MS_INSTALLUSE, CFG_FAT_MEDIA_KIND);
    //end fat file system

    //cpu onchip timer
    extern bool_t ModuleInstall_HardTimer(void);
    ModuleInstall_HardTimer();
    //end cpu onchip timer

    //cpu drive inner flash
    s32 ModuleInstall_EmbededFlash(u32 doformat);
    ModuleInstall_EmbededFlash(CFG_EFLASH_PART_FORMAT);
    //end cpu drive inner flash

    //emflash insatall xip
    extern s32 ModuleInstall_EmFlashInstallXIP(const char *TargetFs,s32 bstart, s32 bend, u32 doformat);
    ModuleInstall_EmFlashInstallXIP(CFG_EFLASH_XIPFSMOUNT_NAME,CFG_EFLASH_XIP_PART_START,
    CFG_EFLASH_XIP_PART_END, CFG_EFLASH_XIP_PART_FORMAT);
    //end emflash insatall xip

    //kernel
    #if(CFG_OS_TINY == flase)
    extern s32 kernel_command(void);
    kernel_command();
    #endif
    //end kernel

    //Nls Charset
    extern ptu32_t ModuleInstall_Charset(ptu32_t para);
    ModuleInstall_Charset(0);
    extern void ModuleInstall_CharsetNls(const char * DefaultCharset);
    ModuleInstall_CharsetNls("C");
    //end Nls Charset

    //Software Timers
    extern bool_t ModuleInstall_Timer(void);
    ModuleInstall_Timer();
    //end Software Timers

    //tcpip
    extern bool_t ModuleInstall_TcpIp(void);
    ModuleInstall_TcpIp( );
    //end tcpip

    //cpu onchip ETH
    extern bool_t ModuleInstall_ETH(void);
    ModuleInstall_ETH( );
    //end cpu onchip ETH

    //norflash W25QXX
    extern s32 ModuleInstall_W25qxx(void);
    ModuleInstall_W25qxx();
    //end norflash W25QXX

    //W25QXX FAT
    extern bool_t ModuleInstall_W25qxxInstallFat(const char *TargetFs, s32 bend, u32 doformat);
    ModuleInstall_W25qxxInstallFat(CFG_W25_FAT_MOUNT_NAME,CFG_W25_FAT_PART_END,CFG_W25_FAT_PART_FORMAT);
    //end W25QXX FAT

    //----------------------------later----------------------------//
    //stdio
    #if(CFG_STDIO_STDIOFILE == true)
    extern s32 ModuleInstall_STDIO(const char *in,const char *out, const char *err);
    ModuleInstall_STDIO(CFG_STDIO_IN_NAME,CFG_STDIO_OUT_NAME,CFG_STDIO_ERR_NAME);
    #endif
    //end stdio

    //network config
    extern void ModuleInstall_InitNet( );
    ModuleInstall_InitNet( );
    //end network config

	evtt_main = DJY_EvttRegist(EN_CORRELATIVE,CN_PRIO_RRS,0,0,
		__djy_main,NULL,CFG_MAINSTACK_LIMIT, "main function");
	//事件的两个参数暂设为0,如果用shell启动,可用来采集shell命令行参数
	DJY_EventPop(evtt_main,NULL,0,0,0,0);

    //----------------------------medium----------------------------//
    //heap
    #if ((CFG_DYNAMIC_MEM == true))
    extern bool_t Heap_DynamicModuleInit(void);
    Heap_DynamicModuleInit ( );
    #endif
    //end heap



	return ;
}

/*Modified at 2023-12-24 19:58:31*/
/****************************************************
 *  Automatically-generated file. Do not edit!	*
 ****************************************************/

#include "project_config.h"
#include "djyos.h"
#include "stdint.h"
#include "stddef.h"
#include "cpu_peri.h"
#include <Iboot_info.h>

#include <djyfs/filesystems.h>

extern ptu32_t djy_main(void);
//如果这个CN_MANUFACTURER_NAME名字要改，那djysrc里的Iboot_info.c中相应的名字也要改
const char CN_MANUFACTURER_NAME[] = PRODUCT_MANUFACTURER_NAME;


const struct ProductInfo Djy_Product_Info __attribute__ ((section(".DjyProductInfo"))) =
{
    .VersionNumber[0] = PRODUCT_VERSION_LARGE,
    .VersionNumber[1] = PRODUCT_VERSION_MEDIUM,
    .VersionNumber[2] = PRODUCT_VERSION_SMALL,
#if(CN_PTR_BITS < 64)
    .ManufacturerNameAddr      = (u32)(&CN_MANUFACTURER_NAME),
    .ManufacturerNamereserved32    = 0xffffffff,
#else
    .ManufacturerNameAddr      = (u64)(&CN_MANUFACTURER_NAME),
#endif
    .ProductClassify = PRODUCT_PRODUCT_CLASSIFY,
    .ProductType = PRODUCT_PRODUCT_MODEL,

    .TypeCode = PRODUCT_PRODUCT_MODEL_CODE,

    .ProductionTime = {'*','*','*','*'},
    .ProductionNumber = {'*','*','*','*','*'},
    .reserved8 = 0,
    .BoardType = PRODUCT_BOARD_TYPE,
    .CPU_Type = PRODUCT_CPU_TYPE,
    .Reserved ={
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff
            },
};


ptu32_t __djy_main(void)
{
    //modbus
    extern bool_t ModuleInstall_Modbus(void);
    ModuleInstall_Modbus();
    //end modbus

    djy_main();

	return 0;
}

void Sys_ModuleInit(void)
{
	uint16_t evtt_main;

    //shell
    extern void Stdio_KnlInOutInit(char * StdioIn, char *StdioOut);
    Stdio_KnlInOutInit(CFG_STDIO_IN_NAME,CFG_STDIO_OUT_NAME);
    extern s32 ModuleInstall_Shell(ptu32_t para);
    ModuleInstall_Shell(0);
    //end shell

    //----------------------------early----------------------------//
    //black box
    extern void ModuleInstall_BlackBox(void);
    ModuleInstall_BlackBox( );
    //end black box

    //device file system
    extern s32 ModuleInstall_dev(void);
    ModuleInstall_dev();    // 安装设备文件系统；
    //end device file system

    //djybus
    extern bool_t ModuleInstall_DjyBus(void);
    ModuleInstall_DjyBus ( );
    //end djybus

    //message queue
    extern bool_t ModuleInstall_MsgQ(void);
    ModuleInstall_MsgQ ( );
    //end message queue

    //multiplex
    extern bool_t ModuleInstall_Multiplex(void);
    ModuleInstall_Multiplex ();
    //end multiplex

    //spi bus
    extern bool_t ModuleInstall_SPIBus(void);
    ModuleInstall_SPIBus();
    //end spi bus

    //cpu onchip spi
    extern bool_t ModuleInstall_SPI(u8 port);
    #if CFG_SPI1_ENABLE==1
    ModuleInstall_SPI(CN_SPI1);
    #endif
    #if CFG_SPI2_ENABLE==1
    ModuleInstall_SPI(CN_SPI2);
    #endif
    #if CFG_SPI3_ENABLE==1
    ModuleInstall_SPI(CN_SPI3);
    #endif
    #if CFG_SPI4_ENABLE==1
    ModuleInstall_SPI(CN_SPI4);
    #endif
    //end cpu onchip spi

    //xip iboot file system
    extern s32 ModuleInstall_XIP_IBOOT_FS(u32 opt, void *data);
    ModuleInstall_XIP_IBOOT_FS(0,NULL);
    //end xip iboot file system

    //cpu drive inner flash
    s32 ModuleInstall_EmbededFlash(u32 doformat);
    ModuleInstall_EmbededFlash(CFG_EFLASH_PART_FORMAT);
    //end cpu drive inner flash

    //emflash insatall xip
    extern s32 ModuleInstall_EmFlashInstallXIP(const char *TargetFs,s32 bstart, s32 bend, u32 doformat);
    ModuleInstall_EmFlashInstallXIP(CFG_EFLASH_XIPFSMOUNT_NAME,CFG_EFLASH_XIP_PART_START,
    CFG_EFLASH_XIP_PART_END, CFG_EFLASH_XIP_PART_FORMAT);
    //end emflash insatall xip

    //kernel
    #if(CFG_OS_TINY == flase)
    extern s32 kernel_command(void);
    kernel_command();
    #endif
    //end kernel

    //Nls Charset
    extern ptu32_t ModuleInstall_Charset(ptu32_t para);
    ModuleInstall_Charset(0);
    extern void ModuleInstall_CharsetNls(const char * DefaultCharset);
    ModuleInstall_CharsetNls("C");
    //end Nls Charset

    //fat file system
    extern s32 ModuleInstall_FAT(const char *dir, u32 opt, void *data);
    ModuleInstall_FAT(CFG_FAT_MOUNT_POINT, CFG_FAT_MS_INSTALLUSE, CFG_FAT_MEDIA_KIND);
    //end fat file system

    //Software Timers
    extern bool_t ModuleInstall_Timer(void);
    ModuleInstall_Timer();
    //end Software Timers

    //cpu onchip timer
    extern bool_t ModuleInstall_HardTimer(void);
    ModuleInstall_HardTimer();
    //end cpu onchip timer

    //tcpip
    extern bool_t ModuleInstall_TcpIp(void);
    ModuleInstall_TcpIp( );
    //end tcpip

    //cpu onchip ETH
    extern bool_t ModuleInstall_ETH(void);
    ModuleInstall_ETH( );
    //end cpu onchip ETH

    //cpu onchip uart
    extern ptu32_t ModuleInstall_UART(ptu32_t SerialNo);
    #if CFG_UART1_ENABLE ==1
    ModuleInstall_UART(CN_UART1);
    #endif
    #if CFG_UART2_ENABLE ==1
    ModuleInstall_UART(CN_UART2);
    #endif
    #if CFG_UART3_ENABLE ==1
    ModuleInstall_UART(CN_UART3);
    #endif
    #if CFG_UART4_ENABLE ==1
    ModuleInstall_UART(CN_UART4);
    #endif
    #if CFG_UART5_ENABLE ==1
    ModuleInstall_UART(CN_UART5);
    #endif
    #if CFG_UART6_ENABLE ==1
    ModuleInstall_UART(CN_UART6);
    #endif
    #if CFG_UART7_ENABLE ==1
    ModuleInstall_UART(CN_UART7);
    #endif
    #if CFG_UART8_ENABLE ==1
    ModuleInstall_UART(CN_UART8);
    #endif
    //end cpu onchip uart

    //norflash W25QXX
    extern s32 ModuleInstall_W25qxx(void);
    ModuleInstall_W25qxx();
    //end norflash W25QXX

    //W25QXX FAT
    extern bool_t ModuleInstall_W25qxxInstallFat(const char *TargetFs, s32 bend, u32 doformat);
    ModuleInstall_W25qxxInstallFat(CFG_W25_FAT_MOUNT_NAME,CFG_W25_FAT_PART_END,CFG_W25_FAT_PART_FORMAT);
    //end W25QXX FAT

    //----------------------------later----------------------------//
    //stdio
    #if(CFG_STDIO_STDIOFILE == true)
    extern s32 ModuleInstall_STDIO(const char *in,const char *out, const char *err);
    ModuleInstall_STDIO(CFG_STDIO_IN_NAME,CFG_STDIO_OUT_NAME,CFG_STDIO_ERR_NAME);
    #endif
    //end stdio

    //network config
    extern void ModuleInstall_InitNet( );
    ModuleInstall_InitNet( );
    //end network config

	evtt_main = DJY_EvttRegist(EN_CORRELATIVE,CN_PRIO_RRS,0,0,
		__djy_main,NULL,CFG_MAINSTACK_LIMIT, "main function");
	//事件的两个参数暂设为0,如果用shell启动,可用来采集shell命令行参数
	DJY_EventPop(evtt_main,NULL,0,0,0,0);

    //----------------------------medium----------------------------//
    //heap
    #if ((CFG_DYNAMIC_MEM == true))
    extern bool_t Heap_DynamicModuleInit(void);
    Heap_DynamicModuleInit ( );
    #endif
    //end heap



	return ;
}

/*Modified at 2023-12-24 19:58:35*/
/****************************************************
 *  Automatically-generated file. Do not edit!	*
 ****************************************************/

#include "project_config.h"
#include "djyos.h"
#include "stdint.h"
#include "stddef.h"
#include "cpu_peri.h"
#include <Iboot_info.h>

#include <djyfs/filesystems.h>

extern ptu32_t djy_main(void);
//如果这个CN_MANUFACTURER_NAME名字要改，那djysrc里的Iboot_info.c中相应的名字也要改
const char CN_MANUFACTURER_NAME[] = PRODUCT_MANUFACTURER_NAME;


const struct ProductInfo Djy_Product_Info __attribute__ ((section(".DjyProductInfo"))) =
{
    .VersionNumber[0] = PRODUCT_VERSION_LARGE,
    .VersionNumber[1] = PRODUCT_VERSION_MEDIUM,
    .VersionNumber[2] = PRODUCT_VERSION_SMALL,
#if(CN_PTR_BITS < 64)
    .ManufacturerNameAddr      = (u32)(&CN_MANUFACTURER_NAME),
    .ManufacturerNamereserved32    = 0xffffffff,
#else
    .ManufacturerNameAddr      = (u64)(&CN_MANUFACTURER_NAME),
#endif
    .ProductClassify = PRODUCT_PRODUCT_CLASSIFY,
    .ProductType = PRODUCT_PRODUCT_MODEL,

    .TypeCode = PRODUCT_PRODUCT_MODEL_CODE,

    .ProductionTime = {'*','*','*','*'},
    .ProductionNumber = {'*','*','*','*','*'},
    .reserved8 = 0,
    .BoardType = PRODUCT_BOARD_TYPE,
    .CPU_Type = PRODUCT_CPU_TYPE,
    .Reserved ={
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff
            },
};


ptu32_t __djy_main(void)
{
    //modbus
    extern bool_t ModuleInstall_Modbus(void);
    ModuleInstall_Modbus();
    //end modbus

    djy_main();

	return 0;
}

void Sys_ModuleInit(void)
{
	uint16_t evtt_main;

    //shell
    extern void Stdio_KnlInOutInit(char * StdioIn, char *StdioOut);
    Stdio_KnlInOutInit(CFG_STDIO_IN_NAME,CFG_STDIO_OUT_NAME);
    extern s32 ModuleInstall_Shell(ptu32_t para);
    ModuleInstall_Shell(0);
    //end shell

    //----------------------------early----------------------------//
    //black box
    extern void ModuleInstall_BlackBox(void);
    ModuleInstall_BlackBox( );
    //end black box

    //device file system
    extern s32 ModuleInstall_dev(void);
    ModuleInstall_dev();    // 安装设备文件系统；
    //end device file system

    //djybus
    extern bool_t ModuleInstall_DjyBus(void);
    ModuleInstall_DjyBus ( );
    //end djybus

    //message queue
    extern bool_t ModuleInstall_MsgQ(void);
    ModuleInstall_MsgQ ( );
    //end message queue

    //multiplex
    extern bool_t ModuleInstall_Multiplex(void);
    ModuleInstall_Multiplex ();
    //end multiplex

    //spi bus
    extern bool_t ModuleInstall_SPIBus(void);
    ModuleInstall_SPIBus();
    //end spi bus

    //xip iboot file system
    extern s32 ModuleInstall_XIP_IBOOT_FS(u32 opt, void *data);
    ModuleInstall_XIP_IBOOT_FS(0,NULL);
    //end xip iboot file system

    //cpu onchip spi
    extern bool_t ModuleInstall_SPI(u8 port);
    #if CFG_SPI1_ENABLE==1
    ModuleInstall_SPI(CN_SPI1);
    #endif
    #if CFG_SPI2_ENABLE==1
    ModuleInstall_SPI(CN_SPI2);
    #endif
    #if CFG_SPI3_ENABLE==1
    ModuleInstall_SPI(CN_SPI3);
    #endif
    #if CFG_SPI4_ENABLE==1
    ModuleInstall_SPI(CN_SPI4);
    #endif
    //end cpu onchip spi

    //fat file system
    extern s32 ModuleInstall_FAT(const char *dir, u32 opt, void *data);
    ModuleInstall_FAT(CFG_FAT_MOUNT_POINT, CFG_FAT_MS_INSTALLUSE, CFG_FAT_MEDIA_KIND);
    //end fat file system

    //cpu onchip timer
    extern bool_t ModuleInstall_HardTimer(void);
    ModuleInstall_HardTimer();
    //end cpu onchip timer

    //cpu drive inner flash
    s32 ModuleInstall_EmbededFlash(u32 doformat);
    ModuleInstall_EmbededFlash(CFG_EFLASH_PART_FORMAT);
    //end cpu drive inner flash

    //emflash insatall xip
    extern s32 ModuleInstall_EmFlashInstallXIP(const char *TargetFs,s32 bstart, s32 bend, u32 doformat);
    ModuleInstall_EmFlashInstallXIP(CFG_EFLASH_XIPFSMOUNT_NAME,CFG_EFLASH_XIP_PART_START,
    CFG_EFLASH_XIP_PART_END, CFG_EFLASH_XIP_PART_FORMAT);
    //end emflash insatall xip

    //cpu onchip uart
    extern ptu32_t ModuleInstall_UART(ptu32_t SerialNo);
    #if CFG_UART1_ENABLE ==1
    ModuleInstall_UART(CN_UART1);
    #endif
    #if CFG_UART2_ENABLE ==1
    ModuleInstall_UART(CN_UART2);
    #endif
    #if CFG_UART3_ENABLE ==1
    ModuleInstall_UART(CN_UART3);
    #endif
    #if CFG_UART4_ENABLE ==1
    ModuleInstall_UART(CN_UART4);
    #endif
    #if CFG_UART5_ENABLE ==1
    ModuleInstall_UART(CN_UART5);
    #endif
    #if CFG_UART6_ENABLE ==1
    ModuleInstall_UART(CN_UART6);
    #endif
    #if CFG_UART7_ENABLE ==1
    ModuleInstall_UART(CN_UART7);
    #endif
    #if CFG_UART8_ENABLE ==1
    ModuleInstall_UART(CN_UART8);
    #endif
    //end cpu onchip uart

    //kernel
    #if(CFG_OS_TINY == flase)
    extern s32 kernel_command(void);
    kernel_command();
    #endif
    //end kernel

    //Nls Charset
    extern ptu32_t ModuleInstall_Charset(ptu32_t para);
    ModuleInstall_Charset(0);
    extern void ModuleInstall_CharsetNls(const char * DefaultCharset);
    ModuleInstall_CharsetNls("C");
    //end Nls Charset

    //Software Timers
    extern bool_t ModuleInstall_Timer(void);
    ModuleInstall_Timer();
    //end Software Timers

    //tcpip
    extern bool_t ModuleInstall_TcpIp(void);
    ModuleInstall_TcpIp( );
    //end tcpip

    //cpu onchip ETH
    extern bool_t ModuleInstall_ETH(void);
    ModuleInstall_ETH( );
    //end cpu onchip ETH

    //norflash W25QXX
    extern s32 ModuleInstall_W25qxx(void);
    ModuleInstall_W25qxx();
    //end norflash W25QXX

    //W25QXX FAT
    extern bool_t ModuleInstall_W25qxxInstallFat(const char *TargetFs, s32 bend, u32 doformat);
    ModuleInstall_W25qxxInstallFat(CFG_W25_FAT_MOUNT_NAME,CFG_W25_FAT_PART_END,CFG_W25_FAT_PART_FORMAT);
    //end W25QXX FAT

    //----------------------------later----------------------------//
    //stdio
    #if(CFG_STDIO_STDIOFILE == true)
    extern s32 ModuleInstall_STDIO(const char *in,const char *out, const char *err);
    ModuleInstall_STDIO(CFG_STDIO_IN_NAME,CFG_STDIO_OUT_NAME,CFG_STDIO_ERR_NAME);
    #endif
    //end stdio

    //network config
    extern void ModuleInstall_InitNet( );
    ModuleInstall_InitNet( );
    //end network config

	evtt_main = DJY_EvttRegist(EN_CORRELATIVE,CN_PRIO_RRS,0,0,
		__djy_main,NULL,CFG_MAINSTACK_LIMIT, "main function");
	//事件的两个参数暂设为0,如果用shell启动,可用来采集shell命令行参数
	DJY_EventPop(evtt_main,NULL,0,0,0,0);

    //----------------------------medium----------------------------//
    //heap
    #if ((CFG_DYNAMIC_MEM == true))
    extern bool_t Heap_DynamicModuleInit(void);
    Heap_DynamicModuleInit ( );
    #endif
    //end heap



	return ;
}

/*Modified at 2023-12-24 19:58:39*/
/****************************************************
 *  Automatically-generated file. Do not edit!	*
 ****************************************************/

#include "project_config.h"
#include "djyos.h"
#include "stdint.h"
#include "stddef.h"
#include "cpu_peri.h"
#include <Iboot_info.h>

#include <djyfs/filesystems.h>

extern ptu32_t djy_main(void);
//如果这个CN_MANUFACTURER_NAME名字要改，那djysrc里的Iboot_info.c中相应的名字也要改
const char CN_MANUFACTURER_NAME[] = PRODUCT_MANUFACTURER_NAME;


const struct ProductInfo Djy_Product_Info __attribute__ ((section(".DjyProductInfo"))) =
{
    .VersionNumber[0] = PRODUCT_VERSION_LARGE,
    .VersionNumber[1] = PRODUCT_VERSION_MEDIUM,
    .VersionNumber[2] = PRODUCT_VERSION_SMALL,
#if(CN_PTR_BITS < 64)
    .ManufacturerNameAddr      = (u32)(&CN_MANUFACTURER_NAME),
    .ManufacturerNamereserved32    = 0xffffffff,
#else
    .ManufacturerNameAddr      = (u64)(&CN_MANUFACTURER_NAME),
#endif
    .ProductClassify = PRODUCT_PRODUCT_CLASSIFY,
    .ProductType = PRODUCT_PRODUCT_MODEL,

    .TypeCode = PRODUCT_PRODUCT_MODEL_CODE,

    .ProductionTime = {'*','*','*','*'},
    .ProductionNumber = {'*','*','*','*','*'},
    .reserved8 = 0,
    .BoardType = PRODUCT_BOARD_TYPE,
    .CPU_Type = PRODUCT_CPU_TYPE,
    .Reserved ={
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff
            },
};


ptu32_t __djy_main(void)
{
    //modbus
    extern bool_t ModuleInstall_Modbus(void);
    ModuleInstall_Modbus();
    //end modbus

    djy_main();

	return 0;
}

void Sys_ModuleInit(void)
{
	uint16_t evtt_main;

    //shell
    extern void Stdio_KnlInOutInit(char * StdioIn, char *StdioOut);
    Stdio_KnlInOutInit(CFG_STDIO_IN_NAME,CFG_STDIO_OUT_NAME);
    extern s32 ModuleInstall_Shell(ptu32_t para);
    ModuleInstall_Shell(0);
    //end shell

    //----------------------------early----------------------------//
    //black box
    extern void ModuleInstall_BlackBox(void);
    ModuleInstall_BlackBox( );
    //end black box

    //device file system
    extern s32 ModuleInstall_dev(void);
    ModuleInstall_dev();    // 安装设备文件系统；
    //end device file system

    //djybus
    extern bool_t ModuleInstall_DjyBus(void);
    ModuleInstall_DjyBus ( );
    //end djybus

    //message queue
    extern bool_t ModuleInstall_MsgQ(void);
    ModuleInstall_MsgQ ( );
    //end message queue

    //multiplex
    extern bool_t ModuleInstall_Multiplex(void);
    ModuleInstall_Multiplex ();
    //end multiplex

    //spi bus
    extern bool_t ModuleInstall_SPIBus(void);
    ModuleInstall_SPIBus();
    //end spi bus

    //cpu onchip spi
    extern bool_t ModuleInstall_SPI(u8 port);
    #if CFG_SPI1_ENABLE==1
    ModuleInstall_SPI(CN_SPI1);
    #endif
    #if CFG_SPI2_ENABLE==1
    ModuleInstall_SPI(CN_SPI2);
    #endif
    #if CFG_SPI3_ENABLE==1
    ModuleInstall_SPI(CN_SPI3);
    #endif
    #if CFG_SPI4_ENABLE==1
    ModuleInstall_SPI(CN_SPI4);
    #endif
    //end cpu onchip spi

    //xip iboot file system
    extern s32 ModuleInstall_XIP_IBOOT_FS(u32 opt, void *data);
    ModuleInstall_XIP_IBOOT_FS(0,NULL);
    //end xip iboot file system

    //cpu drive inner flash
    s32 ModuleInstall_EmbededFlash(u32 doformat);
    ModuleInstall_EmbededFlash(CFG_EFLASH_PART_FORMAT);
    //end cpu drive inner flash

    //emflash insatall xip
    extern s32 ModuleInstall_EmFlashInstallXIP(const char *TargetFs,s32 bstart, s32 bend, u32 doformat);
    ModuleInstall_EmFlashInstallXIP(CFG_EFLASH_XIPFSMOUNT_NAME,CFG_EFLASH_XIP_PART_START,
    CFG_EFLASH_XIP_PART_END, CFG_EFLASH_XIP_PART_FORMAT);
    //end emflash insatall xip

    //kernel
    #if(CFG_OS_TINY == flase)
    extern s32 kernel_command(void);
    kernel_command();
    #endif
    //end kernel

    //Nls Charset
    extern ptu32_t ModuleInstall_Charset(ptu32_t para);
    ModuleInstall_Charset(0);
    extern void ModuleInstall_CharsetNls(const char * DefaultCharset);
    ModuleInstall_CharsetNls("C");
    //end Nls Charset

    //fat file system
    extern s32 ModuleInstall_FAT(const char *dir, u32 opt, void *data);
    ModuleInstall_FAT(CFG_FAT_MOUNT_POINT, CFG_FAT_MS_INSTALLUSE, CFG_FAT_MEDIA_KIND);
    //end fat file system

    //Software Timers
    extern bool_t ModuleInstall_Timer(void);
    ModuleInstall_Timer();
    //end Software Timers

    //cpu onchip timer
    extern bool_t ModuleInstall_HardTimer(void);
    ModuleInstall_HardTimer();
    //end cpu onchip timer

    //tcpip
    extern bool_t ModuleInstall_TcpIp(void);
    ModuleInstall_TcpIp( );
    //end tcpip

    //cpu onchip ETH
    extern bool_t ModuleInstall_ETH(void);
    ModuleInstall_ETH( );
    //end cpu onchip ETH

    //cpu onchip uart
    extern ptu32_t ModuleInstall_UART(ptu32_t SerialNo);
    #if CFG_UART1_ENABLE ==1
    ModuleInstall_UART(CN_UART1);
    #endif
    #if CFG_UART2_ENABLE ==1
    ModuleInstall_UART(CN_UART2);
    #endif
    #if CFG_UART3_ENABLE ==1
    ModuleInstall_UART(CN_UART3);
    #endif
    #if CFG_UART4_ENABLE ==1
    ModuleInstall_UART(CN_UART4);
    #endif
    #if CFG_UART5_ENABLE ==1
    ModuleInstall_UART(CN_UART5);
    #endif
    #if CFG_UART6_ENABLE ==1
    ModuleInstall_UART(CN_UART6);
    #endif
    #if CFG_UART7_ENABLE ==1
    ModuleInstall_UART(CN_UART7);
    #endif
    #if CFG_UART8_ENABLE ==1
    ModuleInstall_UART(CN_UART8);
    #endif
    //end cpu onchip uart

    //norflash W25QXX
    extern s32 ModuleInstall_W25qxx(void);
    ModuleInstall_W25qxx();
    //end norflash W25QXX

    //W25QXX FAT
    extern bool_t ModuleInstall_W25qxxInstallFat(const char *TargetFs, s32 bend, u32 doformat);
    ModuleInstall_W25qxxInstallFat(CFG_W25_FAT_MOUNT_NAME,CFG_W25_FAT_PART_END,CFG_W25_FAT_PART_FORMAT);
    //end W25QXX FAT

    //----------------------------later----------------------------//
    //stdio
    #if(CFG_STDIO_STDIOFILE == true)
    extern s32 ModuleInstall_STDIO(const char *in,const char *out, const char *err);
    ModuleInstall_STDIO(CFG_STDIO_IN_NAME,CFG_STDIO_OUT_NAME,CFG_STDIO_ERR_NAME);
    #endif
    //end stdio

    //network config
    extern void ModuleInstall_InitNet( );
    ModuleInstall_InitNet( );
    //end network config

	evtt_main = DJY_EvttRegist(EN_CORRELATIVE,CN_PRIO_RRS,0,0,
		__djy_main,NULL,CFG_MAINSTACK_LIMIT, "main function");
	//事件的两个参数暂设为0,如果用shell启动,可用来采集shell命令行参数
	DJY_EventPop(evtt_main,NULL,0,0,0,0);

    //----------------------------medium----------------------------//
    //heap
    #if ((CFG_DYNAMIC_MEM == true))
    extern bool_t Heap_DynamicModuleInit(void);
    Heap_DynamicModuleInit ( );
    #endif
    //end heap



	return ;
}

/*Modified at 2023-12-24 19:58:44*/
/****************************************************
 *  Automatically-generated file. Do not edit!	*
 ****************************************************/

#include "project_config.h"
#include "djyos.h"
#include "stdint.h"
#include "stddef.h"
#include "cpu_peri.h"
#include <Iboot_info.h>

#include <djyfs/filesystems.h>

extern ptu32_t djy_main(void);
//如果这个CN_MANUFACTURER_NAME名字要改，那djysrc里的Iboot_info.c中相应的名字也要改
const char CN_MANUFACTURER_NAME[] = PRODUCT_MANUFACTURER_NAME;


const struct ProductInfo Djy_Product_Info __attribute__ ((section(".DjyProductInfo"))) =
{
    .VersionNumber[0] = PRODUCT_VERSION_LARGE,
    .VersionNumber[1] = PRODUCT_VERSION_MEDIUM,
    .VersionNumber[2] = PRODUCT_VERSION_SMALL,
#if(CN_PTR_BITS < 64)
    .ManufacturerNameAddr      = (u32)(&CN_MANUFACTURER_NAME),
    .ManufacturerNamereserved32    = 0xffffffff,
#else
    .ManufacturerNameAddr      = (u64)(&CN_MANUFACTURER_NAME),
#endif
    .ProductClassify = PRODUCT_PRODUCT_CLASSIFY,
    .ProductType = PRODUCT_PRODUCT_MODEL,

    .TypeCode = PRODUCT_PRODUCT_MODEL_CODE,

    .ProductionTime = {'*','*','*','*'},
    .ProductionNumber = {'*','*','*','*','*'},
    .reserved8 = 0,
    .BoardType = PRODUCT_BOARD_TYPE,
    .CPU_Type = PRODUCT_CPU_TYPE,
    .Reserved ={
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff
            },
};


ptu32_t __djy_main(void)
{
    //modbus
    extern bool_t ModuleInstall_Modbus(void);
    ModuleInstall_Modbus();
    //end modbus

    djy_main();

	return 0;
}

void Sys_ModuleInit(void)
{
	uint16_t evtt_main;

    //shell
    extern void Stdio_KnlInOutInit(char * StdioIn, char *StdioOut);
    Stdio_KnlInOutInit(CFG_STDIO_IN_NAME,CFG_STDIO_OUT_NAME);
    extern s32 ModuleInstall_Shell(ptu32_t para);
    ModuleInstall_Shell(0);
    //end shell

    //----------------------------early----------------------------//
    //black box
    extern void ModuleInstall_BlackBox(void);
    ModuleInstall_BlackBox( );
    //end black box

    //device file system
    extern s32 ModuleInstall_dev(void);
    ModuleInstall_dev();    // 安装设备文件系统；
    //end device file system

    //djybus
    extern bool_t ModuleInstall_DjyBus(void);
    ModuleInstall_DjyBus ( );
    //end djybus

    //message queue
    extern bool_t ModuleInstall_MsgQ(void);
    ModuleInstall_MsgQ ( );
    //end message queue

    //multiplex
    extern bool_t ModuleInstall_Multiplex(void);
    ModuleInstall_Multiplex ();
    //end multiplex

    //spi bus
    extern bool_t ModuleInstall_SPIBus(void);
    ModuleInstall_SPIBus();
    //end spi bus

    //xip iboot file system
    extern s32 ModuleInstall_XIP_IBOOT_FS(u32 opt, void *data);
    ModuleInstall_XIP_IBOOT_FS(0,NULL);
    //end xip iboot file system

    //cpu onchip spi
    extern bool_t ModuleInstall_SPI(u8 port);
    #if CFG_SPI1_ENABLE==1
    ModuleInstall_SPI(CN_SPI1);
    #endif
    #if CFG_SPI2_ENABLE==1
    ModuleInstall_SPI(CN_SPI2);
    #endif
    #if CFG_SPI3_ENABLE==1
    ModuleInstall_SPI(CN_SPI3);
    #endif
    #if CFG_SPI4_ENABLE==1
    ModuleInstall_SPI(CN_SPI4);
    #endif
    //end cpu onchip spi

    //fat file system
    extern s32 ModuleInstall_FAT(const char *dir, u32 opt, void *data);
    ModuleInstall_FAT(CFG_FAT_MOUNT_POINT, CFG_FAT_MS_INSTALLUSE, CFG_FAT_MEDIA_KIND);
    //end fat file system

    //cpu onchip timer
    extern bool_t ModuleInstall_HardTimer(void);
    ModuleInstall_HardTimer();
    //end cpu onchip timer

    //cpu drive inner flash
    s32 ModuleInstall_EmbededFlash(u32 doformat);
    ModuleInstall_EmbededFlash(CFG_EFLASH_PART_FORMAT);
    //end cpu drive inner flash

    //emflash insatall xip
    extern s32 ModuleInstall_EmFlashInstallXIP(const char *TargetFs,s32 bstart, s32 bend, u32 doformat);
    ModuleInstall_EmFlashInstallXIP(CFG_EFLASH_XIPFSMOUNT_NAME,CFG_EFLASH_XIP_PART_START,
    CFG_EFLASH_XIP_PART_END, CFG_EFLASH_XIP_PART_FORMAT);
    //end emflash insatall xip

    //cpu onchip uart
    extern ptu32_t ModuleInstall_UART(ptu32_t SerialNo);
    #if CFG_UART1_ENABLE ==1
    ModuleInstall_UART(CN_UART1);
    #endif
    #if CFG_UART2_ENABLE ==1
    ModuleInstall_UART(CN_UART2);
    #endif
    #if CFG_UART3_ENABLE ==1
    ModuleInstall_UART(CN_UART3);
    #endif
    #if CFG_UART4_ENABLE ==1
    ModuleInstall_UART(CN_UART4);
    #endif
    #if CFG_UART5_ENABLE ==1
    ModuleInstall_UART(CN_UART5);
    #endif
    #if CFG_UART6_ENABLE ==1
    ModuleInstall_UART(CN_UART6);
    #endif
    #if CFG_UART7_ENABLE ==1
    ModuleInstall_UART(CN_UART7);
    #endif
    #if CFG_UART8_ENABLE ==1
    ModuleInstall_UART(CN_UART8);
    #endif
    //end cpu onchip uart

    //kernel
    #if(CFG_OS_TINY == flase)
    extern s32 kernel_command(void);
    kernel_command();
    #endif
    //end kernel

    //Nls Charset
    extern ptu32_t ModuleInstall_Charset(ptu32_t para);
    ModuleInstall_Charset(0);
    extern void ModuleInstall_CharsetNls(const char * DefaultCharset);
    ModuleInstall_CharsetNls("C");
    //end Nls Charset

    //Software Timers
    extern bool_t ModuleInstall_Timer(void);
    ModuleInstall_Timer();
    //end Software Timers

    //tcpip
    extern bool_t ModuleInstall_TcpIp(void);
    ModuleInstall_TcpIp( );
    //end tcpip

    //cpu onchip ETH
    extern bool_t ModuleInstall_ETH(void);
    ModuleInstall_ETH( );
    //end cpu onchip ETH

    //norflash W25QXX
    extern s32 ModuleInstall_W25qxx(void);
    ModuleInstall_W25qxx();
    //end norflash W25QXX

    //W25QXX FAT
    extern bool_t ModuleInstall_W25qxxInstallFat(const char *TargetFs, s32 bend, u32 doformat);
    ModuleInstall_W25qxxInstallFat(CFG_W25_FAT_MOUNT_NAME,CFG_W25_FAT_PART_END,CFG_W25_FAT_PART_FORMAT);
    //end W25QXX FAT

    //----------------------------later----------------------------//
    //stdio
    #if(CFG_STDIO_STDIOFILE == true)
    extern s32 ModuleInstall_STDIO(const char *in,const char *out, const char *err);
    ModuleInstall_STDIO(CFG_STDIO_IN_NAME,CFG_STDIO_OUT_NAME,CFG_STDIO_ERR_NAME);
    #endif
    //end stdio

    //network config
    extern void ModuleInstall_InitNet( );
    ModuleInstall_InitNet( );
    //end network config

	evtt_main = DJY_EvttRegist(EN_CORRELATIVE,CN_PRIO_RRS,0,0,
		__djy_main,NULL,CFG_MAINSTACK_LIMIT, "main function");
	//事件的两个参数暂设为0,如果用shell启动,可用来采集shell命令行参数
	DJY_EventPop(evtt_main,NULL,0,0,0,0);

    //----------------------------medium----------------------------//
    //heap
    #if ((CFG_DYNAMIC_MEM == true))
    extern bool_t Heap_DynamicModuleInit(void);
    Heap_DynamicModuleInit ( );
    #endif
    //end heap



	return ;
}

/*Modified at 2023-12-28 19:50:08*/
/****************************************************
 *  Automatically-generated file. Do not edit!	*
 ****************************************************/

#include "project_config.h"
#include "djyos.h"
#include "stdint.h"
#include "stddef.h"
#include "cpu_peri.h"
#include <Iboot_info.h>

#include <djyfs/filesystems.h>

extern ptu32_t djy_main(void);
//如果这个CN_MANUFACTURER_NAME名字要改，那djysrc里的Iboot_info.c中相应的名字也要改
const char CN_MANUFACTURER_NAME[] = PRODUCT_MANUFACTURER_NAME;


const struct ProductInfo Djy_Product_Info __attribute__ ((section(".DjyProductInfo"))) =
{
    .VersionNumber[0] = PRODUCT_VERSION_LARGE,
    .VersionNumber[1] = PRODUCT_VERSION_MEDIUM,
    .VersionNumber[2] = PRODUCT_VERSION_SMALL,
#if(CN_PTR_BITS < 64)
    .ManufacturerNameAddr      = (u32)(&CN_MANUFACTURER_NAME),
    .ManufacturerNamereserved32    = 0xffffffff,
#else
    .ManufacturerNameAddr      = (u64)(&CN_MANUFACTURER_NAME),
#endif
    .ProductClassify = PRODUCT_PRODUCT_CLASSIFY,
    .ProductType = PRODUCT_PRODUCT_MODEL,

    .TypeCode = PRODUCT_PRODUCT_MODEL_CODE,

    .ProductionTime = {'*','*','*','*'},
    .ProductionNumber = {'*','*','*','*','*'},
    .reserved8 = 0,
    .BoardType = PRODUCT_BOARD_TYPE,
    .CPU_Type = PRODUCT_CPU_TYPE,
    .Reserved ={
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff
            },
};


ptu32_t __djy_main(void)
{
    //modbus
    extern bool_t ModuleInstall_Modbus(void);
    ModuleInstall_Modbus();
    //end modbus

    djy_main();

	return 0;
}

void Sys_ModuleInit(void)
{
	uint16_t evtt_main;

    //shell
    extern void Stdio_KnlInOutInit(char * StdioIn, char *StdioOut);
    Stdio_KnlInOutInit(CFG_STDIO_IN_NAME,CFG_STDIO_OUT_NAME);
    extern s32 ModuleInstall_Shell(ptu32_t para);
    ModuleInstall_Shell(0);
    //end shell

    //----------------------------early----------------------------//
    //black box
    extern void ModuleInstall_BlackBox(void);
    ModuleInstall_BlackBox( );
    //end black box

    //device file system
    extern s32 ModuleInstall_dev(void);
    ModuleInstall_dev();    // 安装设备文件系统；
    //end device file system

    //djybus
    extern bool_t ModuleInstall_DjyBus(void);
    ModuleInstall_DjyBus ( );
    //end djybus

    //message queue
    extern bool_t ModuleInstall_MsgQ(void);
    ModuleInstall_MsgQ ( );
    //end message queue

    //multiplex
    extern bool_t ModuleInstall_Multiplex(void);
    ModuleInstall_Multiplex ();
    //end multiplex

    //spi bus
    extern bool_t ModuleInstall_SPIBus(void);
    ModuleInstall_SPIBus();
    //end spi bus

    //cpu onchip spi
    extern bool_t ModuleInstall_SPI(u8 port);
    #if CFG_SPI1_ENABLE==1
    ModuleInstall_SPI(CN_SPI1);
    #endif
    #if CFG_SPI2_ENABLE==1
    ModuleInstall_SPI(CN_SPI2);
    #endif
    #if CFG_SPI3_ENABLE==1
    ModuleInstall_SPI(CN_SPI3);
    #endif
    #if CFG_SPI4_ENABLE==1
    ModuleInstall_SPI(CN_SPI4);
    #endif
    //end cpu onchip spi

    //xip iboot file system
    extern s32 ModuleInstall_XIP_IBOOT_FS(u32 opt, void *data);
    ModuleInstall_XIP_IBOOT_FS(0,NULL);
    //end xip iboot file system

    //cpu drive inner flash
    s32 ModuleInstall_EmbededFlash(u32 doformat);
    ModuleInstall_EmbededFlash(CFG_EFLASH_PART_FORMAT);
    //end cpu drive inner flash

    //emflash insatall xip
    extern s32 ModuleInstall_EmFlashInstallXIP(const char *TargetFs,s32 bstart, s32 bend, u32 doformat);
    ModuleInstall_EmFlashInstallXIP(CFG_EFLASH_XIPFSMOUNT_NAME,CFG_EFLASH_XIP_PART_START,
    CFG_EFLASH_XIP_PART_END, CFG_EFLASH_XIP_PART_FORMAT);
    //end emflash insatall xip

    //kernel
    #if(CFG_OS_TINY == flase)
    extern s32 kernel_command(void);
    kernel_command();
    #endif
    //end kernel

    //Nls Charset
    extern ptu32_t ModuleInstall_Charset(ptu32_t para);
    ModuleInstall_Charset(0);
    extern void ModuleInstall_CharsetNls(const char * DefaultCharset);
    ModuleInstall_CharsetNls("C");
    //end Nls Charset

    //fat file system
    extern s32 ModuleInstall_FAT(const char *dir, u32 opt, void *data);
    ModuleInstall_FAT(CFG_FAT_MOUNT_POINT, CFG_FAT_MS_INSTALLUSE, CFG_FAT_MEDIA_KIND);
    //end fat file system

    //Software Timers
    extern bool_t ModuleInstall_Timer(void);
    ModuleInstall_Timer();
    //end Software Timers

    //cpu onchip timer
    extern bool_t ModuleInstall_HardTimer(void);
    ModuleInstall_HardTimer();
    //end cpu onchip timer

    //tcpip
    extern bool_t ModuleInstall_TcpIp(void);
    ModuleInstall_TcpIp( );
    //end tcpip

    //cpu onchip ETH
    extern bool_t ModuleInstall_ETH(void);
    ModuleInstall_ETH( );
    //end cpu onchip ETH

    //cpu onchip uart
    extern ptu32_t ModuleInstall_UART(ptu32_t SerialNo);
    #if CFG_UART1_ENABLE ==1
    ModuleInstall_UART(CN_UART1);
    #endif
    #if CFG_UART2_ENABLE ==1
    ModuleInstall_UART(CN_UART2);
    #endif
    #if CFG_UART3_ENABLE ==1
    ModuleInstall_UART(CN_UART3);
    #endif
    #if CFG_UART4_ENABLE ==1
    ModuleInstall_UART(CN_UART4);
    #endif
    #if CFG_UART5_ENABLE ==1
    ModuleInstall_UART(CN_UART5);
    #endif
    #if CFG_UART6_ENABLE ==1
    ModuleInstall_UART(CN_UART6);
    #endif
    #if CFG_UART7_ENABLE ==1
    ModuleInstall_UART(CN_UART7);
    #endif
    #if CFG_UART8_ENABLE ==1
    ModuleInstall_UART(CN_UART8);
    #endif
    //end cpu onchip uart

    //norflash W25QXX
    extern s32 ModuleInstall_W25qxx(void);
    ModuleInstall_W25qxx();
    //end norflash W25QXX

    //W25QXX FAT
    extern bool_t ModuleInstall_W25qxxInstallFat(const char *TargetFs, s32 bend, u32 doformat);
    ModuleInstall_W25qxxInstallFat(CFG_W25_FAT_MOUNT_NAME,CFG_W25_FAT_PART_END,CFG_W25_FAT_PART_FORMAT);
    //end W25QXX FAT

    //----------------------------later----------------------------//
    //stdio
    #if(CFG_STDIO_STDIOFILE == true)
    extern s32 ModuleInstall_STDIO(const char *in,const char *out, const char *err);
    ModuleInstall_STDIO(CFG_STDIO_IN_NAME,CFG_STDIO_OUT_NAME,CFG_STDIO_ERR_NAME);
    #endif
    //end stdio

    //network config
    extern void ModuleInstall_InitNet( );
    ModuleInstall_InitNet( );
    //end network config

	evtt_main = DJY_EvttRegist(EN_CORRELATIVE,CN_PRIO_RRS,0,0,
		__djy_main,NULL,CFG_MAINSTACK_LIMIT, "main function");
	//事件的两个参数暂设为0,如果用shell启动,可用来采集shell命令行参数
	DJY_EventPop(evtt_main,NULL,0,0,0,0);

    //----------------------------medium----------------------------//
    //heap
    #if ((CFG_DYNAMIC_MEM == true))
    extern bool_t Heap_DynamicModuleInit(void);
    Heap_DynamicModuleInit ( );
    #endif
    //end heap



	return ;
}

/*Modified at 2023-12-28 19:50:14*/
/****************************************************
 *  Automatically-generated file. Do not edit!	*
 ****************************************************/

#include "project_config.h"
#include "djyos.h"
#include "stdint.h"
#include "stddef.h"
#include "cpu_peri.h"
#include <Iboot_info.h>

#include <djyfs/filesystems.h>

extern ptu32_t djy_main(void);
//如果这个CN_MANUFACTURER_NAME名字要改，那djysrc里的Iboot_info.c中相应的名字也要改
const char CN_MANUFACTURER_NAME[] = PRODUCT_MANUFACTURER_NAME;


const struct ProductInfo Djy_Product_Info __attribute__ ((section(".DjyProductInfo"))) =
{
    .VersionNumber[0] = PRODUCT_VERSION_LARGE,
    .VersionNumber[1] = PRODUCT_VERSION_MEDIUM,
    .VersionNumber[2] = PRODUCT_VERSION_SMALL,
#if(CN_PTR_BITS < 64)
    .ManufacturerNameAddr      = (u32)(&CN_MANUFACTURER_NAME),
    .ManufacturerNamereserved32    = 0xffffffff,
#else
    .ManufacturerNameAddr      = (u64)(&CN_MANUFACTURER_NAME),
#endif
    .ProductClassify = PRODUCT_PRODUCT_CLASSIFY,
    .ProductType = PRODUCT_PRODUCT_MODEL,

    .TypeCode = PRODUCT_PRODUCT_MODEL_CODE,

    .ProductionTime = {'*','*','*','*'},
    .ProductionNumber = {'*','*','*','*','*'},
    .reserved8 = 0,
    .BoardType = PRODUCT_BOARD_TYPE,
    .CPU_Type = PRODUCT_CPU_TYPE,
    .Reserved ={
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff
            },
};


ptu32_t __djy_main(void)
{
    //modbus
    extern bool_t ModuleInstall_Modbus(void);
    ModuleInstall_Modbus();
    //end modbus

    djy_main();

	return 0;
}

void Sys_ModuleInit(void)
{
	uint16_t evtt_main;

    //shell
    extern void Stdio_KnlInOutInit(char * StdioIn, char *StdioOut);
    Stdio_KnlInOutInit(CFG_STDIO_IN_NAME,CFG_STDIO_OUT_NAME);
    extern s32 ModuleInstall_Shell(ptu32_t para);
    ModuleInstall_Shell(0);
    //end shell

    //----------------------------early----------------------------//
    //black box
    extern void ModuleInstall_BlackBox(void);
    ModuleInstall_BlackBox( );
    //end black box

    //device file system
    extern s32 ModuleInstall_dev(void);
    ModuleInstall_dev();    // 安装设备文件系统；
    //end device file system

    //djybus
    extern bool_t ModuleInstall_DjyBus(void);
    ModuleInstall_DjyBus ( );
    //end djybus

    //message queue
    extern bool_t ModuleInstall_MsgQ(void);
    ModuleInstall_MsgQ ( );
    //end message queue

    //multiplex
    extern bool_t ModuleInstall_Multiplex(void);
    ModuleInstall_Multiplex ();
    //end multiplex

    //spi bus
    extern bool_t ModuleInstall_SPIBus(void);
    ModuleInstall_SPIBus();
    //end spi bus

    //xip iboot file system
    extern s32 ModuleInstall_XIP_IBOOT_FS(u32 opt, void *data);
    ModuleInstall_XIP_IBOOT_FS(0,NULL);
    //end xip iboot file system

    //cpu onchip spi
    extern bool_t ModuleInstall_SPI(u8 port);
    #if CFG_SPI1_ENABLE==1
    ModuleInstall_SPI(CN_SPI1);
    #endif
    #if CFG_SPI2_ENABLE==1
    ModuleInstall_SPI(CN_SPI2);
    #endif
    #if CFG_SPI3_ENABLE==1
    ModuleInstall_SPI(CN_SPI3);
    #endif
    #if CFG_SPI4_ENABLE==1
    ModuleInstall_SPI(CN_SPI4);
    #endif
    //end cpu onchip spi

    //cpu onchip uart
    extern ptu32_t ModuleInstall_UART(ptu32_t SerialNo);
    #if CFG_UART1_ENABLE ==1
    ModuleInstall_UART(CN_UART1);
    #endif
    #if CFG_UART2_ENABLE ==1
    ModuleInstall_UART(CN_UART2);
    #endif
    #if CFG_UART3_ENABLE ==1
    ModuleInstall_UART(CN_UART3);
    #endif
    #if CFG_UART4_ENABLE ==1
    ModuleInstall_UART(CN_UART4);
    #endif
    #if CFG_UART5_ENABLE ==1
    ModuleInstall_UART(CN_UART5);
    #endif
    #if CFG_UART6_ENABLE ==1
    ModuleInstall_UART(CN_UART6);
    #endif
    #if CFG_UART7_ENABLE ==1
    ModuleInstall_UART(CN_UART7);
    #endif
    #if CFG_UART8_ENABLE ==1
    ModuleInstall_UART(CN_UART8);
    #endif
    //end cpu onchip uart

    //fat file system
    extern s32 ModuleInstall_FAT(const char *dir, u32 opt, void *data);
    ModuleInstall_FAT(CFG_FAT_MOUNT_POINT, CFG_FAT_MS_INSTALLUSE, CFG_FAT_MEDIA_KIND);
    //end fat file system

    //cpu onchip timer
    extern bool_t ModuleInstall_HardTimer(void);
    ModuleInstall_HardTimer();
    //end cpu onchip timer

    //cpu drive inner flash
    s32 ModuleInstall_EmbededFlash(u32 doformat);
    ModuleInstall_EmbededFlash(CFG_EFLASH_PART_FORMAT);
    //end cpu drive inner flash

    //emflash insatall xip
    extern s32 ModuleInstall_EmFlashInstallXIP(const char *TargetFs,s32 bstart, s32 bend, u32 doformat);
    ModuleInstall_EmFlashInstallXIP(CFG_EFLASH_XIPFSMOUNT_NAME,CFG_EFLASH_XIP_PART_START,
    CFG_EFLASH_XIP_PART_END, CFG_EFLASH_XIP_PART_FORMAT);
    //end emflash insatall xip

    //kernel
    #if(CFG_OS_TINY == flase)
    extern s32 kernel_command(void);
    kernel_command();
    #endif
    //end kernel

    //Nls Charset
    extern ptu32_t ModuleInstall_Charset(ptu32_t para);
    ModuleInstall_Charset(0);
    extern void ModuleInstall_CharsetNls(const char * DefaultCharset);
    ModuleInstall_CharsetNls("C");
    //end Nls Charset

    //Software Timers
    extern bool_t ModuleInstall_Timer(void);
    ModuleInstall_Timer();
    //end Software Timers

    //tcpip
    extern bool_t ModuleInstall_TcpIp(void);
    ModuleInstall_TcpIp( );
    //end tcpip

    //cpu onchip ETH
    extern bool_t ModuleInstall_ETH(void);
    ModuleInstall_ETH( );
    //end cpu onchip ETH

    //norflash W25QXX
    extern s32 ModuleInstall_W25qxx(void);
    ModuleInstall_W25qxx();
    //end norflash W25QXX

    //W25QXX FAT
    extern bool_t ModuleInstall_W25qxxInstallFat(const char *TargetFs, s32 bend, u32 doformat);
    ModuleInstall_W25qxxInstallFat(CFG_W25_FAT_MOUNT_NAME,CFG_W25_FAT_PART_END,CFG_W25_FAT_PART_FORMAT);
    //end W25QXX FAT

    //----------------------------later----------------------------//
    //stdio
    #if(CFG_STDIO_STDIOFILE == true)
    extern s32 ModuleInstall_STDIO(const char *in,const char *out, const char *err);
    ModuleInstall_STDIO(CFG_STDIO_IN_NAME,CFG_STDIO_OUT_NAME,CFG_STDIO_ERR_NAME);
    #endif
    //end stdio

    //network config
    extern void ModuleInstall_InitNet( );
    ModuleInstall_InitNet( );
    //end network config

	evtt_main = DJY_EvttRegist(EN_CORRELATIVE,CN_PRIO_RRS,0,0,
		__djy_main,NULL,CFG_MAINSTACK_LIMIT, "main function");
	//事件的两个参数暂设为0,如果用shell启动,可用来采集shell命令行参数
	DJY_EventPop(evtt_main,NULL,0,0,0,0);

    //----------------------------medium----------------------------//
    //heap
    #if ((CFG_DYNAMIC_MEM == true))
    extern bool_t Heap_DynamicModuleInit(void);
    Heap_DynamicModuleInit ( );
    #endif
    //end heap



	return ;
}

/*Modified at 2023-12-28 19:50:39*/
/****************************************************
 *  Automatically-generated file. Do not edit!	*
 ****************************************************/

#include "project_config.h"
#include "djyos.h"
#include "stdint.h"
#include "stddef.h"
#include "cpu_peri.h"
#include <Iboot_info.h>

#include <djyfs/filesystems.h>

extern ptu32_t djy_main(void);
//如果这个CN_MANUFACTURER_NAME名字要改，那djysrc里的Iboot_info.c中相应的名字也要改
const char CN_MANUFACTURER_NAME[] = PRODUCT_MANUFACTURER_NAME;


const struct ProductInfo Djy_Product_Info __attribute__ ((section(".DjyProductInfo"))) =
{
    .VersionNumber[0] = PRODUCT_VERSION_LARGE,
    .VersionNumber[1] = PRODUCT_VERSION_MEDIUM,
    .VersionNumber[2] = PRODUCT_VERSION_SMALL,
#if(CN_PTR_BITS < 64)
    .ManufacturerNameAddr      = (u32)(&CN_MANUFACTURER_NAME),
    .ManufacturerNamereserved32    = 0xffffffff,
#else
    .ManufacturerNameAddr      = (u64)(&CN_MANUFACTURER_NAME),
#endif
    .ProductClassify = PRODUCT_PRODUCT_CLASSIFY,
    .ProductType = PRODUCT_PRODUCT_MODEL,

    .TypeCode = PRODUCT_PRODUCT_MODEL_CODE,

    .ProductionTime = {'*','*','*','*'},
    .ProductionNumber = {'*','*','*','*','*'},
    .reserved8 = 0,
    .BoardType = PRODUCT_BOARD_TYPE,
    .CPU_Type = PRODUCT_CPU_TYPE,
    .Reserved ={
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff
            },
};


ptu32_t __djy_main(void)
{
    //modbus
    extern bool_t ModuleInstall_Modbus(void);
    ModuleInstall_Modbus();
    //end modbus

    djy_main();

	return 0;
}

void Sys_ModuleInit(void)
{
	uint16_t evtt_main;

    //shell
    extern void Stdio_KnlInOutInit(char * StdioIn, char *StdioOut);
    Stdio_KnlInOutInit(CFG_STDIO_IN_NAME,CFG_STDIO_OUT_NAME);
    extern s32 ModuleInstall_Shell(ptu32_t para);
    ModuleInstall_Shell(0);
    //end shell

    //----------------------------early----------------------------//
    //black box
    extern void ModuleInstall_BlackBox(void);
    ModuleInstall_BlackBox( );
    //end black box

    //device file system
    extern s32 ModuleInstall_dev(void);
    ModuleInstall_dev();    // 安装设备文件系统；
    //end device file system

    //djybus
    extern bool_t ModuleInstall_DjyBus(void);
    ModuleInstall_DjyBus ( );
    //end djybus

    //message queue
    extern bool_t ModuleInstall_MsgQ(void);
    ModuleInstall_MsgQ ( );
    //end message queue

    //multiplex
    extern bool_t ModuleInstall_Multiplex(void);
    ModuleInstall_Multiplex ();
    //end multiplex

    //spi bus
    extern bool_t ModuleInstall_SPIBus(void);
    ModuleInstall_SPIBus();
    //end spi bus

    //cpu onchip spi
    extern bool_t ModuleInstall_SPI(u8 port);
    #if CFG_SPI1_ENABLE==1
    ModuleInstall_SPI(CN_SPI1);
    #endif
    #if CFG_SPI2_ENABLE==1
    ModuleInstall_SPI(CN_SPI2);
    #endif
    #if CFG_SPI3_ENABLE==1
    ModuleInstall_SPI(CN_SPI3);
    #endif
    #if CFG_SPI4_ENABLE==1
    ModuleInstall_SPI(CN_SPI4);
    #endif
    //end cpu onchip spi

    //xip iboot file system
    extern s32 ModuleInstall_XIP_IBOOT_FS(u32 opt, void *data);
    ModuleInstall_XIP_IBOOT_FS(0,NULL);
    //end xip iboot file system

    //cpu drive inner flash
    s32 ModuleInstall_EmbededFlash(u32 doformat);
    ModuleInstall_EmbededFlash(CFG_EFLASH_PART_FORMAT);
    //end cpu drive inner flash

    //emflash insatall xip
    extern s32 ModuleInstall_EmFlashInstallXIP(const char *TargetFs,s32 bstart, s32 bend, u32 doformat);
    ModuleInstall_EmFlashInstallXIP(CFG_EFLASH_XIPFSMOUNT_NAME,CFG_EFLASH_XIP_PART_START,
    CFG_EFLASH_XIP_PART_END, CFG_EFLASH_XIP_PART_FORMAT);
    //end emflash insatall xip

    //kernel
    #if(CFG_OS_TINY == flase)
    extern s32 kernel_command(void);
    kernel_command();
    #endif
    //end kernel

    //Nls Charset
    extern ptu32_t ModuleInstall_Charset(ptu32_t para);
    ModuleInstall_Charset(0);
    extern void ModuleInstall_CharsetNls(const char * DefaultCharset);
    ModuleInstall_CharsetNls("C");
    //end Nls Charset

    //fat file system
    extern s32 ModuleInstall_FAT(const char *dir, u32 opt, void *data);
    ModuleInstall_FAT(CFG_FAT_MOUNT_POINT, CFG_FAT_MS_INSTALLUSE, CFG_FAT_MEDIA_KIND);
    //end fat file system

    //Software Timers
    extern bool_t ModuleInstall_Timer(void);
    ModuleInstall_Timer();
    //end Software Timers

    //cpu onchip timer
    extern bool_t ModuleInstall_HardTimer(void);
    ModuleInstall_HardTimer();
    //end cpu onchip timer

    //tcpip
    extern bool_t ModuleInstall_TcpIp(void);
    ModuleInstall_TcpIp( );
    //end tcpip

    //cpu onchip ETH
    extern bool_t ModuleInstall_ETH(void);
    ModuleInstall_ETH( );
    //end cpu onchip ETH

    //cpu onchip uart
    extern ptu32_t ModuleInstall_UART(ptu32_t SerialNo);
    #if CFG_UART1_ENABLE ==1
    ModuleInstall_UART(CN_UART1);
    #endif
    #if CFG_UART2_ENABLE ==1
    ModuleInstall_UART(CN_UART2);
    #endif
    #if CFG_UART3_ENABLE ==1
    ModuleInstall_UART(CN_UART3);
    #endif
    #if CFG_UART4_ENABLE ==1
    ModuleInstall_UART(CN_UART4);
    #endif
    #if CFG_UART5_ENABLE ==1
    ModuleInstall_UART(CN_UART5);
    #endif
    #if CFG_UART6_ENABLE ==1
    ModuleInstall_UART(CN_UART6);
    #endif
    #if CFG_UART7_ENABLE ==1
    ModuleInstall_UART(CN_UART7);
    #endif
    #if CFG_UART8_ENABLE ==1
    ModuleInstall_UART(CN_UART8);
    #endif
    //end cpu onchip uart

    //norflash W25QXX
    extern s32 ModuleInstall_W25qxx(void);
    ModuleInstall_W25qxx();
    //end norflash W25QXX

    //W25QXX FAT
    extern bool_t ModuleInstall_W25qxxInstallFat(const char *TargetFs, s32 bend, u32 doformat);
    ModuleInstall_W25qxxInstallFat(CFG_W25_FAT_MOUNT_NAME,CFG_W25_FAT_PART_END,CFG_W25_FAT_PART_FORMAT);
    //end W25QXX FAT

    //----------------------------later----------------------------//
    //stdio
    #if(CFG_STDIO_STDIOFILE == true)
    extern s32 ModuleInstall_STDIO(const char *in,const char *out, const char *err);
    ModuleInstall_STDIO(CFG_STDIO_IN_NAME,CFG_STDIO_OUT_NAME,CFG_STDIO_ERR_NAME);
    #endif
    //end stdio

    //network config
    extern void ModuleInstall_InitNet( );
    ModuleInstall_InitNet( );
    //end network config

	evtt_main = DJY_EvttRegist(EN_CORRELATIVE,CN_PRIO_RRS,0,0,
		__djy_main,NULL,CFG_MAINSTACK_LIMIT, "main function");
	//事件的两个参数暂设为0,如果用shell启动,可用来采集shell命令行参数
	DJY_EventPop(evtt_main,NULL,0,0,0,0);

    //----------------------------medium----------------------------//
    //heap
    #if ((CFG_DYNAMIC_MEM == true))
    extern bool_t Heap_DynamicModuleInit(void);
    Heap_DynamicModuleInit ( );
    #endif
    //end heap



	return ;
}

/*Modified at 2023-12-28 19:50:43*/
/****************************************************
 *  Automatically-generated file. Do not edit!	*
 ****************************************************/

#include "project_config.h"
#include "djyos.h"
#include "stdint.h"
#include "stddef.h"
#include "cpu_peri.h"
#include <Iboot_info.h>

#include <djyfs/filesystems.h>

extern ptu32_t djy_main(void);
//如果这个CN_MANUFACTURER_NAME名字要改，那djysrc里的Iboot_info.c中相应的名字也要改
const char CN_MANUFACTURER_NAME[] = PRODUCT_MANUFACTURER_NAME;


const struct ProductInfo Djy_Product_Info __attribute__ ((section(".DjyProductInfo"))) =
{
    .VersionNumber[0] = PRODUCT_VERSION_LARGE,
    .VersionNumber[1] = PRODUCT_VERSION_MEDIUM,
    .VersionNumber[2] = PRODUCT_VERSION_SMALL,
#if(CN_PTR_BITS < 64)
    .ManufacturerNameAddr      = (u32)(&CN_MANUFACTURER_NAME),
    .ManufacturerNamereserved32    = 0xffffffff,
#else
    .ManufacturerNameAddr      = (u64)(&CN_MANUFACTURER_NAME),
#endif
    .ProductClassify = PRODUCT_PRODUCT_CLASSIFY,
    .ProductType = PRODUCT_PRODUCT_MODEL,

    .TypeCode = PRODUCT_PRODUCT_MODEL_CODE,

    .ProductionTime = {'*','*','*','*'},
    .ProductionNumber = {'*','*','*','*','*'},
    .reserved8 = 0,
    .BoardType = PRODUCT_BOARD_TYPE,
    .CPU_Type = PRODUCT_CPU_TYPE,
    .Reserved ={
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff
            },
};


ptu32_t __djy_main(void)
{
    //modbus
    extern bool_t ModuleInstall_Modbus(void);
    ModuleInstall_Modbus();
    //end modbus

    djy_main();

	return 0;
}

void Sys_ModuleInit(void)
{
	uint16_t evtt_main;

    //shell
    extern void Stdio_KnlInOutInit(char * StdioIn, char *StdioOut);
    Stdio_KnlInOutInit(CFG_STDIO_IN_NAME,CFG_STDIO_OUT_NAME);
    extern s32 ModuleInstall_Shell(ptu32_t para);
    ModuleInstall_Shell(0);
    //end shell

    //----------------------------early----------------------------//
    //black box
    extern void ModuleInstall_BlackBox(void);
    ModuleInstall_BlackBox( );
    //end black box

    //device file system
    extern s32 ModuleInstall_dev(void);
    ModuleInstall_dev();    // 安装设备文件系统；
    //end device file system

    //djybus
    extern bool_t ModuleInstall_DjyBus(void);
    ModuleInstall_DjyBus ( );
    //end djybus

    //message queue
    extern bool_t ModuleInstall_MsgQ(void);
    ModuleInstall_MsgQ ( );
    //end message queue

    //multiplex
    extern bool_t ModuleInstall_Multiplex(void);
    ModuleInstall_Multiplex ();
    //end multiplex

    //spi bus
    extern bool_t ModuleInstall_SPIBus(void);
    ModuleInstall_SPIBus();
    //end spi bus

    //xip iboot file system
    extern s32 ModuleInstall_XIP_IBOOT_FS(u32 opt, void *data);
    ModuleInstall_XIP_IBOOT_FS(0,NULL);
    //end xip iboot file system

    //cpu onchip spi
    extern bool_t ModuleInstall_SPI(u8 port);
    #if CFG_SPI1_ENABLE==1
    ModuleInstall_SPI(CN_SPI1);
    #endif
    #if CFG_SPI2_ENABLE==1
    ModuleInstall_SPI(CN_SPI2);
    #endif
    #if CFG_SPI3_ENABLE==1
    ModuleInstall_SPI(CN_SPI3);
    #endif
    #if CFG_SPI4_ENABLE==1
    ModuleInstall_SPI(CN_SPI4);
    #endif
    //end cpu onchip spi

    //cpu onchip uart
    extern ptu32_t ModuleInstall_UART(ptu32_t SerialNo);
    #if CFG_UART1_ENABLE ==1
    ModuleInstall_UART(CN_UART1);
    #endif
    #if CFG_UART2_ENABLE ==1
    ModuleInstall_UART(CN_UART2);
    #endif
    #if CFG_UART3_ENABLE ==1
    ModuleInstall_UART(CN_UART3);
    #endif
    #if CFG_UART4_ENABLE ==1
    ModuleInstall_UART(CN_UART4);
    #endif
    #if CFG_UART5_ENABLE ==1
    ModuleInstall_UART(CN_UART5);
    #endif
    #if CFG_UART6_ENABLE ==1
    ModuleInstall_UART(CN_UART6);
    #endif
    #if CFG_UART7_ENABLE ==1
    ModuleInstall_UART(CN_UART7);
    #endif
    #if CFG_UART8_ENABLE ==1
    ModuleInstall_UART(CN_UART8);
    #endif
    //end cpu onchip uart

    //fat file system
    extern s32 ModuleInstall_FAT(const char *dir, u32 opt, void *data);
    ModuleInstall_FAT(CFG_FAT_MOUNT_POINT, CFG_FAT_MS_INSTALLUSE, CFG_FAT_MEDIA_KIND);
    //end fat file system

    //cpu onchip timer
    extern bool_t ModuleInstall_HardTimer(void);
    ModuleInstall_HardTimer();
    //end cpu onchip timer

    //cpu drive inner flash
    s32 ModuleInstall_EmbededFlash(u32 doformat);
    ModuleInstall_EmbededFlash(CFG_EFLASH_PART_FORMAT);
    //end cpu drive inner flash

    //emflash insatall xip
    extern s32 ModuleInstall_EmFlashInstallXIP(const char *TargetFs,s32 bstart, s32 bend, u32 doformat);
    ModuleInstall_EmFlashInstallXIP(CFG_EFLASH_XIPFSMOUNT_NAME,CFG_EFLASH_XIP_PART_START,
    CFG_EFLASH_XIP_PART_END, CFG_EFLASH_XIP_PART_FORMAT);
    //end emflash insatall xip

    //kernel
    #if(CFG_OS_TINY == flase)
    extern s32 kernel_command(void);
    kernel_command();
    #endif
    //end kernel

    //Nls Charset
    extern ptu32_t ModuleInstall_Charset(ptu32_t para);
    ModuleInstall_Charset(0);
    extern void ModuleInstall_CharsetNls(const char * DefaultCharset);
    ModuleInstall_CharsetNls("C");
    //end Nls Charset

    //Software Timers
    extern bool_t ModuleInstall_Timer(void);
    ModuleInstall_Timer();
    //end Software Timers

    //tcpip
    extern bool_t ModuleInstall_TcpIp(void);
    ModuleInstall_TcpIp( );
    //end tcpip

    //cpu onchip ETH
    extern bool_t ModuleInstall_ETH(void);
    ModuleInstall_ETH( );
    //end cpu onchip ETH

    //norflash W25QXX
    extern s32 ModuleInstall_W25qxx(void);
    ModuleInstall_W25qxx();
    //end norflash W25QXX

    //W25QXX FAT
    extern bool_t ModuleInstall_W25qxxInstallFat(const char *TargetFs, s32 bend, u32 doformat);
    ModuleInstall_W25qxxInstallFat(CFG_W25_FAT_MOUNT_NAME,CFG_W25_FAT_PART_END,CFG_W25_FAT_PART_FORMAT);
    //end W25QXX FAT

    //----------------------------later----------------------------//
    //stdio
    #if(CFG_STDIO_STDIOFILE == true)
    extern s32 ModuleInstall_STDIO(const char *in,const char *out, const char *err);
    ModuleInstall_STDIO(CFG_STDIO_IN_NAME,CFG_STDIO_OUT_NAME,CFG_STDIO_ERR_NAME);
    #endif
    //end stdio

    //network config
    extern void ModuleInstall_InitNet( );
    ModuleInstall_InitNet( );
    //end network config

	evtt_main = DJY_EvttRegist(EN_CORRELATIVE,CN_PRIO_RRS,0,0,
		__djy_main,NULL,CFG_MAINSTACK_LIMIT, "main function");
	//事件的两个参数暂设为0,如果用shell启动,可用来采集shell命令行参数
	DJY_EventPop(evtt_main,NULL,0,0,0,0);

    //----------------------------medium----------------------------//
    //heap
    #if ((CFG_DYNAMIC_MEM == true))
    extern bool_t Heap_DynamicModuleInit(void);
    Heap_DynamicModuleInit ( );
    #endif
    //end heap



	return ;
}

/*Modified at 2024-01-23 16:29:49*/
/****************************************************
 *  Automatically-generated file. Do not edit!	*
 ****************************************************/

#include "project_config.h"
#include "djyos.h"
#include "stdint.h"
#include "stddef.h"
#include "cpu_peri.h"
#include <Iboot_info.h>

#include <djyfs/filesystems.h>

extern ptu32_t djy_main(void);
//如果这个CN_MANUFACTURER_NAME名字要改，那djysrc里的Iboot_info.c中相应的名字也要改
const char CN_MANUFACTURER_NAME[] = PRODUCT_MANUFACTURER_NAME;


const struct ProductInfo Djy_Product_Info __attribute__ ((section(".DjyProductInfo"))) =
{
    .VersionNumber[0] = PRODUCT_VERSION_LARGE,
    .VersionNumber[1] = PRODUCT_VERSION_MEDIUM,
    .VersionNumber[2] = PRODUCT_VERSION_SMALL,
#if(CN_PTR_BITS < 64)
    .ManufacturerNameAddr      = (u32)(&CN_MANUFACTURER_NAME),
    .ManufacturerNamereserved32    = 0xffffffff,
#else
    .ManufacturerNameAddr      = (u64)(&CN_MANUFACTURER_NAME),
#endif
    .ProductClassify = PRODUCT_PRODUCT_CLASSIFY,
    .ProductType = PRODUCT_PRODUCT_MODEL,

    .TypeCode = PRODUCT_PRODUCT_MODEL_CODE,

    .ProductionTime = {'*','*','*','*'},
    .ProductionNumber = {'*','*','*','*','*'},
    .reserved8 = 0,
    .BoardType = PRODUCT_BOARD_TYPE,
    .CPU_Type = PRODUCT_CPU_TYPE,
    .Reserved ={
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff
            },
};


ptu32_t __djy_main(void)
{
    //modbus
    extern bool_t ModuleInstall_Modbus(void);
    ModuleInstall_Modbus();
    //end modbus

    djy_main();

	return 0;
}

void Sys_ModuleInit(void)
{
	uint16_t evtt_main;

    //shell
    extern void Stdio_KnlInOutInit(char * StdioIn, char *StdioOut);
    Stdio_KnlInOutInit(CFG_STDIO_IN_NAME,CFG_STDIO_OUT_NAME);
    extern s32 ModuleInstall_Shell(ptu32_t para);
    ModuleInstall_Shell(0);
    //end shell

    //----------------------------early----------------------------//
    //black box
    extern void ModuleInstall_BlackBox(void);
    ModuleInstall_BlackBox( );
    //end black box

    //device file system
    extern s32 ModuleInstall_dev(void);
    ModuleInstall_dev();    // 安装设备文件系统；
    //end device file system

    //djybus
    extern bool_t ModuleInstall_DjyBus(void);
    ModuleInstall_DjyBus ( );
    //end djybus

    //message queue
    extern bool_t ModuleInstall_MsgQ(void);
    ModuleInstall_MsgQ ( );
    //end message queue

    //multiplex
    extern bool_t ModuleInstall_Multiplex(void);
    ModuleInstall_Multiplex ();
    //end multiplex

    //spi bus
    extern bool_t ModuleInstall_SPIBus(void);
    ModuleInstall_SPIBus();
    //end spi bus

    //cpu onchip spi
    extern bool_t ModuleInstall_SPI(u8 port);
    #if CFG_SPI1_ENABLE==1
    ModuleInstall_SPI(CN_SPI1);
    #endif
    #if CFG_SPI2_ENABLE==1
    ModuleInstall_SPI(CN_SPI2);
    #endif
    #if CFG_SPI3_ENABLE==1
    ModuleInstall_SPI(CN_SPI3);
    #endif
    #if CFG_SPI4_ENABLE==1
    ModuleInstall_SPI(CN_SPI4);
    #endif
    //end cpu onchip spi

    //xip iboot file system
    extern s32 ModuleInstall_XIP_IBOOT_FS(u32 opt, void *data);
    ModuleInstall_XIP_IBOOT_FS(0,NULL);
    //end xip iboot file system

    //cpu drive inner flash
    s32 ModuleInstall_EmbededFlash(u32 doformat);
    ModuleInstall_EmbededFlash(CFG_EFLASH_PART_FORMAT);
    //end cpu drive inner flash

    //emflash insatall xip
    extern s32 ModuleInstall_EmFlashInstallXIP(const char *TargetFs,s32 bstart, s32 bend, u32 doformat);
    ModuleInstall_EmFlashInstallXIP(CFG_EFLASH_XIPFSMOUNT_NAME,CFG_EFLASH_XIP_PART_START,
    CFG_EFLASH_XIP_PART_END, CFG_EFLASH_XIP_PART_FORMAT);
    //end emflash insatall xip

    //kernel
    #if(CFG_OS_TINY == flase)
    extern s32 kernel_command(void);
    kernel_command();
    #endif
    //end kernel

    //Nls Charset
    extern ptu32_t ModuleInstall_Charset(ptu32_t para);
    ModuleInstall_Charset(0);
    extern void ModuleInstall_CharsetNls(const char * DefaultCharset);
    ModuleInstall_CharsetNls("C");
    //end Nls Charset

    //fat file system
    extern s32 ModuleInstall_FAT(const char *dir, u32 opt, void *data);
    ModuleInstall_FAT(CFG_FAT_MOUNT_POINT, CFG_FAT_MS_INSTALLUSE, CFG_FAT_MEDIA_KIND);
    //end fat file system

    //Software Timers
    extern bool_t ModuleInstall_Timer(void);
    ModuleInstall_Timer();
    //end Software Timers

    //cpu onchip timer
    extern bool_t ModuleInstall_HardTimer(void);
    ModuleInstall_HardTimer();
    //end cpu onchip timer

    //tcpip
    extern bool_t ModuleInstall_TcpIp(void);
    ModuleInstall_TcpIp( );
    //end tcpip

    //cpu onchip ETH
    extern bool_t ModuleInstall_ETH(void);
    ModuleInstall_ETH( );
    //end cpu onchip ETH

    //cpu onchip uart
    extern ptu32_t ModuleInstall_UART(ptu32_t SerialNo);
    #if CFG_UART1_ENABLE ==1
    ModuleInstall_UART(CN_UART1);
    #endif
    #if CFG_UART2_ENABLE ==1
    ModuleInstall_UART(CN_UART2);
    #endif
    #if CFG_UART3_ENABLE ==1
    ModuleInstall_UART(CN_UART3);
    #endif
    #if CFG_UART4_ENABLE ==1
    ModuleInstall_UART(CN_UART4);
    #endif
    #if CFG_UART5_ENABLE ==1
    ModuleInstall_UART(CN_UART5);
    #endif
    #if CFG_UART6_ENABLE ==1
    ModuleInstall_UART(CN_UART6);
    #endif
    #if CFG_UART7_ENABLE ==1
    ModuleInstall_UART(CN_UART7);
    #endif
    #if CFG_UART8_ENABLE ==1
    ModuleInstall_UART(CN_UART8);
    #endif
    //end cpu onchip uart

    //norflash W25QXX
    extern s32 ModuleInstall_W25qxx(void);
    ModuleInstall_W25qxx();
    //end norflash W25QXX

    //W25QXX FAT
    extern bool_t ModuleInstall_W25qxxInstallFat(const char *TargetFs, s32 bend, u32 doformat);
    ModuleInstall_W25qxxInstallFat(CFG_W25_FAT_MOUNT_NAME,CFG_W25_FAT_PART_END,CFG_W25_FAT_PART_FORMAT);
    //end W25QXX FAT

    //----------------------------later----------------------------//
    //stdio
    #if(CFG_STDIO_STDIOFILE == true)
    extern s32 ModuleInstall_STDIO(const char *in,const char *out, const char *err);
    ModuleInstall_STDIO(CFG_STDIO_IN_NAME,CFG_STDIO_OUT_NAME,CFG_STDIO_ERR_NAME);
    #endif
    //end stdio

    //network config
    extern void ModuleInstall_InitNet( );
    ModuleInstall_InitNet( );
    //end network config

	evtt_main = DJY_EvttRegist(EN_CORRELATIVE,CN_PRIO_RRS,0,0,
		__djy_main,NULL,CFG_MAINSTACK_LIMIT, "main function");
	//事件的两个参数暂设为0,如果用shell启动,可用来采集shell命令行参数
	DJY_EventPop(evtt_main,NULL,0,0,0,0);

    //----------------------------medium----------------------------//
    //heap
    #if ((CFG_DYNAMIC_MEM == true))
    extern bool_t Heap_DynamicModuleInit(void);
    Heap_DynamicModuleInit ( );
    #endif
    //end heap



	return ;
}

/*Modified at 2024-01-23 16:29:53*/
/****************************************************
 *  Automatically-generated file. Do not edit!	*
 ****************************************************/

#include "project_config.h"
#include "djyos.h"
#include "stdint.h"
#include "stddef.h"
#include "cpu_peri.h"
#include <Iboot_info.h>

#include <djyfs/filesystems.h>

extern ptu32_t djy_main(void);
//如果这个CN_MANUFACTURER_NAME名字要改，那djysrc里的Iboot_info.c中相应的名字也要改
const char CN_MANUFACTURER_NAME[] = PRODUCT_MANUFACTURER_NAME;


const struct ProductInfo Djy_Product_Info __attribute__ ((section(".DjyProductInfo"))) =
{
    .VersionNumber[0] = PRODUCT_VERSION_LARGE,
    .VersionNumber[1] = PRODUCT_VERSION_MEDIUM,
    .VersionNumber[2] = PRODUCT_VERSION_SMALL,
#if(CN_PTR_BITS < 64)
    .ManufacturerNameAddr      = (u32)(&CN_MANUFACTURER_NAME),
    .ManufacturerNamereserved32    = 0xffffffff,
#else
    .ManufacturerNameAddr      = (u64)(&CN_MANUFACTURER_NAME),
#endif
    .ProductClassify = PRODUCT_PRODUCT_CLASSIFY,
    .ProductType = PRODUCT_PRODUCT_MODEL,

    .TypeCode = PRODUCT_PRODUCT_MODEL_CODE,

    .ProductionTime = {'*','*','*','*'},
    .ProductionNumber = {'*','*','*','*','*'},
    .reserved8 = 0,
    .BoardType = PRODUCT_BOARD_TYPE,
    .CPU_Type = PRODUCT_CPU_TYPE,
    .Reserved ={
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff
            },
};


ptu32_t __djy_main(void)
{
    //modbus
    extern bool_t ModuleInstall_Modbus(void);
    ModuleInstall_Modbus();
    //end modbus

    djy_main();

	return 0;
}

void Sys_ModuleInit(void)
{
	uint16_t evtt_main;

    //shell
    extern void Stdio_KnlInOutInit(char * StdioIn, char *StdioOut);
    Stdio_KnlInOutInit(CFG_STDIO_IN_NAME,CFG_STDIO_OUT_NAME);
    extern s32 ModuleInstall_Shell(ptu32_t para);
    ModuleInstall_Shell(0);
    //end shell

    //----------------------------early----------------------------//
    //black box
    extern void ModuleInstall_BlackBox(void);
    ModuleInstall_BlackBox( );
    //end black box

    //device file system
    extern s32 ModuleInstall_dev(void);
    ModuleInstall_dev();    // 安装设备文件系统；
    //end device file system

    //djybus
    extern bool_t ModuleInstall_DjyBus(void);
    ModuleInstall_DjyBus ( );
    //end djybus

    //message queue
    extern bool_t ModuleInstall_MsgQ(void);
    ModuleInstall_MsgQ ( );
    //end message queue

    //multiplex
    extern bool_t ModuleInstall_Multiplex(void);
    ModuleInstall_Multiplex ();
    //end multiplex

    //spi bus
    extern bool_t ModuleInstall_SPIBus(void);
    ModuleInstall_SPIBus();
    //end spi bus

    //xip iboot file system
    extern s32 ModuleInstall_XIP_IBOOT_FS(u32 opt, void *data);
    ModuleInstall_XIP_IBOOT_FS(0,NULL);
    //end xip iboot file system

    //cpu onchip spi
    extern bool_t ModuleInstall_SPI(u8 port);
    #if CFG_SPI1_ENABLE==1
    ModuleInstall_SPI(CN_SPI1);
    #endif
    #if CFG_SPI2_ENABLE==1
    ModuleInstall_SPI(CN_SPI2);
    #endif
    #if CFG_SPI3_ENABLE==1
    ModuleInstall_SPI(CN_SPI3);
    #endif
    #if CFG_SPI4_ENABLE==1
    ModuleInstall_SPI(CN_SPI4);
    #endif
    //end cpu onchip spi

    //cpu onchip uart
    extern ptu32_t ModuleInstall_UART(ptu32_t SerialNo);
    #if CFG_UART1_ENABLE ==1
    ModuleInstall_UART(CN_UART1);
    #endif
    #if CFG_UART2_ENABLE ==1
    ModuleInstall_UART(CN_UART2);
    #endif
    #if CFG_UART3_ENABLE ==1
    ModuleInstall_UART(CN_UART3);
    #endif
    #if CFG_UART4_ENABLE ==1
    ModuleInstall_UART(CN_UART4);
    #endif
    #if CFG_UART5_ENABLE ==1
    ModuleInstall_UART(CN_UART5);
    #endif
    #if CFG_UART6_ENABLE ==1
    ModuleInstall_UART(CN_UART6);
    #endif
    #if CFG_UART7_ENABLE ==1
    ModuleInstall_UART(CN_UART7);
    #endif
    #if CFG_UART8_ENABLE ==1
    ModuleInstall_UART(CN_UART8);
    #endif
    //end cpu onchip uart

    //fat file system
    extern s32 ModuleInstall_FAT(const char *dir, u32 opt, void *data);
    ModuleInstall_FAT(CFG_FAT_MOUNT_POINT, CFG_FAT_MS_INSTALLUSE, CFG_FAT_MEDIA_KIND);
    //end fat file system

    //cpu onchip timer
    extern bool_t ModuleInstall_HardTimer(void);
    ModuleInstall_HardTimer();
    //end cpu onchip timer

    //cpu drive inner flash
    s32 ModuleInstall_EmbededFlash(u32 doformat);
    ModuleInstall_EmbededFlash(CFG_EFLASH_PART_FORMAT);
    //end cpu drive inner flash

    //emflash insatall xip
    extern s32 ModuleInstall_EmFlashInstallXIP(const char *TargetFs,s32 bstart, s32 bend, u32 doformat);
    ModuleInstall_EmFlashInstallXIP(CFG_EFLASH_XIPFSMOUNT_NAME,CFG_EFLASH_XIP_PART_START,
    CFG_EFLASH_XIP_PART_END, CFG_EFLASH_XIP_PART_FORMAT);
    //end emflash insatall xip

    //kernel
    #if(CFG_OS_TINY == flase)
    extern s32 kernel_command(void);
    kernel_command();
    #endif
    //end kernel

    //Nls Charset
    extern ptu32_t ModuleInstall_Charset(ptu32_t para);
    ModuleInstall_Charset(0);
    extern void ModuleInstall_CharsetNls(const char * DefaultCharset);
    ModuleInstall_CharsetNls("C");
    //end Nls Charset

    //Software Timers
    extern bool_t ModuleInstall_Timer(void);
    ModuleInstall_Timer();
    //end Software Timers

    //tcpip
    extern bool_t ModuleInstall_TcpIp(void);
    ModuleInstall_TcpIp( );
    //end tcpip

    //cpu onchip ETH
    extern bool_t ModuleInstall_ETH(void);
    ModuleInstall_ETH( );
    //end cpu onchip ETH

    //norflash W25QXX
    extern s32 ModuleInstall_W25qxx(void);
    ModuleInstall_W25qxx();
    //end norflash W25QXX

    //W25QXX FAT
    extern bool_t ModuleInstall_W25qxxInstallFat(const char *TargetFs, s32 bend, u32 doformat);
    ModuleInstall_W25qxxInstallFat(CFG_W25_FAT_MOUNT_NAME,CFG_W25_FAT_PART_END,CFG_W25_FAT_PART_FORMAT);
    //end W25QXX FAT

    //----------------------------later----------------------------//
    //stdio
    #if(CFG_STDIO_STDIOFILE == true)
    extern s32 ModuleInstall_STDIO(const char *in,const char *out, const char *err);
    ModuleInstall_STDIO(CFG_STDIO_IN_NAME,CFG_STDIO_OUT_NAME,CFG_STDIO_ERR_NAME);
    #endif
    //end stdio

    //network config
    extern void ModuleInstall_InitNet( );
    ModuleInstall_InitNet( );
    //end network config

	evtt_main = DJY_EvttRegist(EN_CORRELATIVE,CN_PRIO_RRS,0,0,
		__djy_main,NULL,CFG_MAINSTACK_LIMIT, "main function");
	//事件的两个参数暂设为0,如果用shell启动,可用来采集shell命令行参数
	DJY_EventPop(evtt_main,NULL,0,0,0,0);

    //----------------------------medium----------------------------//
    //heap
    #if ((CFG_DYNAMIC_MEM == true))
    extern bool_t Heap_DynamicModuleInit(void);
    Heap_DynamicModuleInit ( );
    #endif
    //end heap



	return ;
}

/*Modified at 2024-01-23 16:30:02*/
/****************************************************
 *  Automatically-generated file. Do not edit!	*
 ****************************************************/

#include "project_config.h"
#include "djyos.h"
#include "stdint.h"
#include "stddef.h"
#include "cpu_peri.h"
#include <Iboot_info.h>

#include <djyfs/filesystems.h>

extern ptu32_t djy_main(void);
//如果这个CN_MANUFACTURER_NAME名字要改，那djysrc里的Iboot_info.c中相应的名字也要改
const char CN_MANUFACTURER_NAME[] = PRODUCT_MANUFACTURER_NAME;


const struct ProductInfo Djy_Product_Info __attribute__ ((section(".DjyProductInfo"))) =
{
    .VersionNumber[0] = PRODUCT_VERSION_LARGE,
    .VersionNumber[1] = PRODUCT_VERSION_MEDIUM,
    .VersionNumber[2] = PRODUCT_VERSION_SMALL,
#if(CN_PTR_BITS < 64)
    .ManufacturerNameAddr      = (u32)(&CN_MANUFACTURER_NAME),
    .ManufacturerNamereserved32    = 0xffffffff,
#else
    .ManufacturerNameAddr      = (u64)(&CN_MANUFACTURER_NAME),
#endif
    .ProductClassify = PRODUCT_PRODUCT_CLASSIFY,
    .ProductType = PRODUCT_PRODUCT_MODEL,

    .TypeCode = PRODUCT_PRODUCT_MODEL_CODE,

    .ProductionTime = {'*','*','*','*'},
    .ProductionNumber = {'*','*','*','*','*'},
    .reserved8 = 0,
    .BoardType = PRODUCT_BOARD_TYPE,
    .CPU_Type = PRODUCT_CPU_TYPE,
    .Reserved ={
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff
            },
};


ptu32_t __djy_main(void)
{
    //modbus
    extern bool_t ModuleInstall_Modbus(void);
    ModuleInstall_Modbus();
    //end modbus

    djy_main();

	return 0;
}

void Sys_ModuleInit(void)
{
	uint16_t evtt_main;

    //shell
    extern void Stdio_KnlInOutInit(char * StdioIn, char *StdioOut);
    Stdio_KnlInOutInit(CFG_STDIO_IN_NAME,CFG_STDIO_OUT_NAME);
    extern s32 ModuleInstall_Shell(ptu32_t para);
    ModuleInstall_Shell(0);
    //end shell

    //----------------------------early----------------------------//
    //black box
    extern void ModuleInstall_BlackBox(void);
    ModuleInstall_BlackBox( );
    //end black box

    //device file system
    extern s32 ModuleInstall_dev(void);
    ModuleInstall_dev();    // 安装设备文件系统；
    //end device file system

    //djybus
    extern bool_t ModuleInstall_DjyBus(void);
    ModuleInstall_DjyBus ( );
    //end djybus

    //message queue
    extern bool_t ModuleInstall_MsgQ(void);
    ModuleInstall_MsgQ ( );
    //end message queue

    //multiplex
    extern bool_t ModuleInstall_Multiplex(void);
    ModuleInstall_Multiplex ();
    //end multiplex

    //spi bus
    extern bool_t ModuleInstall_SPIBus(void);
    ModuleInstall_SPIBus();
    //end spi bus

    //cpu onchip spi
    extern bool_t ModuleInstall_SPI(u8 port);
    #if CFG_SPI1_ENABLE==1
    ModuleInstall_SPI(CN_SPI1);
    #endif
    #if CFG_SPI2_ENABLE==1
    ModuleInstall_SPI(CN_SPI2);
    #endif
    #if CFG_SPI3_ENABLE==1
    ModuleInstall_SPI(CN_SPI3);
    #endif
    #if CFG_SPI4_ENABLE==1
    ModuleInstall_SPI(CN_SPI4);
    #endif
    //end cpu onchip spi

    //xip iboot file system
    extern s32 ModuleInstall_XIP_IBOOT_FS(u32 opt, void *data);
    ModuleInstall_XIP_IBOOT_FS(0,NULL);
    //end xip iboot file system

    //cpu drive inner flash
    s32 ModuleInstall_EmbededFlash(u32 doformat);
    ModuleInstall_EmbededFlash(CFG_EFLASH_PART_FORMAT);
    //end cpu drive inner flash

    //emflash insatall xip
    extern s32 ModuleInstall_EmFlashInstallXIP(const char *TargetFs,s32 bstart, s32 bend, u32 doformat);
    ModuleInstall_EmFlashInstallXIP(CFG_EFLASH_XIPFSMOUNT_NAME,CFG_EFLASH_XIP_PART_START,
    CFG_EFLASH_XIP_PART_END, CFG_EFLASH_XIP_PART_FORMAT);
    //end emflash insatall xip

    //kernel
    #if(CFG_OS_TINY == flase)
    extern s32 kernel_command(void);
    kernel_command();
    #endif
    //end kernel

    //Nls Charset
    extern ptu32_t ModuleInstall_Charset(ptu32_t para);
    ModuleInstall_Charset(0);
    extern void ModuleInstall_CharsetNls(const char * DefaultCharset);
    ModuleInstall_CharsetNls("C");
    //end Nls Charset

    //fat file system
    extern s32 ModuleInstall_FAT(const char *dir, u32 opt, void *data);
    ModuleInstall_FAT(CFG_FAT_MOUNT_POINT, CFG_FAT_MS_INSTALLUSE, CFG_FAT_MEDIA_KIND);
    //end fat file system

    //Software Timers
    extern bool_t ModuleInstall_Timer(void);
    ModuleInstall_Timer();
    //end Software Timers

    //cpu onchip timer
    extern bool_t ModuleInstall_HardTimer(void);
    ModuleInstall_HardTimer();
    //end cpu onchip timer

    //tcpip
    extern bool_t ModuleInstall_TcpIp(void);
    ModuleInstall_TcpIp( );
    //end tcpip

    //cpu onchip ETH
    extern bool_t ModuleInstall_ETH(void);
    ModuleInstall_ETH( );
    //end cpu onchip ETH

    //cpu onchip uart
    extern ptu32_t ModuleInstall_UART(ptu32_t SerialNo);
    #if CFG_UART1_ENABLE ==1
    ModuleInstall_UART(CN_UART1);
    #endif
    #if CFG_UART2_ENABLE ==1
    ModuleInstall_UART(CN_UART2);
    #endif
    #if CFG_UART3_ENABLE ==1
    ModuleInstall_UART(CN_UART3);
    #endif
    #if CFG_UART4_ENABLE ==1
    ModuleInstall_UART(CN_UART4);
    #endif
    #if CFG_UART5_ENABLE ==1
    ModuleInstall_UART(CN_UART5);
    #endif
    #if CFG_UART6_ENABLE ==1
    ModuleInstall_UART(CN_UART6);
    #endif
    #if CFG_UART7_ENABLE ==1
    ModuleInstall_UART(CN_UART7);
    #endif
    #if CFG_UART8_ENABLE ==1
    ModuleInstall_UART(CN_UART8);
    #endif
    //end cpu onchip uart

    //norflash W25QXX
    extern s32 ModuleInstall_W25qxx(void);
    ModuleInstall_W25qxx();
    //end norflash W25QXX

    //W25QXX FAT
    extern bool_t ModuleInstall_W25qxxInstallFat(const char *TargetFs, s32 bend, u32 doformat);
    ModuleInstall_W25qxxInstallFat(CFG_W25_FAT_MOUNT_NAME,CFG_W25_FAT_PART_END,CFG_W25_FAT_PART_FORMAT);
    //end W25QXX FAT

    //----------------------------later----------------------------//
    //stdio
    #if(CFG_STDIO_STDIOFILE == true)
    extern s32 ModuleInstall_STDIO(const char *in,const char *out, const char *err);
    ModuleInstall_STDIO(CFG_STDIO_IN_NAME,CFG_STDIO_OUT_NAME,CFG_STDIO_ERR_NAME);
    #endif
    //end stdio

    //network config
    extern void ModuleInstall_InitNet( );
    ModuleInstall_InitNet( );
    //end network config

	evtt_main = DJY_EvttRegist(EN_CORRELATIVE,CN_PRIO_RRS,0,0,
		__djy_main,NULL,CFG_MAINSTACK_LIMIT, "main function");
	//事件的两个参数暂设为0,如果用shell启动,可用来采集shell命令行参数
	DJY_EventPop(evtt_main,NULL,0,0,0,0);

    //----------------------------medium----------------------------//
    //heap
    #if ((CFG_DYNAMIC_MEM == true))
    extern bool_t Heap_DynamicModuleInit(void);
    Heap_DynamicModuleInit ( );
    #endif
    //end heap



	return ;
}

/*Modified at 2024-01-23 16:30:06*/
/****************************************************
 *  Automatically-generated file. Do not edit!	*
 ****************************************************/

#include "project_config.h"
#include "djyos.h"
#include "stdint.h"
#include "stddef.h"
#include "cpu_peri.h"
#include <Iboot_info.h>

#include <djyfs/filesystems.h>

extern ptu32_t djy_main(void);
//如果这个CN_MANUFACTURER_NAME名字要改，那djysrc里的Iboot_info.c中相应的名字也要改
const char CN_MANUFACTURER_NAME[] = PRODUCT_MANUFACTURER_NAME;


const struct ProductInfo Djy_Product_Info __attribute__ ((section(".DjyProductInfo"))) =
{
    .VersionNumber[0] = PRODUCT_VERSION_LARGE,
    .VersionNumber[1] = PRODUCT_VERSION_MEDIUM,
    .VersionNumber[2] = PRODUCT_VERSION_SMALL,
#if(CN_PTR_BITS < 64)
    .ManufacturerNameAddr      = (u32)(&CN_MANUFACTURER_NAME),
    .ManufacturerNamereserved32    = 0xffffffff,
#else
    .ManufacturerNameAddr      = (u64)(&CN_MANUFACTURER_NAME),
#endif
    .ProductClassify = PRODUCT_PRODUCT_CLASSIFY,
    .ProductType = PRODUCT_PRODUCT_MODEL,

    .TypeCode = PRODUCT_PRODUCT_MODEL_CODE,

    .ProductionTime = {'*','*','*','*'},
    .ProductionNumber = {'*','*','*','*','*'},
    .reserved8 = 0,
    .BoardType = PRODUCT_BOARD_TYPE,
    .CPU_Type = PRODUCT_CPU_TYPE,
    .Reserved ={
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff
            },
};


ptu32_t __djy_main(void)
{
    //modbus
    extern bool_t ModuleInstall_Modbus(void);
    ModuleInstall_Modbus();
    //end modbus

    djy_main();

	return 0;
}

void Sys_ModuleInit(void)
{
	uint16_t evtt_main;

    //shell
    extern void Stdio_KnlInOutInit(char * StdioIn, char *StdioOut);
    Stdio_KnlInOutInit(CFG_STDIO_IN_NAME,CFG_STDIO_OUT_NAME);
    extern s32 ModuleInstall_Shell(ptu32_t para);
    ModuleInstall_Shell(0);
    //end shell

    //----------------------------early----------------------------//
    //black box
    extern void ModuleInstall_BlackBox(void);
    ModuleInstall_BlackBox( );
    //end black box

    //device file system
    extern s32 ModuleInstall_dev(void);
    ModuleInstall_dev();    // 安装设备文件系统；
    //end device file system

    //djybus
    extern bool_t ModuleInstall_DjyBus(void);
    ModuleInstall_DjyBus ( );
    //end djybus

    //message queue
    extern bool_t ModuleInstall_MsgQ(void);
    ModuleInstall_MsgQ ( );
    //end message queue

    //multiplex
    extern bool_t ModuleInstall_Multiplex(void);
    ModuleInstall_Multiplex ();
    //end multiplex

    //spi bus
    extern bool_t ModuleInstall_SPIBus(void);
    ModuleInstall_SPIBus();
    //end spi bus

    //xip iboot file system
    extern s32 ModuleInstall_XIP_IBOOT_FS(u32 opt, void *data);
    ModuleInstall_XIP_IBOOT_FS(0,NULL);
    //end xip iboot file system

    //cpu onchip spi
    extern bool_t ModuleInstall_SPI(u8 port);
    #if CFG_SPI1_ENABLE==1
    ModuleInstall_SPI(CN_SPI1);
    #endif
    #if CFG_SPI2_ENABLE==1
    ModuleInstall_SPI(CN_SPI2);
    #endif
    #if CFG_SPI3_ENABLE==1
    ModuleInstall_SPI(CN_SPI3);
    #endif
    #if CFG_SPI4_ENABLE==1
    ModuleInstall_SPI(CN_SPI4);
    #endif
    //end cpu onchip spi

    //cpu onchip uart
    extern ptu32_t ModuleInstall_UART(ptu32_t SerialNo);
    #if CFG_UART1_ENABLE ==1
    ModuleInstall_UART(CN_UART1);
    #endif
    #if CFG_UART2_ENABLE ==1
    ModuleInstall_UART(CN_UART2);
    #endif
    #if CFG_UART3_ENABLE ==1
    ModuleInstall_UART(CN_UART3);
    #endif
    #if CFG_UART4_ENABLE ==1
    ModuleInstall_UART(CN_UART4);
    #endif
    #if CFG_UART5_ENABLE ==1
    ModuleInstall_UART(CN_UART5);
    #endif
    #if CFG_UART6_ENABLE ==1
    ModuleInstall_UART(CN_UART6);
    #endif
    #if CFG_UART7_ENABLE ==1
    ModuleInstall_UART(CN_UART7);
    #endif
    #if CFG_UART8_ENABLE ==1
    ModuleInstall_UART(CN_UART8);
    #endif
    //end cpu onchip uart

    //fat file system
    extern s32 ModuleInstall_FAT(const char *dir, u32 opt, void *data);
    ModuleInstall_FAT(CFG_FAT_MOUNT_POINT, CFG_FAT_MS_INSTALLUSE, CFG_FAT_MEDIA_KIND);
    //end fat file system

    //cpu onchip timer
    extern bool_t ModuleInstall_HardTimer(void);
    ModuleInstall_HardTimer();
    //end cpu onchip timer

    //cpu drive inner flash
    s32 ModuleInstall_EmbededFlash(u32 doformat);
    ModuleInstall_EmbededFlash(CFG_EFLASH_PART_FORMAT);
    //end cpu drive inner flash

    //emflash insatall xip
    extern s32 ModuleInstall_EmFlashInstallXIP(const char *TargetFs,s32 bstart, s32 bend, u32 doformat);
    ModuleInstall_EmFlashInstallXIP(CFG_EFLASH_XIPFSMOUNT_NAME,CFG_EFLASH_XIP_PART_START,
    CFG_EFLASH_XIP_PART_END, CFG_EFLASH_XIP_PART_FORMAT);
    //end emflash insatall xip

    //kernel
    #if(CFG_OS_TINY == flase)
    extern s32 kernel_command(void);
    kernel_command();
    #endif
    //end kernel

    //Nls Charset
    extern ptu32_t ModuleInstall_Charset(ptu32_t para);
    ModuleInstall_Charset(0);
    extern void ModuleInstall_CharsetNls(const char * DefaultCharset);
    ModuleInstall_CharsetNls("C");
    //end Nls Charset

    //Software Timers
    extern bool_t ModuleInstall_Timer(void);
    ModuleInstall_Timer();
    //end Software Timers

    //tcpip
    extern bool_t ModuleInstall_TcpIp(void);
    ModuleInstall_TcpIp( );
    //end tcpip

    //cpu onchip ETH
    extern bool_t ModuleInstall_ETH(void);
    ModuleInstall_ETH( );
    //end cpu onchip ETH

    //norflash W25QXX
    extern s32 ModuleInstall_W25qxx(void);
    ModuleInstall_W25qxx();
    //end norflash W25QXX

    //W25QXX FAT
    extern bool_t ModuleInstall_W25qxxInstallFat(const char *TargetFs, s32 bend, u32 doformat);
    ModuleInstall_W25qxxInstallFat(CFG_W25_FAT_MOUNT_NAME,CFG_W25_FAT_PART_END,CFG_W25_FAT_PART_FORMAT);
    //end W25QXX FAT

    //----------------------------later----------------------------//
    //stdio
    #if(CFG_STDIO_STDIOFILE == true)
    extern s32 ModuleInstall_STDIO(const char *in,const char *out, const char *err);
    ModuleInstall_STDIO(CFG_STDIO_IN_NAME,CFG_STDIO_OUT_NAME,CFG_STDIO_ERR_NAME);
    #endif
    //end stdio

    //network config
    extern void ModuleInstall_InitNet( );
    ModuleInstall_InitNet( );
    //end network config

	evtt_main = DJY_EvttRegist(EN_CORRELATIVE,CN_PRIO_RRS,0,0,
		__djy_main,NULL,CFG_MAINSTACK_LIMIT, "main function");
	//事件的两个参数暂设为0,如果用shell启动,可用来采集shell命令行参数
	DJY_EventPop(evtt_main,NULL,0,0,0,0);

    //----------------------------medium----------------------------//
    //heap
    #if ((CFG_DYNAMIC_MEM == true))
    extern bool_t Heap_DynamicModuleInit(void);
    Heap_DynamicModuleInit ( );
    #endif
    //end heap



	return ;
}

/*Modified at 2024-01-23 17:17:35*/
/****************************************************
 *  Automatically-generated file. Do not edit!	*
 ****************************************************/

#include "project_config.h"
#include "djyos.h"
#include "stdint.h"
#include "stddef.h"
#include "cpu_peri.h"
#include <Iboot_info.h>

#include <djyfs/filesystems.h>

extern ptu32_t djy_main(void);
//如果这个CN_MANUFACTURER_NAME名字要改，那djysrc里的Iboot_info.c中相应的名字也要改
const char CN_MANUFACTURER_NAME[] = PRODUCT_MANUFACTURER_NAME;


const struct ProductInfo Djy_Product_Info __attribute__ ((section(".DjyProductInfo"))) =
{
    .VersionNumber[0] = PRODUCT_VERSION_LARGE,
    .VersionNumber[1] = PRODUCT_VERSION_MEDIUM,
    .VersionNumber[2] = PRODUCT_VERSION_SMALL,
#if(CN_PTR_BITS < 64)
    .ManufacturerNameAddr      = (u32)(&CN_MANUFACTURER_NAME),
    .ManufacturerNamereserved32    = 0xffffffff,
#else
    .ManufacturerNameAddr      = (u64)(&CN_MANUFACTURER_NAME),
#endif
    .ProductClassify = PRODUCT_PRODUCT_CLASSIFY,
    .ProductType = PRODUCT_PRODUCT_MODEL,

    .TypeCode = PRODUCT_PRODUCT_MODEL_CODE,

    .ProductionTime = {'*','*','*','*'},
    .ProductionNumber = {'*','*','*','*','*'},
    .reserved8 = 0,
    .BoardType = PRODUCT_BOARD_TYPE,
    .CPU_Type = PRODUCT_CPU_TYPE,
    .Reserved ={
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff
            },
};


ptu32_t __djy_main(void)
{
    //modbus
    extern bool_t ModuleInstall_Modbus(void);
    ModuleInstall_Modbus();
    //end modbus

    djy_main();

	return 0;
}

void Sys_ModuleInit(void)
{
	uint16_t evtt_main;

    //shell
    extern void Stdio_KnlInOutInit(char * StdioIn, char *StdioOut);
    Stdio_KnlInOutInit(CFG_STDIO_IN_NAME,CFG_STDIO_OUT_NAME);
    extern s32 ModuleInstall_Shell(ptu32_t para);
    ModuleInstall_Shell(0);
    //end shell

    //----------------------------early----------------------------//
    //black box
    extern void ModuleInstall_BlackBox(void);
    ModuleInstall_BlackBox( );
    //end black box

    //device file system
    extern s32 ModuleInstall_dev(void);
    ModuleInstall_dev();    // 安装设备文件系统；
    //end device file system

    //djybus
    extern bool_t ModuleInstall_DjyBus(void);
    ModuleInstall_DjyBus ( );
    //end djybus

    //message queue
    extern bool_t ModuleInstall_MsgQ(void);
    ModuleInstall_MsgQ ( );
    //end message queue

    //multiplex
    extern bool_t ModuleInstall_Multiplex(void);
    ModuleInstall_Multiplex ();
    //end multiplex

    //spi bus
    extern bool_t ModuleInstall_SPIBus(void);
    ModuleInstall_SPIBus();
    //end spi bus

    //cpu onchip spi
    extern bool_t ModuleInstall_SPI(u8 port);
    #if CFG_SPI1_ENABLE==1
    ModuleInstall_SPI(CN_SPI1);
    #endif
    #if CFG_SPI2_ENABLE==1
    ModuleInstall_SPI(CN_SPI2);
    #endif
    #if CFG_SPI3_ENABLE==1
    ModuleInstall_SPI(CN_SPI3);
    #endif
    #if CFG_SPI4_ENABLE==1
    ModuleInstall_SPI(CN_SPI4);
    #endif
    //end cpu onchip spi

    //xip iboot file system
    extern s32 ModuleInstall_XIP_IBOOT_FS(u32 opt, void *data);
    ModuleInstall_XIP_IBOOT_FS(0,NULL);
    //end xip iboot file system

    //cpu drive inner flash
    s32 ModuleInstall_EmbededFlash(u32 doformat);
    ModuleInstall_EmbededFlash(CFG_EFLASH_PART_FORMAT);
    //end cpu drive inner flash

    //emflash insatall xip
    extern s32 ModuleInstall_EmFlashInstallXIP(const char *TargetFs,s32 bstart, s32 bend, u32 doformat);
    ModuleInstall_EmFlashInstallXIP(CFG_EFLASH_XIPFSMOUNT_NAME,CFG_EFLASH_XIP_PART_START,
    CFG_EFLASH_XIP_PART_END, CFG_EFLASH_XIP_PART_FORMAT);
    //end emflash insatall xip

    //kernel
    #if(CFG_OS_TINY == flase)
    extern s32 kernel_command(void);
    kernel_command();
    #endif
    //end kernel

    //Nls Charset
    extern ptu32_t ModuleInstall_Charset(ptu32_t para);
    ModuleInstall_Charset(0);
    extern void ModuleInstall_CharsetNls(const char * DefaultCharset);
    ModuleInstall_CharsetNls("C");
    //end Nls Charset

    //fat file system
    extern s32 ModuleInstall_FAT(const char *dir, u32 opt, void *data);
    ModuleInstall_FAT(CFG_FAT_MOUNT_POINT, CFG_FAT_MS_INSTALLUSE, CFG_FAT_MEDIA_KIND);
    //end fat file system

    //Software Timers
    extern bool_t ModuleInstall_Timer(void);
    ModuleInstall_Timer();
    //end Software Timers

    //cpu onchip timer
    extern bool_t ModuleInstall_HardTimer(void);
    ModuleInstall_HardTimer();
    //end cpu onchip timer

    //tcpip
    extern bool_t ModuleInstall_TcpIp(void);
    ModuleInstall_TcpIp( );
    //end tcpip

    //cpu onchip ETH
    extern bool_t ModuleInstall_ETH(void);
    ModuleInstall_ETH( );
    //end cpu onchip ETH

    //cpu onchip uart
    extern ptu32_t ModuleInstall_UART(ptu32_t SerialNo);
    #if CFG_UART1_ENABLE ==1
    ModuleInstall_UART(CN_UART1);
    #endif
    #if CFG_UART2_ENABLE ==1
    ModuleInstall_UART(CN_UART2);
    #endif
    #if CFG_UART3_ENABLE ==1
    ModuleInstall_UART(CN_UART3);
    #endif
    #if CFG_UART4_ENABLE ==1
    ModuleInstall_UART(CN_UART4);
    #endif
    #if CFG_UART5_ENABLE ==1
    ModuleInstall_UART(CN_UART5);
    #endif
    #if CFG_UART6_ENABLE ==1
    ModuleInstall_UART(CN_UART6);
    #endif
    #if CFG_UART7_ENABLE ==1
    ModuleInstall_UART(CN_UART7);
    #endif
    #if CFG_UART8_ENABLE ==1
    ModuleInstall_UART(CN_UART8);
    #endif
    //end cpu onchip uart

    //norflash W25QXX
    extern s32 ModuleInstall_W25qxx(void);
    ModuleInstall_W25qxx();
    //end norflash W25QXX

    //W25QXX FAT
    extern bool_t ModuleInstall_W25qxxInstallFat(const char *TargetFs, s32 bend, u32 doformat);
    ModuleInstall_W25qxxInstallFat(CFG_W25_FAT_MOUNT_NAME,CFG_W25_FAT_PART_END,CFG_W25_FAT_PART_FORMAT);
    //end W25QXX FAT

    //----------------------------later----------------------------//
    //stdio
    #if(CFG_STDIO_STDIOFILE == true)
    extern s32 ModuleInstall_STDIO(const char *in,const char *out, const char *err);
    ModuleInstall_STDIO(CFG_STDIO_IN_NAME,CFG_STDIO_OUT_NAME,CFG_STDIO_ERR_NAME);
    #endif
    //end stdio

    //network config
    extern void ModuleInstall_InitNet( );
    ModuleInstall_InitNet( );
    //end network config

	evtt_main = DJY_EvttRegist(EN_CORRELATIVE,CN_PRIO_RRS,0,0,
		__djy_main,NULL,CFG_MAINSTACK_LIMIT, "main function");
	//事件的两个参数暂设为0,如果用shell启动,可用来采集shell命令行参数
	DJY_EventPop(evtt_main,NULL,0,0,0,0);

    //----------------------------medium----------------------------//
    //heap
    #if ((CFG_DYNAMIC_MEM == true))
    extern bool_t Heap_DynamicModuleInit(void);
    Heap_DynamicModuleInit ( );
    #endif
    //end heap



	return ;
}

/*Modified at 2024-01-23 17:17:41*/
/****************************************************
 *  Automatically-generated file. Do not edit!	*
 ****************************************************/

#include "project_config.h"
#include "djyos.h"
#include "stdint.h"
#include "stddef.h"
#include "cpu_peri.h"
#include <Iboot_info.h>

#include <djyfs/filesystems.h>

extern ptu32_t djy_main(void);
//如果这个CN_MANUFACTURER_NAME名字要改，那djysrc里的Iboot_info.c中相应的名字也要改
const char CN_MANUFACTURER_NAME[] = PRODUCT_MANUFACTURER_NAME;


const struct ProductInfo Djy_Product_Info __attribute__ ((section(".DjyProductInfo"))) =
{
    .VersionNumber[0] = PRODUCT_VERSION_LARGE,
    .VersionNumber[1] = PRODUCT_VERSION_MEDIUM,
    .VersionNumber[2] = PRODUCT_VERSION_SMALL,
#if(CN_PTR_BITS < 64)
    .ManufacturerNameAddr      = (u32)(&CN_MANUFACTURER_NAME),
    .ManufacturerNamereserved32    = 0xffffffff,
#else
    .ManufacturerNameAddr      = (u64)(&CN_MANUFACTURER_NAME),
#endif
    .ProductClassify = PRODUCT_PRODUCT_CLASSIFY,
    .ProductType = PRODUCT_PRODUCT_MODEL,

    .TypeCode = PRODUCT_PRODUCT_MODEL_CODE,

    .ProductionTime = {'*','*','*','*'},
    .ProductionNumber = {'*','*','*','*','*'},
    .reserved8 = 0,
    .BoardType = PRODUCT_BOARD_TYPE,
    .CPU_Type = PRODUCT_CPU_TYPE,
    .Reserved ={
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,\
                0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff,0xff
            },
};


ptu32_t __djy_main(void)
{
    //modbus
    extern bool_t ModuleInstall_Modbus(void);
    ModuleInstall_Modbus();
    //end modbus

    djy_main();

	return 0;
}

void Sys_ModuleInit(void)
{
	uint16_t evtt_main;

    //shell
    extern void Stdio_KnlInOutInit(char * StdioIn, char *StdioOut);
    Stdio_KnlInOutInit(CFG_STDIO_IN_NAME,CFG_STDIO_OUT_NAME);
    extern s32 ModuleInstall_Shell(ptu32_t para);
    ModuleInstall_Shell(0);
    //end shell

    //----------------------------early----------------------------//
    //black box
    extern void ModuleInstall_BlackBox(void);
    ModuleInstall_BlackBox( );
    //end black box

    //device file system
    extern s32 ModuleInstall_dev(void);
    ModuleInstall_dev();    // 安装设备文件系统；
    //end device file system

    //djybus
    extern bool_t ModuleInstall_DjyBus(void);
    ModuleInstall_DjyBus ( );
    //end djybus

    //message queue
    extern bool_t ModuleInstall_MsgQ(void);
    ModuleInstall_MsgQ ( );
    //end message queue

    //multiplex
    extern bool_t ModuleInstall_Multiplex(void);
    ModuleInstall_Multiplex ();
    //end multiplex

    //spi bus
    extern bool_t ModuleInstall_SPIBus(void);
    ModuleInstall_SPIBus();
    //end spi bus

    //xip iboot file system
    extern s32 ModuleInstall_XIP_IBOOT_FS(u32 opt, void *data);
    ModuleInstall_XIP_IBOOT_FS(0,NULL);
    //end xip iboot file system

    //cpu onchip spi
    extern bool_t ModuleInstall_SPI(u8 port);
    #if CFG_SPI1_ENABLE==1
    ModuleInstall_SPI(CN_SPI1);
    #endif
    #if CFG_SPI2_ENABLE==1
    ModuleInstall_SPI(CN_SPI2);
    #endif
    #if CFG_SPI3_ENABLE==1
    ModuleInstall_SPI(CN_SPI3);
    #endif
    #if CFG_SPI4_ENABLE==1
    ModuleInstall_SPI(CN_SPI4);
    #endif
    //end cpu onchip spi

    //cpu onchip uart
    extern ptu32_t ModuleInstall_UART(ptu32_t SerialNo);
    #if CFG_UART1_ENABLE ==1
    ModuleInstall_UART(CN_UART1);
    #endif
    #if CFG_UART2_ENABLE ==1
    ModuleInstall_UART(CN_UART2);
    #endif
    #if CFG_UART3_ENABLE ==1
    ModuleInstall_UART(CN_UART3);
    #endif
    #if CFG_UART4_ENABLE ==1
    ModuleInstall_UART(CN_UART4);
    #endif
    #if CFG_UART5_ENABLE ==1
    ModuleInstall_UART(CN_UART5);
    #endif
    #if CFG_UART6_ENABLE ==1
    ModuleInstall_UART(CN_UART6);
    #endif
    #if CFG_UART7_ENABLE ==1
    ModuleInstall_UART(CN_UART7);
    #endif
    #if CFG_UART8_ENABLE ==1
    ModuleInstall_UART(CN_UART8);
    #endif
    //end cpu onchip uart

    //fat file system
    extern s32 ModuleInstall_FAT(const char *dir, u32 opt, void *data);
    ModuleInstall_FAT(CFG_FAT_MOUNT_POINT, CFG_FAT_MS_INSTALLUSE, CFG_FAT_MEDIA_KIND);
    //end fat file system

    //cpu onchip timer
    extern bool_t ModuleInstall_HardTimer(void);
    ModuleInstall_HardTimer();
    //end cpu onchip timer

    //cpu drive inner flash
    s32 ModuleInstall_EmbededFlash(u32 doformat);
    ModuleInstall_EmbededFlash(CFG_EFLASH_PART_FORMAT);
    //end cpu drive inner flash

    //emflash insatall xip
    extern s32 ModuleInstall_EmFlashInstallXIP(const char *TargetFs,s32 bstart, s32 bend, u32 doformat);
    ModuleInstall_EmFlashInstallXIP(CFG_EFLASH_XIPFSMOUNT_NAME,CFG_EFLASH_XIP_PART_START,
    CFG_EFLASH_XIP_PART_END, CFG_EFLASH_XIP_PART_FORMAT);
    //end emflash insatall xip

    //kernel
    #if(CFG_OS_TINY == flase)
    extern s32 kernel_command(void);
    kernel_command();
    #endif
    //end kernel

    //Nls Charset
    extern ptu32_t ModuleInstall_Charset(ptu32_t para);
    ModuleInstall_Charset(0);
    extern void ModuleInstall_CharsetNls(const char * DefaultCharset);
    ModuleInstall_CharsetNls("C");
    //end Nls Charset

    //Software Timers
    extern bool_t ModuleInstall_Timer(void);
    ModuleInstall_Timer();
    //end Software Timers

    //tcpip
    extern bool_t ModuleInstall_TcpIp(void);
    ModuleInstall_TcpIp( );
    //end tcpip

    //cpu onchip ETH
    extern bool_t ModuleInstall_ETH(void);
    ModuleInstall_ETH( );
    //end cpu onchip ETH

    //norflash W25QXX
    extern s32 ModuleInstall_W25qxx(void);
    ModuleInstall_W25qxx();
    //end norflash W25QXX

    //W25QXX FAT
    extern bool_t ModuleInstall_W25qxxInstallFat(const char *TargetFs, s32 bend, u32 doformat);
    ModuleInstall_W25qxxInstallFat(CFG_W25_FAT_MOUNT_NAME,CFG_W25_FAT_PART_END,CFG_W25_FAT_PART_FORMAT);
    //end W25QXX FAT

    //----------------------------later----------------------------//
    //stdio
    #if(CFG_STDIO_STDIOFILE == true)
    extern s32 ModuleInstall_STDIO(const char *in,const char *out, const char *err);
    ModuleInstall_STDIO(CFG_STDIO_IN_NAME,CFG_STDIO_OUT_NAME,CFG_STDIO_ERR_NAME);
    #endif
    //end stdio

    //network config
    extern void ModuleInstall_InitNet( );
    ModuleInstall_InitNet( );
    //end network config

	evtt_main = DJY_EvttRegist(EN_CORRELATIVE,CN_PRIO_RRS,0,0,
		__djy_main,NULL,CFG_MAINSTACK_LIMIT, "main function");
	//事件的两个参数暂设为0,如果用shell启动,可用来采集shell命令行参数
	DJY_EventPop(evtt_main,NULL,0,0,0,0);

    //----------------------------medium----------------------------//
    //heap
    #if ((CFG_DYNAMIC_MEM == true))
    extern bool_t Heap_DynamicModuleInit(void);
    Heap_DynamicModuleInit ( );
    #endif
    //end heap



	return ;
}

